;RSen_C_model##OTHER##;RSen_C_type##OTHER##;RSen_C_type_comments##OTHER##;RSen_C_description##OTHER##;RSen_C_code_article##OTHER##;RSen_C_length##LENGTH##MILLIMETERS;RSen_C_height##LENGTH##MILLIMETERS;RSen_C_depth##LENGTH##MILLIMETERS;ZZZ_V Component_01_description_Text##OTHER##;ZZZ_V Component_01_length_Length##LENGTH##MILLIMETERS;ZZZ_V Component_01_height_Length##LENGTH##MILLIMETERS;ZZZ_V Component_01_width_Length##LENGTH##MILLIMETERS;ZZZ_V Component_01_plane_Integer##OTHER##;ZZZ_V Component_01_X_Length##LENGTH##MILLIMETERS;ZZZ_V Component_01_Y_Length##LENGTH##MILLIMETERS;ZZZ_V Component_01_Z_Length##LENGTH##MILLIMETERS;ZZZ_Cut out_length_Length##LENGTH##MILLIMETERS;ZZZ_Cut out_width_Length##LENGTH##MILLIMETERS;ZZZ_Cut out_height_Length##LENGTH##MILLIMETERS;ZZZ_Cut out_position_X_Length##LENGTH##MILLIMETERS;ZZZ_Cut out_position_Y_Length##LENGTH##MILLIMETERS;ZZZ_Parallel wall mounted_YesNo##OTHER##;ZZZ_Pendant - vertical mounted_YesNo##OTHER##;ZZZ_Recess depth_Length##LENGTH##MILLIMETERS;ZZZ_Recessed_YesNo##OTHER##;ZZZ_Surface mounted_YesNo##OTHER##;TBQen_C_offset_from_base_level##LENGTH##MILLIMETERS;TBQ_I Offset from base level_min##LENGTH##MILLIMETERS;TBQ_I Offset from base level_max##LENGTH##MILLIMETERS;ZZZ_Logo_plane_Integer##OTHER##;ZZZ_V Logo_FamilyType_Generic Models##OTHER##;ZZZ_Logo_Rotation about axis_Angle##ANGLE##DEGREES;ZZZ_Logo_X_Length##LENGTH##MILLIMETERS;ZZZ_Logo_Y_Length##LENGTH##MILLIMETERS;ZZZ_Logo_Z_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_back_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_bottom_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_front_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_left_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_right_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_top_Length##LENGTH##MILLIMETERS;RSen_C_material##OTHER##;ZZZ_V Component_01_material_Material##OTHER##;TBQ_I Default Emission_Heating##HVAC_POWER##WATTS;TBQ_I N-Value##OTHER##;TBQ_I Default Emission_Cooling##HVAC_POWER##WATTS
bamc0.06309022/bt/20 - ceiling mounted - 2 pipe_jaga_briza 22_lxhxd 900x630x270 mm;Briza 22;2 pipe;Ceiling mounted;BRIZA 22 CEILING L090 BT LEFT 2P;BAMC0.06309022/BT/20;900;630;270;convector;900;630;270;2;0;0;0;0;0;0;0;0;0;1;0;0;0;0;0;0;4;RSen_55_GM_FB_logo - SH_jaga : standard;180;0;0;0;0;0;0;0;0;0;RSen_x_rgb 241 236 225 T00 white 101_gen;RSen_x_rgb 241 236 225 T00 white 101_gen;6060;0;1891
