{"text_format":"3","workbook":"xlsx","n_sheets":13,"sheets":["Mini Canal","data","NL","EN","DE","FR","NR","SP","SW","TS","ExtraTaal1","ExtraTaal2","ExtraTaal3"],"not_rendered":{"images":5,"macros":1,"defined_names":50},"read":"whole","date_system":"1900"}

{"sheet":"Mini Canal","index":0,"n_rows":343,"n_cols":13,"rows_kept":343,"merged":[[1,1,1,10],[3,1,3,3],[3,6,3,8],[3,9,3,10],[3,11,3,12],[4,6,4,8],[4,9,4,10],[5,6,5,8],[5,11,5,12],[6,9,7,9],[6,10,7,10],[6,11,7,12],[9,1,9,3],[9,6,9,8],[9,11,9,12],[10,1,10,3],[10,6,10,8],[10,11,13,12],[11,1,11,3],[11,6,11,8],[12,6,12,8],[16,1,16,12]]}
[]
[null,{"$f":"IF(data!$R$2=7,\"Effektsimulering Under DBE (Hybrid)\",\"Selectiontool Mini Canal\")","v":"Selectiontool Mini Canal"}]
[]
[{"$nulls":6},"Taal/Language/Sprache/Språk/Jazyk",null,null,"English"]
[{"$nulls":6},{"$f":"IF(data!$R$2=1,NL!G3,IF(data!$R$2=2,EN!G3,IF(data!$R$2=3,DE!G3,IF(data!$R$2=4,FR!G3,IF(data!$R$2=5,NR!G3,IF(data!$R$2=6,SP!G3,IF(data!$R$2=7,SW!G3,IF(data!$R$2=8,TS!G3,IF(data!$R$2=9,ExtraTaal1!G3,IF(data!$R$2=10,ExtraTaal2!G3,IF(data!$R$2=11,ExtraTaal3!G3,)))))))))))","v":"Device"},{"$f":"IF(data!$R$2=1,NL!H3,IF(data!$R$2=2,EN!H3,IF(data!$R$2=3,DE!H3,IF(data!$R$2=4,FR!H3,))))","v":0},{"$f":"IF(data!$R$2=1,NL!I3,IF(data!$R$2=2,EN!I3,IF(data!$R$2=3,DE!I3,IF(data!$R$2=4,FR!I3,))))","v":0},"Mini Canal Hybrid"]
[{"$nulls":6},{"$f":"IF(data!$R$2=1,NL!G4,IF(data!$R$2=2,EN!G4,IF(data!$R$2=3,DE!G4,IF(data!$R$2=4,FR!G4,IF(data!$R$2=5,NR!G4,IF(data!$R$2=6,SP!G4,IF(data!$R$2=7,SW!G4,IF(data!$R$2=8,TS!G4,IF(data!$R$2=9,ExtraTaal1!G4,IF(data!$R$2=10,ExtraTaal2!G4,IF(data!$R$2=11,ExtraTaal3!G4,)))))))))))","v":"Version"},{"$f":"IF(data!$R$2=1,NL!H4,IF(data!$R$2=2,EN!H4,IF(data!$R$2=3,DE!H4,IF(data!$R$2=4,FR!H4,))))","v":0},{"$f":"IF(data!$R$2=1,NL!I4,IF(data!$R$2=2,EN!I4,IF(data!$R$2=3,DE!I4,IF(data!$R$2=4,FR!I4,))))","v":0},14,34,290]
[{"$nulls":9},{"$f":"IF(data!$R$2=1,NL!J6,IF(data!$R$2=2,EN!J6,IF(data!$R$2=3,DE!J6,IF(data!$R$2=4,FR!J6,IF(data!$R$2=5,NR!J6,IF(data!$R$2=6,SP!J6,IF(data!$R$2=7,SW!J6,IF(data!$R$2=8,TS!J6,IF(data!$R$2=9,ExtraTaal1!J6,IF(data!$R$2=10,ExtraTaal2!J6,IF(data!$R$2=11,ExtraTaal3!J6,)))))))))))","v":"Heigth"},{"$f":"IF(data!$R$2=1,NL!K6,IF(data!$R$2=2,EN!K6,IF(data!$R$2=3,DE!K6,IF(data!$R$2=4,FR!K6,IF(data!$R$2=5,NR!K6,IF(data!$R$2=6,SP!K6,IF(data!$R$2=7,SW!K6,IF(data!$R$2=8,TS!K6,IF(data!$R$2=9,ExtraTaal1!K6,IF(data!$R$2=10,ExtraTaal2!K6,IF(data!$R$2=11,ExtraTaal3!K6,)))))))))))","v":"Width"},{"$f":"IF(data!$R$2=1,NL!L6,IF(data!$R$2=2,EN!L6,IF(data!$R$2=3,DE!L6,IF(data!$R$2=4,FR!L6,IF(data!$R$2=5,NR!L6,IF(data!$R$2=6,SP!L6,IF(data!$R$2=7,SW!L6,IF(data!$R$2=8,TS!L6,IF(data!$R$2=9,ExtraTaal1!L6,IF(data!$R$2=10,ExtraTaal2!L6,IF(data!$R$2=11,ExtraTaal3!L6,)))))))))))","v":"Length"},{"$f":"IF(data!$R$2=1,NL!M6,IF(data!$R$2=2,EN!M6,IF(data!$R$2=3,DE!M6,IF(data!$R$2=4,FR!M6,IF(data!$R$2=5,NR!M6,)))))","v":"Type"}]
[null,{"$f":"IF(data!$R$2=1,NL!A6,IF(data!$R$2=2,EN!A6,IF(data!$R$2=3,DE!A6,IF(data!$R$2=4,FR!A6,IF(data!$R$2=5,NR!A6,IF(data!$R$2=6,SP!A6,IF(data!$R$2=7,SW!A6,IF(data!$R$2=8,TS!A6,IF(data!$R$2=9,ExtraTaal1!A6,IF(data!$R$2=10,ExtraTaal2!A6,IF(data!$R$2=11,ExtraTaal3!A6,)))))))))))","v":"Temperatures"},{"$nulls":7},{"$f":"IF(data!$R$2=1,NL!J6,IF(data!$R$2=2,EN!J6,IF(data!$R$2=3,DE!J6,IF(data!$R$2=4,FR!J6,))))","v":"Heigth"},{"$f":"IF(data!$R$2=1,NL!K6,IF(data!$R$2=2,EN!K6,IF(data!$R$2=3,DE!K6,IF(data!$R$2=4,FR!K6,))))","v":"Width"},{"$f":"IF(data!$R$2=1,NL!L6,IF(data!$R$2=2,EN!L6,IF(data!$R$2=3,DE!L6,IF(data!$R$2=4,FR!L6,))))","v":"Length"},{"$f":"IF(data!$R$2=1,NL!M6,IF(data!$R$2=2,EN!M6,IF(data!$R$2=3,DE!M6,IF(data!$R$2=4,FR!M6,))))","v":"Type"}]
[null,{"$f":"IF(data!$R$2=1,NL!A7,IF(data!$R$2=2,EN!A7,IF(data!$R$2=3,DE!A7,IF(data!$R$2=4,FR!A7,IF(data!$R$2=5,NR!A7,IF(data!$R$2=6,SP!A7,IF(data!$R$2=7,SW!A7,IF(data!$R$2=8,TS!A7,IF(data!$R$2=9,ExtraTaal1!A7,IF(data!$R$2=10,ExtraTaal2!A7,IF(data!$R$2=11,ExtraTaal3!A7,)))))))))))","v":"Heating:"},{"$nulls":4},{"$f":"IF(data!$R$2=1,NL!F7,IF(data!$R$2=2,EN!F7,IF(data!$R$2=3,DE!F7,IF(data!$R$2=4,FR!F7,IF(data!$R$2=5,NR!F7,IF(data!$R$2=6,SP!F7,IF(data!$R$2=7,SW!F7,IF(data!$R$2=8,TS!F7,IF(data!$R$2=9,ExtraTaal1!F7,IF(data!$R$2=10,ExtraTaal2!F7,IF(data!$R$2=11,ExtraTaal3!F7,)))))))))))","v":"Cooling:"}]
[null,{"$f":"IF(data!$R$2=1,NL!A8,IF(data!$R$2=2,EN!A8,IF(data!$R$2=3,DE!A8,IF(data!$R$2=4,FR!A8,IF(data!$R$2=5,NR!A8,IF(data!$R$2=6,SP!A8,IF(data!$R$2=7,SW!A8,IF(data!$R$2=8,TS!A8,IF(data!$R$2=9,ExtraTaal1!A8,IF(data!$R$2=10,ExtraTaal2!A8,IF(data!$R$2=11,ExtraTaal3!A8,)))))))))))","v":"Inlet temp."},{"$f":"IF(data!$R$2=1,NL!B8,IF(data!$R$2=2,EN!B8,IF(data!$R$2=3,DE!B8,IF(data!$R$2=4,FR!B8,IF(data!$R$2=5,NR!B8,IF(data!$R$2=6,SP!B8,IF(data!$R$2=7,SW!B8,IF(data!$R$2=8,TS!B8,IF(data!$R$2=9,ExtraTaal1!B8,IF(data!$R$2=10,ExtraTaal2!B8,IF(data!$R$2=11,ExtraTaal3!B8,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!C8,IF(data!$R$2=2,EN!C8,IF(data!$R$2=3,DE!C8,IF(data!$R$2=4,FR!C8,IF(data!$R$2=5,NR!C8,IF(data!$R$2=6,SP!C8,IF(data!$R$2=7,SW!C8,IF(data!$R$2=8,TS!C8,IF(data!$R$2=9,ExtraTaal1!C8,IF(data!$R$2=10,ExtraTaal2!C8,IF(data!$R$2=11,ExtraTaal3!C8,)))))))))))","v":0},35,{"$f":"IF(data!$P$1=1,\"°C\",IF(data!$P$1=2,\"°F\"))","v":"°C"},{"$f":"B10","v":"Inlet temp."},{"$f":"IF(data!$R$2=1,NL!G8,IF(data!$R$2=2,EN!G8,IF(data!$R$2=3,DE!G8,IF(data!$R$2=4,FR!G8,))))","v":0},{"$f":"IF(data!$R$2=1,NL!H8,IF(data!$R$2=2,EN!H8,IF(data!$R$2=3,DE!H8,IF(data!$R$2=4,FR!H8,))))","v":0},16,{"$f":"F10","v":"°C"},{"$f":"IF(data!$R$2=1,NL!L8,IF(data!$R$2=2,EN!L8,IF(data!$R$2=3,DE!L8,IF(data!$R$2=4,FR!L8,IF(data!$R$2=5,NR!L8,IF(data!$R$2=6,SP!L8,IF(data!$R$2=7,SW!L8,IF(data!$R$2=8,TS!L8,IF(data!$R$2=9,ExtraTaal1!L8,IF(data!$R$2=10,ExtraTaal2!L8,IF(data!$R$2=11,ExtraTaal3!L8,)))))))))))","v":"Unit conversion"},{"$f":"IF(data!$R$2=1,NL!L8,IF(data!$R$2=2,EN!L8,IF(data!$R$2=3,DE!L8,IF(data!$R$2=4,FR!L8,IF(data!$R$2=5,NR!L8,IF(data!$R$2=6,SP!L8,IF(data!$R$2=7,SW!L8,IF(data!$R$2=8,TS!L8,IF(data!$R$2=9,ExtraTaal1!L8,IF(data!$R$2=10,ExtraTaal2!L8,IF(data!$R$2=11,ExtraTaal3!L8,)))))))))))","v":"Unit conversion"}]
[null,{"$f":"IF(data!$R$2=1,NL!A9,IF(data!$R$2=2,EN!A9,IF(data!$R$2=3,DE!A9,IF(data!$R$2=4,FR!A9,IF(data!$R$2=5,NR!A9,IF(data!$R$2=6,SP!A9,IF(data!$R$2=7,SW!A9,IF(data!$R$2=8,TS!A9,IF(data!$R$2=9,ExtraTaal1!A9,IF(data!$R$2=10,ExtraTaal2!A9,IF(data!$R$2=11,ExtraTaal3!A9,)))))))))))","v":"Return temp."},{"$f":"IF(data!$R$2=1,NL!B9,IF(data!$R$2=2,EN!B9,IF(data!$R$2=3,DE!B9,IF(data!$R$2=4,FR!B9,IF(data!$R$2=5,NR!B9,IF(data!$R$2=6,SP!B9,IF(data!$R$2=7,SW!B9,IF(data!$R$2=8,TS!B9,IF(data!$R$2=9,ExtraTaal1!B9,IF(data!$R$2=10,ExtraTaal2!B9,IF(data!$R$2=11,ExtraTaal3!B9,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!C9,IF(data!$R$2=2,EN!C9,IF(data!$R$2=3,DE!C9,IF(data!$R$2=4,FR!C9,IF(data!$R$2=5,NR!C9,IF(data!$R$2=6,SP!C9,IF(data!$R$2=7,SW!C9,IF(data!$R$2=8,TS!C9,IF(data!$R$2=9,ExtraTaal1!C9,IF(data!$R$2=10,ExtraTaal2!C9,IF(data!$R$2=11,ExtraTaal3!C9,)))))))))))","v":0},30,{"$f":"F10","v":"°C"},{"$f":"B11","v":"Return temp."},{"$f":"IF(data!$R$2=1,NL!G9,IF(data!$R$2=2,EN!G9,IF(data!$R$2=3,DE!G9,IF(data!$R$2=4,FR!G9,))))","v":0},{"$f":"IF(data!$R$2=1,NL!H9,IF(data!$R$2=2,EN!H9,IF(data!$R$2=3,DE!H9,IF(data!$R$2=4,FR!H9,))))","v":0},18,{"$f":"F10","v":"°C"}]
[null,{"$f":"IF(data!$R$2=1,NL!A10,IF(data!$R$2=2,EN!A10,IF(data!$R$2=3,DE!A10,IF(data!$R$2=4,FR!A10,IF(data!$R$2=5,NR!A10,IF(data!$R$2=6,SP!A10,IF(data!$R$2=7,SW!A10,IF(data!$R$2=8,TS!A10,IF(data!$R$2=9,ExtraTaal1!A10,IF(data!$R$2=10,ExtraTaal2!A10,IF(data!$R$2=11,ExtraTaal3!A10,)))))))))))","v":"Room temp."},{"$f":"IF(data!$R$2=1,NL!B10,IF(data!$R$2=2,EN!B10,IF(data!$R$2=3,DE!B10,IF(data!$R$2=4,FR!B10,IF(data!$R$2=5,NR!B10,IF(data!$R$2=6,SP!B10,IF(data!$R$2=7,SW!B10,IF(data!$R$2=8,TS!B10,IF(data!$R$2=9,ExtraTaal1!B10,IF(data!$R$2=10,ExtraTaal2!B10,IF(data!$R$2=11,ExtraTaal3!B10,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!C10,IF(data!$R$2=2,EN!C10,IF(data!$R$2=3,DE!C10,IF(data!$R$2=4,FR!C10,IF(data!$R$2=5,NR!C10,IF(data!$R$2=6,SP!C10,IF(data!$R$2=7,SW!C10,IF(data!$R$2=8,TS!C10,IF(data!$R$2=9,ExtraTaal1!C10,IF(data!$R$2=10,ExtraTaal2!C10,IF(data!$R$2=11,ExtraTaal3!C10,)))))))))))","v":0},20,{"$f":"F10","v":"°C"},{"$f":"B12","v":"Room temp."},{"$f":"IF(data!$R$2=1,NL!G10,IF(data!$R$2=2,EN!G10,IF(data!$R$2=3,DE!G10,IF(data!$R$2=4,FR!G10,))))","v":0},{"$f":"IF(data!$R$2=1,NL!H10,IF(data!$R$2=2,EN!H10,IF(data!$R$2=3,DE!H10,IF(data!$R$2=4,FR!H10,))))","v":0},{"v":26.999999999999996,"d":"27"},{"$f":"F10","v":"°C"}]
[{"$nulls":6},{"$f":"IF(data!$R$2=1,NL!F11,IF(data!$R$2=2,EN!F11,IF(data!$R$2=3,DE!F11,IF(data!$R$2=4,FR!F11,IF(data!$R$2=5,NR!F11,IF(data!$R$2=6,SP!F11,IF(data!$R$2=7,SW!F11,IF(data!$R$2=8,TS!F11,IF(data!$R$2=9,ExtraTaal1!F11,IF(data!$R$2=10,ExtraTaal2!F11,IF(data!$R$2=11,ExtraTaal3!F11,)))))))))))","v":"rel. humid. [%]"},{"$f":"IF(data!$R$2=1,NL!G11,IF(data!$R$2=2,EN!G11,IF(data!$R$2=3,DE!G11,IF(data!$R$2=4,FR!G11,IF(data!$R$2=5,NR!G11,IF(data!$R$2=6,SP!G11,IF(data!$R$2=7,SW!G11,IF(data!$R$2=8,TS!G11,IF(data!$R$2=9,ExtraTaal1!G11,IF(data!$R$2=10,ExtraTaal2!G11,IF(data!$R$2=11,ExtraTaal3!G11,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!H11,IF(data!$R$2=2,EN!H11,IF(data!$R$2=3,DE!H11,IF(data!$R$2=4,FR!H11,IF(data!$R$2=5,NR!H11,IF(data!$R$2=6,SP!H11,IF(data!$R$2=7,SW!H11,IF(data!$R$2=8,TS!H11,IF(data!$R$2=9,ExtraTaal1!H11,IF(data!$R$2=10,ExtraTaal2!H11,IF(data!$R$2=11,ExtraTaal3!H11,)))))))))))","v":0},{"v":0.5,"d":"50%"}]
[]
[]
[null,{"$f":"IF(data!$R$2=1,NL!A14,IF(data!$R$2=2,EN!A14,IF(data!$R$2=3,DE!A14,IF(data!$R$2=4,FR!A14,IF(data!$R$2=5,NR!A14,IF(data!$R$2=6,SP!A14,IF(data!$R$2=7,SW!A14,IF(data!$R$2=8,TS!A14,IF(data!$R$2=9,ExtraTaal1!A14,IF(data!$R$2=10,ExtraTaal2!A14,IF(data!$R$2=11,ExtraTaal3!A14,)))))))))))","v":"Speed level:"},{"$f":"IF(data!$R$2=1,NL!B14,IF(data!$R$2=2,EN!B14,IF(data!$R$2=3,DE!B14,IF(data!$R$2=4,FR!B14,IF(data!$R$2=5,NR!B14,IF(data!$R$2=6,SP!B14,IF(data!$R$2=7,SW!B14,IF(data!$R$2=8,TS!B14,IF(data!$R$2=9,ExtraTaal1!B14,IF(data!$R$2=10,ExtraTaal2!B14,IF(data!$R$2=11,ExtraTaal3!B14,)))))))))))","v":"Control voltage [V]"},{"$f":"IF(data!$R$2=1,NL!C14,IF(data!$R$2=2,EN!C14,IF(data!$R$2=3,DE!C14,IF(data!$R$2=4,FR!C14,IF(data!$R$2=5,NR!C14,IF(data!$R$2=6,SP!C14,IF(data!$R$2=7,SW!C14,IF(data!$R$2=8,TS!C14,IF(data!$R$2=9,ExtraTaal1!C14,IF(data!$R$2=10,ExtraTaal2!C14,IF(data!$R$2=11,ExtraTaal3!C14,)))))))))))","v":"Heat output * 35/30/20 [W]"},{"$f":"IF(data!$R$2=1,NL!D14,IF(data!$R$2=2,EN!D14,IF(data!$R$2=3,DE!D14,IF(data!$R$2=4,FR!D14,IF(data!$R$2=5,NR!D14,IF(data!$R$2=6,SP!D14,IF(data!$R$2=7,SW!D14,IF(data!$R$2=8,TS!D14,IF(data!$R$2=9,ExtraTaal1!D14,IF(data!$R$2=10,ExtraTaal2!D14,IF(data!$R$2=11,ExtraTaal3!D14,)))))))))))","v":"Water flowrate, heating [l/h]"},{"$f":"IF(data!$R$2=1,NL!E14,IF(data!$R$2=2,EN!E14,IF(data!$R$2=3,DE!E14,IF(data!$R$2=4,FR!E14,IF(data!$R$2=5,NR!E14,IF(data!$R$2=6,SP!E14,IF(data!$R$2=7,SW!E14,IF(data!$R$2=8,TS!E14,IF(data!$R$2=9,ExtraTaal1!E14,IF(data!$R$2=10,ExtraTaal2!E14,IF(data!$R$2=11,ExtraTaal3!E14,)))))))))))","v":"Watersided pressure loss [kPa]"},{"$f":"IF(data!$R$2=1,NL!F14,IF(data!$R$2=2,EN!F14,IF(data!$R$2=3,DE!F14,IF(data!$R$2=4,FR!F14,IF(data!$R$2=5,NR!F14,IF(data!$R$2=6,SP!F14,IF(data!$R$2=7,SW!F14,IF(data!$R$2=8,TS!F14,IF(data!$R$2=9,ExtraTaal1!F14,IF(data!$R$2=10,ExtraTaal2!F14,IF(data!$R$2=11,ExtraTaal3!F14,)))))))))))","v":"Cooling capacity * 16/18/27 [W]"},{"$f":"IF(data!$R$2=1,NL!H14,IF(data!$R$2=2,EN!H14,IF(data!$R$2=3,DE!H14,IF(data!$R$2=4,FR!H14,IF(data!$R$2=5,NR!H14,IF(data!$R$2=6,SP!H14,IF(data!$R$2=7,SW!H14,IF(data!$R$2=8,TS!H14,IF(data!$R$2=9,ExtraTaal1!H14,IF(data!$R$2=10,ExtraTaal2!H14,IF(data!$R$2=11,ExtraTaal3!H14,)))))))))))","v":"Water flowrate, cooling [l/h]"},{"$f":"IF(data!$R$2=1,NL!E14,IF(data!$R$2=2,EN!E14,IF(data!$R$2=3,DE!E14,IF(data!$R$2=4,FR!E14,IF(data!$R$2=5,NR!E14,IF(data!$R$2=6,SP!E14,IF(data!$R$2=7,SW!E14,IF(data!$R$2=8,TS!E14,IF(data!$R$2=9,ExtraTaal1!E14,IF(data!$R$2=10,ExtraTaal2!E14,IF(data!$R$2=11,ExtraTaal3!E14,)))))))))))","v":"Watersided pressure loss [kPa]"},{"$f":"IF(data!$R$2=1,NL!J14,IF(data!$R$2=2,EN!J14,IF(data!$R$2=3,DE!J14,IF(data!$R$2=4,FR!J14,IF(data!$R$2=5,NR!J14,IF(data!$R$2=6,SP!J14,IF(data!$R$2=7,SW!J14,IF(data!$R$2=8,TS!J14,IF(data!$R$2=9,ExtraTaal1!J14,IF(data!$R$2=10,ExtraTaal2!J14,IF(data!$R$2=11,ExtraTaal3!J14,)))))))))))","v":"Sound pressure *** [dB(A)]"},{"$f":"IF(data!$R$2=1,NL!K14,IF(data!$R$2=2,EN!K14,IF(data!$R$2=3,DE!K14,IF(data!$R$2=4,FR!K14,IF(data!$R$2=5,NR!K14,IF(data!$R$2=6,SP!K14,IF(data!$R$2=7,SW!K14,IF(data!$R$2=8,TS!K14,IF(data!$R$2=9,ExtraTaal1!K14,IF(data!$R$2=10,ExtraTaal2!K14,IF(data!$R$2=11,ExtraTaal3!K14,)))))))))))","v":"Sound power ** [dB(A)]"},{"$f":"IF(data!$R$2=1,NL!L14,IF(data!$R$2=2,EN!L14,IF(data!$R$2=3,DE!L14,IF(data!$R$2=4,FR!L14,IF(data!$R$2=5,NR!L14,IF(data!$R$2=6,SP!L14,IF(data!$R$2=7,SW!L14,IF(data!$R$2=8,TS!L14,IF(data!$R$2=9,ExtraTaal1!L14,IF(data!$R$2=10,ExtraTaal2!L14,IF(data!$R$2=11,ExtraTaal3!L14,)))))))))))","v":"Electrical power [W]"},{"$f":"IF(data!$R$2=1,NL!M14,IF(data!$R$2=2,EN!M14,IF(data!$R$2=3,DE!M14,IF(data!$R$2=4,FR!M14,IF(data!$R$2=5,NR!M14,IF(data!$R$2=6,SP!M14,IF(data!$R$2=7,SW!M14,IF(data!$R$2=8,TS!M14,IF(data!$R$2=9,ExtraTaal1!M14,IF(data!$R$2=10,ExtraTaal2!M14,IF(data!$R$2=11,ExtraTaal3!M14,)))))))))))","v":"Water volume [l]"}]
[null,{"$f":"IF(data!$R$2=1,NL!A15,IF(data!$R$2=2,EN!A15,IF(data!$R$2=3,DE!A15,IF(data!$R$2=4,FR!A15,IF(data!$R$2=5,NR!A15,IF(data!$R$2=6,SP!A15,IF(data!$R$2=7,SW!A15,IF(data!$R$2=8,TS!A15,IF(data!$R$2=9,ExtraTaal1!A15,IF(data!$R$2=10,ExtraTaal2!A15,IF(data!$R$2=11,ExtraTaal3!A15,)))))))))))","v":"Mini Canal, Length 290cm, Heigth 14cm, Width 34cm"},{"$f":"IF(data!$R$2=1,NL!B15,IF(data!$R$2=2,EN!B15,IF(data!$R$2=3,DE!B15,IF(data!$R$2=4,FR!B15,IF(data!$R$2=5,NR!B15,IF(data!$R$2=6,SP!B15,IF(data!$R$2=7,SW!B15,IF(data!$R$2=8,TS!B15,IF(data!$R$2=9,ExtraTaal1!B15,IF(data!$R$2=10,ExtraTaal2!B15,IF(data!$R$2=11,ExtraTaal3!B15,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!C15,IF(data!$R$2=2,EN!C15,IF(data!$R$2=3,DE!C15,IF(data!$R$2=4,FR!C15,IF(data!$R$2=5,NR!C15,IF(data!$R$2=6,SP!C15,IF(data!$R$2=7,SW!C15,IF(data!$R$2=8,TS!C15,IF(data!$R$2=9,ExtraTaal1!C15,IF(data!$R$2=10,ExtraTaal2!C15,IF(data!$R$2=11,ExtraTaal3!C15,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!D15,IF(data!$R$2=2,EN!D15,IF(data!$R$2=3,DE!D15,IF(data!$R$2=4,FR!D15,IF(data!$R$2=5,NR!D15,IF(data!$R$2=6,SP!D15,IF(data!$R$2=7,SW!D15,IF(data!$R$2=8,TS!D15,IF(data!$R$2=9,ExtraTaal1!D15,IF(data!$R$2=10,ExtraTaal2!D15,IF(data!$R$2=11,ExtraTaal3!D15,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!E15,IF(data!$R$2=2,EN!E15,IF(data!$R$2=3,DE!E15,IF(data!$R$2=4,FR!E15,IF(data!$R$2=5,NR!E15,IF(data!$R$2=6,SP!E15,IF(data!$R$2=7,SW!E15,IF(data!$R$2=8,TS!E15,IF(data!$R$2=9,ExtraTaal1!E15,IF(data!$R$2=10,ExtraTaal2!E15,IF(data!$R$2=11,ExtraTaal3!E15,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!F15,IF(data!$R$2=2,EN!F15,IF(data!$R$2=3,DE!F15,IF(data!$R$2=4,FR!F15,IF(data!$R$2=5,NR!F15,IF(data!$R$2=6,SP!F15,IF(data!$R$2=7,SW!F15,IF(data!$R$2=8,TS!F15,IF(data!$R$2=9,ExtraTaal1!F15,IF(data!$R$2=10,ExtraTaal2!F15,IF(data!$R$2=11,ExtraTaal3!F15,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!G15,IF(data!$R$2=2,EN!G15,IF(data!$R$2=3,DE!G15,IF(data!$R$2=4,FR!G15,IF(data!$R$2=5,NR!G15,IF(data!$R$2=6,SP!G15,IF(data!$R$2=7,SW!G15,IF(data!$R$2=8,TS!G15,IF(data!$R$2=9,ExtraTaal1!G15,IF(data!$R$2=10,ExtraTaal2!G15,IF(data!$R$2=11,ExtraTaal3!G15,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!H15,IF(data!$R$2=2,EN!H15,IF(data!$R$2=3,DE!H15,IF(data!$R$2=4,FR!H15,IF(data!$R$2=5,NR!H15,IF(data!$R$2=6,SP!H15,IF(data!$R$2=7,SW!H15,IF(data!$R$2=8,TS!H15,IF(data!$R$2=9,ExtraTaal1!H15,IF(data!$R$2=10,ExtraTaal2!H15,IF(data!$R$2=11,ExtraTaal3!H15,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!I15,IF(data!$R$2=2,EN!I15,IF(data!$R$2=3,DE!I15,IF(data!$R$2=4,FR!I15,IF(data!$R$2=5,NR!I15,IF(data!$R$2=6,SP!I15,IF(data!$R$2=7,SW!I15,IF(data!$R$2=8,TS!I15,IF(data!$R$2=9,ExtraTaal1!I15,IF(data!$R$2=10,ExtraTaal2!I15,IF(data!$R$2=11,ExtraTaal3!I15,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!J15,IF(data!$R$2=2,EN!J15,IF(data!$R$2=3,DE!J15,IF(data!$R$2=4,FR!J15,IF(data!$R$2=5,NR!J15,IF(data!$R$2=6,SP!J15,IF(data!$R$2=7,SW!J15,IF(data!$R$2=8,TS!J15,IF(data!$R$2=9,ExtraTaal1!J15,IF(data!$R$2=10,ExtraTaal2!J15,IF(data!$R$2=11,ExtraTaal3!J15,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!K15,IF(data!$R$2=2,EN!K15,IF(data!$R$2=3,DE!K15,IF(data!$R$2=4,FR!K15,IF(data!$R$2=5,NR!K15,IF(data!$R$2=6,SP!K15,IF(data!$R$2=7,SW!K15,IF(data!$R$2=8,TS!K15,IF(data!$R$2=9,ExtraTaal1!K15,IF(data!$R$2=10,ExtraTaal2!K15,IF(data!$R$2=11,ExtraTaal3!K15,)))))))))))","v":0},{"$f":"IF(data!$R$2=1,NL!L15,IF(data!$R$2=2,EN!L15,IF(data!$R$2=3,DE!L15,IF(data!$R$2=4,FR!L15,IF(data!$R$2=5,NR!L15,IF(data!$R$2=6,SP!L15,IF(data!$R$2=7,SW!L15,IF(data!$R$2=8,TS!L15,IF(data!$R$2=9,ExtraTaal1!L15,IF(data!$R$2=10,ExtraTaal2!L15,IF(data!$R$2=11,ExtraTaal3!L15,)))))))))))","v":0}]
[null,{"$f":"IF(J5=data!Z1,data!S8,\"\")","v":0},{"$f":"IF(J5=data!Z1,data!BG5,data!AA2)","v":{"v":0,"d":"0.0"}},{"$f":"ROUND(IF(data!$P$1=1,data!S5,IF(data!$P$1=2,data!S5*3.412141633,)),0)","v":183},{"$f":"IF(data!$P$1=1,ROUND(data!W5,0),IF(data!$P$1=2,ROUND(data!W5/272.7654,1),))","v":31},{"$f":"IF(data!$P$1=1,data!AA5,IF(data!$P$1=2,data!AA5*0.334552563,))","v":{"v":0.4596260269960454,"d":"0.46"}},{"$nulls":3},{"v":0,"d":"0.0"},{"v":0,"d":"0.0"},{"v":0,"d":"0.0"},{"$f":"data!AW5","v":{"v":2.9,"d":"2.90"}}]
[null,{"$f":"data!T8","v":1},{"$f":"data!BH5","v":{"v":6.0515594714640155,"d":"6.1"}},{"$f":"ROUND(IF(data!$P$1=1,data!T5,IF(data!$P$1=2,data!T5*3.412141633,)),0)","v":1219},{"$f":"IF(data!$P$1=1,ROUND(data!X5,0),IF(data!$P$1=2,ROUND(data!X5/272.7654,1),))","v":210},{"$f":"IF(data!$P$1=1,data!AB5,IF(data!$P$1=2,data!AB5*0.334552563,))","v":{"v":13.56176252546608,"d":"13.56"}},{"$f":"IF(data!AQ5>data!AK5,\"\",ROUND(IF(data!$P$1=1,data!AQ5,IF(data!$P$1=2,data!AQ5*3.412141633,)),0))","v":292},{"$f":"IF(data!AQ5>data!AK5,\"\",IF(data!$P$1=1,ROUND(data!AN5,0),IF(data!$P$1=2,ROUND(data!AN5/272.7654,1),)))","v":126},{"$f":"IF(data!AQ5>data!AK5,\"\",IF(data!$P$1=1,data!AT5,IF(data!$P$1=2,data!AT5*0.334552563,)))","v":{"v":5.492030247267677,"d":"5.49"}},{"$f":"data!H5","v":{"v":26,"d":"26.0"}},{"$f":"J19+8","v":{"v":34,"d":"34.0"}},{"$f":"data!AX5","v":26.5},{"$f":"data!AW5","v":{"v":2.9,"d":"2.90"}}]
[null,{"$f":"data!U8","v":2},{"$f":"data!BI5","v":{"v":6.87363114546986,"d":"6.9"}},{"$f":"ROUND(IF(data!$P$1=1,data!U5,IF(data!$P$1=2,data!U5*3.412141633,)),0)","v":1355},{"$f":"IF(data!$P$1=1,ROUND(data!Y5,0),IF(data!$P$1=2,ROUND(data!Y5/272.7654,1),))","v":233},{"$f":"IF(data!$P$1=1,data!AC5,IF(data!$P$1=2,data!AC5*0.334552563,))","v":{"v":16.30047092944978,"d":"16.30"}},{"$f":"IF(data!AR5>data!AL5,\"\",ROUND(IF(data!$P$1=1,data!AR5,IF(data!$P$1=2,data!AR5*3.412141633,)),0))","v":343},{"$f":"IF(data!AR5>data!AL5,\"\",IF(data!$P$1=1,ROUND(data!AO5,0),IF(data!$P$1=2,ROUND(data!AO5/272.7654,1),)))","v":147},{"$f":"IF(data!AR5>data!AL5,\"\",IF(data!$P$1=1,data!AU5,IF(data!$P$1=2,data!AU5*0.334552563,)))","v":{"v":7.214284956260687,"d":"7.21"}},{"$f":"data!I5","v":{"v":30,"d":"30.0"}},{"$f":"J20+8","v":{"v":38,"d":"38.0"}},{"$f":"data!AY5","v":29.4},{"$f":"data!AW5","v":{"v":2.9,"d":"2.90"}}]
[null,{"$f":"data!V8","v":3},{"$f":"data!BJ5","v":{"v":9,"d":"9.0"}},{"$f":"ROUND(IF(data!$P$1=1,data!V5,IF(data!$P$1=2,data!V5*3.412141633,)),0)","v":1536},{"$f":"IF(data!$P$1=1,ROUND(data!Z5,0),IF(data!$P$1=2,ROUND(data!Z5/272.7654,1),))","v":264},{"$f":"IF(data!$P$1=1,data!AD5,IF(data!$P$1=2,data!AD5*0.334552563,))","v":{"v":20.33361557989624,"d":"20.33"}},{"$f":"IF(data!AS5>data!AM5,\"\",ROUND(IF(data!$P$1=1,data!AS5,IF(data!$P$1=2,data!AS5*3.412141633,)),0))","v":403},{"$f":"IF(data!AS5>data!AM5,\"\",IF(data!$P$1=1,ROUND(data!AP5,0),IF(data!$P$1=2,ROUND(data!AP5/272.7654,1),)))","v":173},{"$f":"IF(data!AS5>data!AM5,\"\",IF(data!$P$1=1,data!AV5,IF(data!$P$1=2,data!AV5*0.334552563,)))","v":{"v":9.623957351948448,"d":"9.62"}},{"$f":"data!J5","v":{"v":38.12842680822206,"d":"38.1"}},{"$f":"J21+8","v":{"v":46.12842680822206,"d":"46.1"}},{"$f":"data!AZ5","v":36.8},{"$f":"data!AW5","v":{"v":2.9,"d":"2.90"}}]
[null,"*",{"$f":"IF(data!$R$2=1,NL!A20,IF(data!$R$2=2,EN!A20,IF(data!$R$2=3,DE!A20,IF(data!$R$2=4,FR!A20,IF(data!$R$2=5,NR!A20,IF(data!$R$2=6,SP!A20,IF(data!$R$2=7,SW!A20,IF(data!$R$2=8,TS!A20,IF(data!$R$2=9,ExtraTaal1!A20,IF(data!$R$2=10,ExtraTaal2!A20,IF(data!$R$2=11,ExtraTaal3!A20,)))))))))))","v":"Values according to EN 16430"},{"$nulls":9},"v2023-06-16"]
[null,"**",{"$f":"IF(data!$R$2=1,NL!A21,IF(data!$R$2=2,EN!A21,IF(data!$R$2=3,DE!A21,IF(data!$R$2=4,FR!A21,IF(data!$R$2=5,NR!A21,IF(data!$R$2=6,SP!A21,IF(data!$R$2=7,SW!A21,IF(data!$R$2=8,TS!A21,IF(data!$R$2=9,ExtraTaal1!A21,IF(data!$R$2=10,ExtraTaal2!A21,IF(data!$R$2=11,ExtraTaal3!A21,)))))))))))","v":"Sound power according to ISO 3741:2010"}]
[null,"***",{"$f":"IF(data!$R$2=1,NL!A22,IF(data!$R$2=2,EN!A22,IF(data!$R$2=3,DE!A22,IF(data!$R$2=4,FR!A22,IF(data!$R$2=5,NR!A22,IF(data!$R$2=6,SP!A22,IF(data!$R$2=7,SW!A22,IF(data!$R$2=8,TS!A22,IF(data!$R$2=9,ExtraTaal1!A22,IF(data!$R$2=10,ExtraTaal2!A22,IF(data!$R$2=11,ExtraTaal3!A22,)))))))))))","v":"Sound pressure with an assumed room damping of 8dB(A)"}]
{"$rows_empty":318}
[{"$nulls":12},true]

{"sheet":"data","index":1,"n_rows":981,"n_cols":75,"rows_kept":981,"hidden":true}
[{"$nulls":10},"heating","Ti",{"$f":"IF($P$1=1,$N1,IF($P$1=2,(N1-32)/1.8,))","v":35},{"$f":"'Mini Canal'!E10","v":35},null,1,{"$nulls":7},"Mini Canal","Mini Canal Pro","Mini Canal Hybrid",{"$nulls":4},"cooling","Ti",{"$f":"IF($P$1=1,$AH1,IF($P$1=2,($AH1-32)/1.8,))","v":16},{"$f":"'Mini Canal'!J10","v":16},{"$nulls":10},{"$error":"#VALUE!"},{"$nulls":5},"Nederlands","English","Deutsch","Français","Norsk","Español","Svenska","Čeština","ExtraTaal1","ExtraTaal2","ExtraTaal3"]
[{"$nulls":11},"Tr",{"$f":"IF($P$1=1,$N2,IF($P$1=2,(N2-32)/1.8,))","v":30},{"$f":"'Mini Canal'!E11","v":30},null,"SI/Imperial",null,{"$f":"IF('Mini Canal'!J4=data!AY1,1,IF('Mini Canal'!J4=data!AZ1,2,IF('Mini Canal'!J4=data!BA1,3,IF('Mini Canal'!J4=data!BB1,4,IF('Mini Canal'!J4=data!BC1,5,IF('Mini Canal'!J4=data!BD1,6,IF('Mini Canal'!J4=data!BE1,7,IF('Mini Canal'!J4=data!BF1,8,IF('Mini Canal'!J4=data!BG1,9,IF('Mini Canal'!J4=data!BH1,10,IF('Mini Canal'!J4=data!BI1,11,\"ERROR\")))))))))))","v":2},{"$nulls":5},{"$f":"IF('Mini Canal'!J5=data!X1,2,IF('Mini Canal'!J5=data!Y1,3,IF('Mini Canal'!J5=data!Z1,1,)))","v":1},null,null,{"$f":"IF(R2=1,\"Statisch\",IF(R2=2,\"Static\",IF(R2=3,\"Statisch\",IF(R2=4,\"Statique\",IF(R2=5,\"Statisk\",IF(R2=6,\"Estático\",IF(R2=7,\"Statisk\",\"ERROR\")))))))","v":"Static"},{"$nulls":4},"Tr",{"$f":"IF($P$1=1,$AH2,IF($P$1=2,($AH2-32)/1.8,))","v":18},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":36},"Hoogte","lengte","breedte",null,{"$f":"IF($R$2=1,NL!Q7,IF($R$2=2,EN!Q7,IF($R$2=3,DE!Q7,IF($R$2=4,FR!Q7,IF($R$2=5,NR!Q7,IF($R$2=6,SP!Q7,IF($R$2=7,SW!Q7,IF($R$2=8,TS!Q7,IF($R$2=9,ExtraTaal1!Q7,IF($R$2=10,ExtraTaal2!Q7,IF($R$2=11,ExtraTaal3!Q7,)))))))))))","v":"Copy all data"}]
[{"$nulls":11},"Ta",{"$f":"IF($P$1=1,$N3,IF($P$1=2,(N3-32)/1.8,))","v":20},{"$f":"'Mini Canal'!E12","v":20},{"$nulls":17},"Ta",{"$f":"IF($P$1=1,$AH3,IF($P$1=2,($AH3-32)/1.8,))","v":26.999999999999996},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}},{"$nulls":36},"geselecteerd",{"$nulls":3},{"$f":"IF($R$2=1,NL!Q8,IF($R$2=2,EN!Q8,IF($R$2=3,DE!Q8,IF($R$2=4,FR!Q8,IF($R$2=5,NR!Q8,IF($R$2=6,SP!Q8,IF($R$2=7,SW!Q8,IF($R$2=8,TS!Q8,IF($R$2=9,ExtraTaal1!Q8,IF($R$2=10,ExtraTaal2!Q8,IF($R$2=11,ExtraTaal3!Q8,)))))))))))","v":"SI-units"}]
["kolomindex",2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,62,63,64,65,66,67,null,null,{"$f":"IF('Mini Canal'!$J$5=data!$X$1,\"Standaard\",IF('Mini Canal'!$J$5=data!$Y$1,\"PRO\",IF('Mini Canal'!$J$5=data!$Z$1,\"DBE\",)))","v":"DBE"},{"$f":"CONCATENATE($BS$4,\"_L\")","v":"DBE_L"},{"$f":"CONCATENATE($BS$4,\"_B\")","v":"DBE_B"},null,{"$f":"IF($R$2=1,NL!Q9,IF($R$2=2,EN!Q9,IF($R$2=3,DE!Q9,IF($R$2=4,FR!Q9,IF($R$2=5,NR!Q9,IF($R$2=6,SP!Q9,IF($R$2=7,SW!Q9,IF($R$2=8,TS!Q9,IF($R$2=9,ExtraTaal1!Q9,IF($R$2=10,ExtraTaal2!Q9,IF($R$2=11,ExtraTaal3!Q9,)))))))))))","v":"Imperial-units"}]
[{"$f":"CONCATENATE('Mini Canal'!J6,'Mini Canal'!L6,'Mini Canal'!K6,$X$2)","v":"14290341"},{"$f":"VLOOKUP($A$5,$A$9:$BK$981,B4,0)","v":14},290,1,34,15,0,26,30,38.12842680822206,1227,5665,6295,7138,1.362,1.1,1.1,1.1,183,1219,1355,{"$f":"VLOOKUP($A$5,$A$9:$BK$981,V4,0)","v":1536},31,210,233,264,0.4596260269960454,13.56176252546608,16.30047092944978,20.33361557989624,292,343,403,0.98,0.98,0.98,292,343,403,126,147,173,292,343,403,5.492030247267677,7.214284956260687,9.623957351948448,2.9,26.5,29.4,36.8,0,0,506,576,757,0,0,6.0515594714640155,6.87363114546986,9,{"$f":"VLOOKUP($A$5,$A$9:$BK$981,BK4,0)","v":9},{"$f":"VLOOKUP($A$5,$A$9:$BP$981,BL4,0)","v":0},{"$f":"VLOOKUP($A$5,$A$9:$BP$981,BM4,0)","v":0},{"$f":"VLOOKUP($A$5,$A$9:$BP$981,BN4,0)","v":0.00019563320356262},{"$f":"VLOOKUP($A$5,$A$9:$BP$981,BO4,0)","v":4.4708458846471E-4},{"$f":"VLOOKUP($A$5,$A$9:$BP$981,BP4,0)","v":1.766459432507}]
[]
[{"$nulls":5},"Type","soundpressure level",{"$nulls":3},"power","75/65/20",null,null,"n",{"$nulls":3},"result","power",null,null,"result","flow",{"$nulls":5},"dP","power","16/18/27",null,"n",null,null,"result","power",null,"result","flow",null,"Total power, result",{"$nulls":4},"dP","Water content","electrical power nominal",{"$nulls":4},"Airflow",{"$nulls":5},"BMS-stuurspanning"]
["lookup code","height","length","DBE?","depth","WW",0,1,2,3,0,1,2,3,0,1,2,3,0,1,2,3,0,1,2,3,0,1,2,3,1,2,3,1,2,3,1,2,3,1,2,3,1,2,3,1,2,3,null,1,2,3,null,0,1,2,3,null,0,1,2,3,null,null,"k1","k2","x","t"]
[{"$f":"CONCATENATE(B9,C9,E9,D9)","v":"1470261"},14,70,1,26,{"$f":"IF($E9=26,10,IF($E9=34,15,IF($E9=42,20,)))","v":10},0,21.228787452803378,25.22878745280341,{"v":30.974299956639804,"d":"31.0"},143,517,550,570,1.362,1.1,1.1,1.1,{"$f":"ROUND(K9*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O9),0)","v":21},111,118,123,{"$f":"ROUND(S9*3600/(4186*ABS($M$1-$M$2)),0)","v":4},19,20,21,{"$f":"0.0098*(($BM9*(W9^$BO9)*($C9-14.4)*$BP9)+($BN9*W9*W9))","v":0.012474492861344375},{"$f":"0.0098*(($BM9*(X9^$BO9)*($C9-14.4)*$BP9)+($BN9*X9*X9))","v":0.1272664460194499},{"$f":"0.0098*(($BM9*(Y9^$BO9)*($C9-14.4)*$BP9)+($BN9*Y9*Y9))","v":0.13739099657002593},0.1477689797580916,49,52,{"v":51.800000000000004,"d":"52"},0.98,0.98,0.98,{"$f":"ROUND(AE9*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH9),0)","v":49},{"$f":"ROUND(AF9*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI9),0)","v":52},{"$f":"ROUND(AG9*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ9),0)","v":52},{"$f":"ROUND(AK9*3600/(4186*ABS($AG$1-$AG$2)),0)","v":21},{"$f":"ROUND(AL9*3600/(4186*ABS($AG$1-$AG$2)),0)","v":22},{"$f":"ROUND(AM9*3600/(4186*ABS($AG$1-$AG$2)),0)","v":22},{"$f":"(AK9/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":49},{"$f":"(AL9/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":52},{"$f":"(AM9/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":52},{"$f":"0.0098*(($BM9*(AN9^$BO9)*($C9-14.4)*$BP9)+($BN9*AN9*AN9))","v":0.1477689797580916},{"$f":"0.0098*(($BM9*(AO9^$BO9)*($C9-14.4)*$BP9)+($BN9*AO9*AO9))","v":0.1583943094552189},{"$f":"0.0098*(($BM9*(AP9^$BO9)*($C9-14.4)*$BP9)+($BN9*AP9*AP9))","v":0.1583943094552189},{"$f":"IF($F9=$BR$70,$C9*$BS$70,IF($F9=$BR$71,$C9*$BS$71,IF($F9=$BR$72,$C9*$BS$72,IF($F9=$BR$73,$C9*$BS$73,IF($F9=$BR$74,$C9*$BS$74,IF($F9=$BR$75,$C9*$BS$75,IF($F9=$BR$76,$C9*$BS$76,IF($F9=$BR$77,$C9*$BS$77,IF($F9=$BR$78,$C9*$BS$78,IF($F9=$BR$79,$C9*$BS$79,IF($F9=$BR$80,$C9*$BS$80,)))))))))))","v":{"v":0.4666666666666667,"d":"0.47"}},{"$f":"(0.1175*$C9)-4.485","v":{"v":3.7399999999999993,"d":"3.7"}},{"$f":"(0.1312*$C9)-5.1167","v":{"v":4.067300000000001,"d":"4.1"}},{"$f":"(0.1832*$C9)-8.1317","v":{"v":4.6922999999999995,"d":"4.7"}},null,0,{"$f":"(2.215*$C9)-76.45","v":78.59999999999998},{"$f":"($C9*2.515)-85.45","v":90.60000000000001},{"$f":"($C9*3.83)-161.5","v":106.60000000000002},null,0,7.245893006319797,8.270521810264206,10,null,null,{"$f":"IF($F9=$BR$70,$BT$70,IF($F9=$BR$71,$BT$71,IF($F9=$BR$72,$BT$72,IF($F9=$BR$73,$BT$73,IF($F9=$BR$74,$BT$74,IF($F9=$BR$75,$BT$75,IF($F9=$BR$76,$BT$76,IF($F9=$BR$77,$BT$77,IF($F9=$BR$78,$BT$78,IF($F9=$BR$79,$BT$79,IF($F9=$BR$80,$BT$80,)))))))))))","v":0.0014501879713726},{"$f":"IF($F9=$BR$70,$BU$70,IF($F9=$BR$71,$BU$71,IF($F9=$BR$72,$BU$72,IF($F9=$BR$73,$BU$73,IF($F9=$BR$74,$BU$74,IF($F9=$BR$75,$BU$75,IF($F9=$BR$76,$BU$76,IF($F9=$BR$77,$BU$77,IF($F9=$BR$78,$BU$78,IF($F9=$BR$79,$BU$79,IF($F9=$BR$80,$BU$80,)))))))))))","v":0.00037831632653061},{"$f":"IF($F9=$BR$70,$BV$70,IF($F9=$BR$71,$BV$71,IF($F9=$BR$72,$BV$72,IF($F9=$BR$73,$BV$73,IF($F9=$BR$74,$BV$74,IF($F9=$BR$75,$BV$75,IF($F9=$BR$76,$BV$76,IF($F9=$BR$77,$BV$77,IF($F9=$BR$78,$BV$78,IF($F9=$BR$79,$BV$79,IF($F9=$BR$80,$BV$80,)))))))))))","v":1.4868910444209},{"$f":"IF($F9=$BR$70,$BW$70,IF($F9=$BR$71,$BW$71,IF($F9=$BR$72,$BW$72,IF($F9=$BR$73,$BW$73,IF($F9=$BR$74,$BW$74,IF($F9=$BR$75,$BW$75,IF($F9=$BR$76,$BW$76,IF($F9=$BR$77,$BW$77,IF($F9=$BR$78,$BW$78,IF($F9=$BR$79,$BW$79,IF($F9=$BR$80,$BW$80,)))))))))))","v":2}]
["1470341",14,70,1,34,{"$f":"IF($E10=26,10,IF($E10=34,15,IF($E10=42,20,)))","v":15},0,21.228787452803378,25.22878745280341,{"v":30.974299956639804,"d":"31.0"},188,670,711,726,1.362,1.1,1.1,1.1,28,144,153,156,5,25,26,27,{"$f":"0.0098*(($BM10*(W10^$BO10)*($C10-14.4)*$BP10)+($BN10*W10*W10))","v":3.7694893856778672E-3},0.06556993884066971,{"$f":"0.0098*(($BM10*(Y10^$BO10)*($C10-14.4)*$BP10)+($BN10*Y10*Y10))","v":0.07030081252003907},{"$f":"0.0098*(($BM10*(Z10^$BO10)*($C10-14.4)*$BP10)+($BN10*Z10*Z10))","v":0.07517532298995575},56,61,61,0.98,0.98,0.98,56,61,61,24,26,26,{"$f":"(AK10/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":56},{"$f":"(AL10/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":61},{"$f":"(AM10/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":61},{"$f":"0.0098*(($BM10*(AN10^$BO10)*($C10-14.4)*$BP10)+($BN10*AN10*AN10))","v":0.0609839434167593},{"$f":"0.0098*(($BM10*(AO10^$BO10)*($C10-14.4)*$BP10)+($BN10*AO10*AO10))","v":0.07030081252003907},{"$f":"0.0098*(($BM10*(AP10^$BO10)*($C10-14.4)*$BP10)+($BN10*AP10*AP10))","v":0.07030081252003907},{"v":0.7000000000000001,"d":"0.70"},{"$f":"(0.1175*$C10)-4.485","v":{"v":3.7399999999999993,"d":"3.7"}},{"$f":"(0.1312*$C10)-5.1167","v":{"v":4.067300000000001,"d":"4.1"}},{"$f":"(0.1832*$C10)-8.1317","v":{"v":4.6922999999999995,"d":"4.7"}},null,0,{"$f":"(2.215*$C10)-76.45","v":78.59999999999998},{"$f":"($C10*2.515)-85.45","v":90.60000000000001},{"$f":"($C10*3.83)-161.5","v":106.60000000000002},null,0,7.245893006319797,8.270521810264206,10,null,null,{"$f":"IF($F10=$BR$70,$BT$70,IF($F10=$BR$71,$BT$71,IF($F10=$BR$72,$BT$72,IF($F10=$BR$73,$BT$73,IF($F10=$BR$74,$BT$74,IF($F10=$BR$75,$BT$75,IF($F10=$BR$76,$BT$76,IF($F10=$BR$77,$BT$77,IF($F10=$BR$78,$BT$78,IF($F10=$BR$79,$BT$79,IF($F10=$BR$80,$BT$80,)))))))))))","v":0.00019563320356262},{"$f":"IF($F10=$BR$70,$BU$70,IF($F10=$BR$71,$BU$71,IF($F10=$BR$72,$BU$72,IF($F10=$BR$73,$BU$73,IF($F10=$BR$74,$BU$74,IF($F10=$BR$75,$BU$75,IF($F10=$BR$76,$BU$76,IF($F10=$BR$77,$BU$77,IF($F10=$BR$78,$BU$78,IF($F10=$BR$79,$BU$79,IF($F10=$BR$80,$BU$80,)))))))))))","v":4.4708458846471E-4},{"$f":"IF($F10=$BR$70,$BV$70,IF($F10=$BR$71,$BV$71,IF($F10=$BR$72,$BV$72,IF($F10=$BR$73,$BV$73,IF($F10=$BR$74,$BV$74,IF($F10=$BR$75,$BV$75,IF($F10=$BR$76,$BV$76,IF($F10=$BR$77,$BV$77,IF($F10=$BR$78,$BV$78,IF($F10=$BR$79,$BV$79,IF($F10=$BR$80,$BV$80,)))))))))))","v":1.766459432507},{"$f":"IF($F10=$BR$70,$BW$70,IF($F10=$BR$71,$BW$71,IF($F10=$BR$72,$BW$72,IF($F10=$BR$73,$BW$73,IF($F10=$BR$74,$BW$74,IF($F10=$BR$75,$BW$75,IF($F10=$BR$76,$BW$76,IF($F10=$BR$77,$BW$77,IF($F10=$BR$78,$BW$78,IF($F10=$BR$79,$BW$79,IF($F10=$BR$80,$BW$80,)))))))))))","v":2}]
["1470421",14,70,1,42,20,0,21.228787452803378,25.22878745280341,{"v":30.974299956639804,"d":"31.0"},233,792,838,855,1.362,1.1,1.1,1.1,35,170,180,184,6,29,31,32,0.021313433516572066,0.186002754669839,0.20391447256706824,0.21303956834213023,30,32,32,0.98,0.98,0.98,30,32,32,13,14,14,{"$f":"(AK11/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":30},{"$f":"(AL11/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":32},{"$f":"(AM11/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":32},0.061645085901544945,0.06825726703240045,0.06825726703240045,{"v":0.9333333333333333,"d":"0.93"},{"v":3.7399999999999993,"d":"3.7"},{"v":4.067300000000001,"d":"4.1"},{"v":4.6922999999999995,"d":"4.7"},null,0,78.59999999999998,90.60000000000001,106.60000000000002,null,0,7.245893006319797,8.270521810264206,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["1480261",14,80,1,26,10,0,24.239087409443187,28.239087409443215,33.98459991327962,178,927,991,1033,1.362,1.1,1.1,1.1,27,199,213,222,5,34,37,38,0.020504259301806473,0.35724668676814364,0.405323694829561,0.4217915716522394,61,65,{"v":64.75,"d":"65"},0.98,0.98,0.98,61,65,65,26,28,28,{"$f":"(AK12/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":61},{"$f":"(AL12/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":65},{"$f":"(AM12/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":65},0.2393682789635703,0.26736091480682406,0.26736091480682406,{"v":0.5333333333333333,"d":"0.53"},{"v":4.914999999999998,"d":"4.9"},{"v":5.379300000000001,"d":"5.4"},{"v":6.5243,"d":"6.5"},null,0,100.74999999999999,115.75000000000001,144.89999999999998,null,0,7.245893006319797,8.27052181026421,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1480341",14,80,1,34,15,0,24.239087409443187,28.239087409443215,33.98459991327962,235,1198,1280,1311,1.362,1.1,1.1,1.1,{"$f":"ROUND(K13*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O13),0)","v":35},{"$f":"ROUND(L13*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P13),0)","v":258},{"$f":"ROUND(M13*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q13),0)","v":275},282,{"$f":"ROUND(S13*3600/(4186*ABS($M$1-$M$2)),0)","v":6},44,47,49,0.006116754880905961,0.20971348091226538,0.2357759466268188,0.25388882675059216,69,76,76,0.98,0.98,0.98,69,76,76,30,33,33,{"$f":"(AK13/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":69},{"$f":"(AL13/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":76},{"$f":"(AM13/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":76},0.1062436669829139,0.12583000479754045,0.12583000479754045,{"v":0.8,"d":"0.80"},{"v":4.914999999999998,"d":"4.9"},{"v":5.379300000000001,"d":"5.4"},{"v":6.5243,"d":"6.5"},null,0,100.74999999999999,115.75000000000001,144.89999999999998,null,0,7.2458930063198,8.27052181026421,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["1480421",14,80,1,42,20,0,24.239087409443187,28.239087409443215,33.98459991327962,291,1408,1500,1535,1.362,1.1,1.1,1.1,43,303,323,330,7,52,56,57,0.03104478166721315,0.48978243602075383,0.5425502189443238,0.5559753436495258,60,64,64,0.98,0.98,0.98,60,64,64,26,28,28,{"$f":"(AK14/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":60},{"$f":"(AL14/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":64},{"$f":"(AM14/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":64},0.18840398205268113,0.2086398511771051,0.2086398511771051,{"v":1.0666666666666667,"d":"1.07"},{"v":4.914999999999998,"d":"4.9"},{"v":5.379300000000001,"d":"5.4"},{"v":6.5243,"d":"6.5"},null,0,100.74999999999999,115.75000000000001,144.89999999999998,null,0,7.2458930063198,8.27052181026421,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["1490261",14,90,1,26,10,0,24.239087409443187,28.239087409443215,33.98459991327962,214,963,1027,1069,1.362,1.1,1.1,1.1,32,207,221,230,6,36,38,40,0.030981560817359595,0.44765264320206183,0.48527296519678814,0.5238855560838587,73,78,{"v":77.7,"d":"78"},0.98,0.98,0.98,73,78,78,31,34,34,{"$f":"(AK15/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":73},{"$f":"(AL15/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":78},{"$f":"(AM15/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":78},0.35812680441442796,0.41105168932426306,0.41105168932426306,{"v":0.6000000000000001,"d":"0.60"},{"v":6.089999999999999,"d":"6.1"},{"v":6.691300000000002,"d":"6.7"},{"v":8.3563,"d":"8.4"},null,0,122.89999999999999,140.90000000000003,183.2,null,0,7.2458930063198,8.27052181026421,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1490341",14,90,1,34,15,0,26,30,33.98459991327962,282,1245,1328,1358,1.362,1.1,1.1,1.1,42,268,286,292,7,46,49,50,0.009231477582349023,0.2601214409876896,0.2909877620861006,0.3016114000158458,83,91,91,0.98,0.98,0.98,83,91,91,36,39,39,{"$f":"(AK16/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":83},{"$f":"(AL16/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":91},{"$f":"(AM16/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":91},0.16837013258769398,0.19406498618925894,0.19406498618925894,{"v":0.9,"d":"0.90"},{"v":6.089999999999999,"d":"6.1"},{"v":6.691300000000002,"d":"6.7"},{"v":8.3563,"d":"8.4"},null,0,122.89999999999999,140.90000000000003,183.2,null,0,7.2458930063198,8.27052181026421,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["1490421",14,90,1,42,20,0,26,30,33.98459991327962,350,1467,1558,1593,1.362,1.1,1.1,1.1,52,316,{"$f":"ROUND(M17*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q17),0)","v":335},{"$f":"ROUND(N17*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R17),0)","v":343},{"$f":"ROUND(S17*3600/(4186*ABS($M$1-$M$2)),0)","v":9},{"$f":"ROUND(T17*3600/(4186*ABS($M$1-$M$2)),0)","v":54},{"$f":"ROUND(U17*3600/(4186*ABS($M$1-$M$2)),0)","v":58},{"$f":"ROUND(V17*3600/(4186*ABS($M$1-$M$2)),0)","v":59},0.050475660483342656,0.5931984439188136,0.6546496947214655,0.6702731960795403,60,64,64,0.98,0.98,0.98,60,64,64,26,28,28,{"$f":"(AK17/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":60},{"$f":"(AL17/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":64},{"$f":"(AM17/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":64},0.21679155323413588,0.24005902952974664,0.24005902952974664,{"v":1.2000000000000002,"d":"1.20"},{"v":6.089999999999999,"d":"6.1"},{"v":6.691300000000002,"d":"6.7"},{"v":8.3563,"d":"8.4"},null,0,122.89999999999999,140.90000000000003,183.2,null,0,7.2458930063198,8.27052181026421,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14100261",14,100,1,26,10,0,26,30,35.74551250383643,251,1375,1471,1534,1.362,1.1,1.1,1.1,37,296,317,330,6,51,55,57,0.03506199611066113,0.8512804351534938,0.9528528739568339,1.0050444879105715,86,91,{"v":90.64999999999999,"d":"91"},0.98,0.98,0.98,86,91,91,37,39,39,{"$f":"(AK18/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":86},{"$f":"(AL18/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":91},{"$f":"(AM18/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":91},0.5273505629178418,0.5704380174353442,0.5704380174353442,{"v":0.6666666666666667,"d":"0.67"},{"v":7.265,"d":"7.3"},{"v":8.003300000000001,"d":"8.0"},{"v":10.1883,"d":"10.2"},null,0,145.05,166.05,{"$f":"($C18*3.83)-191.5","v":191.5},null,0,7.2458930063198,8.27052181026421,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14100341",14,100,1,34,15,0,26,30,35.74551250383643,331,1776,1899,1945,1.362,1.1,1.1,1.1,49,382,409,419,8,66,70,72,0.013205818497395473,0.5565167976473344,0.6177668463947412,0.6494352848143417,97,106,106,0.98,0.98,0.98,97,106,106,42,46,46,{"$f":"(AK19/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":97},{"$f":"(AL19/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":106},{"$f":"(AM19/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":106},0.2495957322177884,0.29330270253446394,0.29330270253446394,{"v":1,"d":"1.00"},{"v":7.265,"d":"7.3"},{"v":8.003300000000001,"d":"8.0"},{"v":10.1883,"d":"10.2"},null,0,145.05,166.05,191.5,null,0,7.2458930063198,8.27052181026421,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14100421",14,100,1,42,20,0,26,30,35.74551250383643,411,2086,2224,2276,1.362,1.1,1.1,1.1,61,449,479,490,10,77,82,84,0.06600212420266471,1.0936017559358464,1.1928256219216933,1.2331815126101726,89,96,96,0.98,0.98,0.98,89,96,96,38,41,41,{"$f":"(AK20/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":89},{"$f":"(AL20/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":96},{"$f":"(AM20/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":96},0.41322073237104706,0.4587813653728488,0.4587813653728488,{"v":1.3333333333333335,"d":"1.33"},{"v":7.265,"d":"7.3"},{"v":8.003300000000001,"d":"8.0"},{"v":10.1883,"d":"10.2"},null,0,145.05,166.05,191.5,null,0,7.2458930063198,8.27052181026421,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14110261",14,110,1,26,10,0,26,30,35.74551250383643,285,1409,1505,1568,1.362,1.1,1.1,1.1,43,303,324,337,7,52,56,58,0.049239343377749274,0.9775190479956335,1.0918247564265802,1.1505278216448729,98,103,{"v":103.60000000000001,"d":"104"},0.98,0.98,0.98,98,103,104,42,44,45,{"$f":"(AK21/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":98},{"$f":"(AL21/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":103},{"$f":"(AM21/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":104},0.7108001476413914,0.761875945358432,0.7878499768650176,{"v":0.7333333333333334,"d":"0.73"},8.4,9.4,{"v":11,"d":"11.0"},null,0,166,190,230,null,0,7.2458930063198,8.270521810264206,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14110341",14,110,1,34,15,0,26,30,35.74551250383643,376,1821,1944,1990,1.362,1.1,1.1,1.1,56,392,418,428,10,67,72,74,0.021848108168779724,0.6360412114839971,0.7226504667126655,0.7586394068793433,111,121,122,0.98,0.98,0.98,111,121,122,48,52,52,{"$f":"(AK22/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":111},{"$f":"(AL22/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":121},{"$f":"(AM22/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":122},0.35207502057754325,0.4057662879305438,0.4057662879305438,{"v":1.1,"d":"1.10"},8.4,9.4,{"v":11,"d":"11.0"},null,0,166,190,230,null,0,7.2458930063198,8.270521810264206,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14110421",14,110,1,42,20,0,26,30,35.74551250383643,466,2141,2279,2332,1.362,1.1,1.1,1.1,{"$f":"ROUND(K23*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O23),0)","v":70},461,490,502,12,79,84,86,0.09461608123208196,1.26300947121311,1.3745846833994466,1.4199430804993158,89,96,96,0.98,0.98,0.98,89,96,96,38,41,41,{"$f":"(AK23/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":89},{"$f":"(AL23/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":96},{"$f":"(AM23/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":96},0.460949798910589,0.5117435875056905,0.5117435875056905,{"v":1.4666666666666668,"d":"1.47"},8.4,9.4,{"v":11,"d":"11.0"},null,0,166,190,230,null,0,7.2458930063198,8.270521810264206,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14120261",14,120,1,26,10,0,26,30,36.99489986991943,335,1787,1925,2045,1.362,1.1,1.1,1.1,{"$f":"ROUND(K24*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O24),0)","v":50},385,414,440,9,66,71,76,0.07904094554017056,1.5395285413037345,1.716791406724147,1.9003383506789056,108,115,{"v":116.55,"d":"117"},0.98,0.98,0.98,108,115,117,46,49,50,{"$f":"(AK24/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":108},{"$f":"(AL24/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":115},{"$f":"(AM24/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":117},0.8984477897518957,0.9872234438840091,1.0174243626306168,{"v":0.8,"d":"0.80"},{"$f":"(0.1175*$C24)-4.485","v":{"v":9.614999999999998,"d":"9.6"}},{"v":10.627300000000002,"d":"10.6"},{"v":13.852300000000001,"d":"13.9"},null,0,{"$f":"(2.215*$C24)-76.45","v":189.34999999999997},{"$f":"($C24*2.515)-85.45","v":216.35000000000002},{"$f":"($C24*3.83)-191.5","v":268.1},null,0,6.960594861911879,7.930446398428071,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14120341",14,120,1,34,15,0,26,30,36.99489986991943,442,2305,2488,2593,1.362,1.1,1.1,1.1,66,496,535,558,11,85,92,96,0.0285161308735637,1.0682358043280231,1.2291882558605745,1.3255601821796497,120,133,137,0.98,0.98,0.98,120,133,137,52,57,59,{"$f":"(AK25/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":120},{"$f":"(AL25/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":133},{"$f":"(AM25/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":137},0.44697119420710235,0.5259692445436212,0.5591288825574118,{"v":1.2,"d":"1.20"},{"v":9.614999999999998,"d":"9.6"},{"v":10.627300000000002,"d":"10.6"},{"v":13.852300000000001,"d":"13.9"},null,0,189.34999999999997,216.35000000000002,268.1,null,0,6.960594861911879,7.930446398428071,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14120421",14,120,1,42,20,0,26,30,36.99489986991943,547,2711,2915,3034,1.362,1.1,1.1,1.1,82,583,627,653,14,100,108,112,0.1290708971910842,1.9280960179411648,2.14414033418327,2.2545261522047557,115,126,128,0.98,0.98,0.98,115,126,128,49,54,55,{"$f":"(AK26/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":115},{"$f":"(AL26/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":126},{"$f":"(AM26/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":128},0.7216218068665896,0.8248604438076913,0.845958474903727,{"v":1.6,"d":"1.60"},{"v":9.614999999999998,"d":"9.6"},{"v":10.627300000000002,"d":"10.6"},{"v":13.852300000000001,"d":"13.9"},null,0,189.34999999999997,216.35000000000002,268.1,null,0,6.960594861911879,7.930446398428071,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14130261",14,130,1,26,10,0,26,30,36.99489986991943,359,1810,1949,2068,1.362,1.1,1.1,1.1,54,390,419,445,9,67,72,77,0.08649744535458066,1.7219888405995782,1.917189312481924,2.11920359257698,120,128,{"v":129.5,"d":"130"},0.98,0.98,0.98,120,128,130,52,55,56,{"$f":"(AK27/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":120},{"$f":"(AL27/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":128},{"$f":"(AM27/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":130},1.1799236438106198,1.2828660818272195,1.3178076092354882,{"v":0.8666666666666667,"d":"0.87"},10.8,{"v":12,"d":"12.0"},14.7,null,0,212,242,306,null,0,6.960594861911879,7.930446398428071,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14130341",14,130,1,34,15,0,26,30,36.99489986991943,473,2336,2519,2624,1.362,1.1,1.1,1.1,71,503,542,565,12,87,93,97,0.036357087805478215,1.2154926033065978,1.3680484265103714,1.4740993272567449,134,148,152,0.98,0.98,0.98,134,148,152,58,64,65,{"$f":"(AK28/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":134},{"$f":"(AL28/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":148},{"$f":"(AM28/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":152},0.5924100194506847,0.7053314489023773,0.7249825896988851,{"v":1.3,"d":"1.30"},10.8,{"v":12,"d":"12.0"},14.7,null,0,212,242,306,null,0,6.960594861911879,7.930446398428071,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14130421",14,130,1,42,20,0,26,30,36.99489986991943,586,2749,2953,3072,1.362,1.1,1.1,1.1,87,592,635,661,15,102,109,114,0.15525643939683478,2.1659682004427023,2.3736038363727263,2.5251015667770647,115,126,128,0.98,0.98,0.98,115,126,128,49,54,55,{"$f":"(AK29/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":115},{"$f":"(AL29/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":126},{"$f":"(AM29/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":128},0.7892234693420891,0.9020811104373171,0.9251437511849864,{"v":1.7333333333333334,"d":"1.73"},10.8,{"v":12,"d":"12.0"},14.7,null,0,212,242,306,null,0,6.960594861911879,7.930446398428071,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14150261",14,150,1,26,10,0,26,30,37.96399999999999,430,2198,2379,2567,1.362,1.1,1.1,1.1,64,473,512,552,11,81,88,95,0.13671147273156925,2.6767879557211414,3.029074774689942,3.3954746433514806,141,151,{"v":155.4,"d":"155"},0.98,0.98,0.98,141,151,155,61,65,67,{"$f":"(AK30/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":141},{"$f":"(AL30/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":151},{"$f":"(AM30/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":155},1.7537225071032394,1.9279142937656535,2.017031379198121,{"v":1,"d":"1.00"},13.2,14.6,18.3,null,0,257,293,383,null,0,6.748591169784535,7.6795991751328705,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14150341",14,150,1,34,15,0,26,30,37.96399999999999,566,2831,3076,3256,1.362,1.1,1.1,1.1,84,609,662,701,14,105,114,121,0.055882107412772754,1.9816407733691246,2.2925575392119653,2.547934593310699,155,174,182,0.98,0.98,0.98,155,174,182,67,75,78,{"$f":"(AK31/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":155},{"$f":"(AL31/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":174},{"$f":"(AM31/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":182},0.8939378545180305,1.0916788618611046,1.1702369675071707,{"v":1.5,"d":"1.50"},13.2,14.6,18.3,null,0,257,293,383,null,0,6.748591169784535,7.6795991751328705,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14150421",14,150,1,42,20,0,26,30,37.96399999999999,702,3334,3607,3810,1.362,1.1,1.1,1.1,105,717,776,820,18,123,133,141,0.2337094288806026,3.280963056797484,3.654321307441527,3.9609001591247837,140,155,160,0.98,0.98,0.98,140,155,160,60,67,69,{"$f":"(AK32/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":140},{"$f":"(AL32/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":155},{"$f":"(AM32/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":160},1.2212221192498607,1.4213738129023603,1.4800673636731172,{"v":2,"d":"2.00"},13.2,14.6,18.3,null,0,257,293,383,null,0,6.748591169784535,7.6795991751328705,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2,null,"standaard",null,"PRO",null,"DBE"]
["14170261",14,170,1,26,10,0,26,30,38.75581246047624,503,2577,2802,3067,1.362,1.1,1.1,1.1,75,555,603,660,13,95,104,114,0.20107485814440137,3.8913469819726427,4.45375926500831,5.107400341620808,161,174,{"v":181.29999999999998,"d":"181"},0.98,0.98,0.98,161,174,181,69,75,78,{"$f":"(AK33/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":161},{"$f":"(AL33/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":174},{"$f":"(AM33/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":181},2.4157012616733295,2.7354291731094427,2.9001435603408043,{"v":1.1333333333333333,"d":"1.13"},15.5,17.2,{"v":22,"d":"22.0"},null,0,301,343,460,null,0,6.580727318795408,7.482644568320627,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2,null,9,null,9,null,14]
["14170341",14,170,1,34,15,0,26,30,38.75581246047624,663,3315,3622,3890,1.362,1.1,1.1,1.1,99,713,779,837,17,123,134,144,0.09023679501737059,3.0001563791253782,3.4918008608532705,3.966712705508078,176,200,213,0.98,0.98,0.98,176,200,213,76,86,92,{"$f":"(AK34/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":176},{"$f":"(AL34/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":200},{"$f":"(AM34/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":213},1.2787055499264082,1.5916748470285405,1.7936313624345679,{"v":1.7,"d":"1.70"},15.5,17.2,{"v":22,"d":"22.0"},null,0,301,343,460,null,0,6.580727318795408,7.482644568320627,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2,null,11,null,12]
["14170421",14,170,1,42,20,0,26,30,38.75581246047624,821,3908,4249,4552,1.362,1.1,1.1,1.1,123,841,914,980,21,145,157,169,0.33113984637332533,4.7139179745082105,5.259972098011565,5.822260986923726,164,183,192,0.98,0.98,0.98,164,183,192,71,79,83,{"$f":"(AK35/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":164},{"$f":"(AL35/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":183},{"$f":"(AM35/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":192},1.764060870291305,2.0430528906503342,2.186680541964693,{"v":2.2666666666666666,"d":"2.27"},15.5,17.2,{"v":22,"d":"22.0"},null,0,301,343,460,null,0,6.580727318795408,7.482644568320627,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2,null,14,null,15]
["14190261",14,190,1,26,10,0,26,30,{"v":39.42528035678237,"d":"39.4"},587,2960,3228,3578,1.362,1.1,1.1,1.1,88,637,695,770,15,110,120,132,0.28068362736371244,5.459049388491679,6.215376109448306,7.164745310248498,181,197,{"v":207.20000000000002,"d":"207"},0.98,0.98,0.98,181,197,207,78,85,89,{"$f":"(AK36/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":181},{"$f":"(AL36/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":197},{"$f":"(AM36/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":207},3.2700133714385937,3.716907653739507,3.980625437542319,{"v":1.2666666666666668,"d":"1.27"},17.8,19.7,25.7,null,0,343,391,536,null,0,6.442201120776372,7.321401284497683,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2,null,19,null,20]
["14190341",14,190,1,34,15,0,26,30,{"v":39.42528035678237,"d":"39.4"},773,3801,4171,4539,1.362,1.1,1.1,1.1,115,818,898,977,20,141,154,168,0.1355475634426454,4.301466145680473,5.028723153148789,5.866699857095715,196,224,243,0.98,0.98,0.98,196,224,243,84,96,104,{"$f":"(AK37/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":196},{"$f":"(AL37/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":224},{"$f":"(AM37/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":243},1.7189620162176487,2.177479361132434,2.509064549341087,{"v":1.9000000000000001,"d":"1.90"},17.8,19.7,25.7,null,0,343,391,536,null,0,6.442201120776372,7.321401284497683,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14190421",14,190,1,42,20,0,26,30,{"v":39.42528035678237,"d":"39.4"},958,4485,4897,5310,1.362,1.1,1.1,1.1,143,965,1054,1143,25,166,181,197,0.4744399626441079,6.398879804610867,7.209133258832896,8.102170314813634,187,210,224,0.98,0.98,0.98,187,210,224,80,90,96,{"$f":"(AK38/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":187},{"$f":"(AL38/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":210},{"$f":"(AM38/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":224},2.3432389477245463,2.7551717253273282,3.0108989753720743,{"v":2.5333333333333337,"d":"2.53"},17.8,19.7,25.7,null,0,343,391,536,null,0,6.442201120776372,7.321401284497683,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14210261",14,210,1,26,10,0,26,30,39.42528035678237,644,3017,3285,3636,1.362,1.1,1.1,1.1,96,649,707,782,17,112,122,135,0.3765565624441472,6.241105141642494,7.089775307968622,8.245123219579515,204,222,{"v":233.1,"d":"233"},0.98,0.98,0.98,204,222,233,88,95,100,{"$f":"(AK39/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":204},{"$f":"(AL39/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":222},{"$f":"(AM39/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":233},4.3566694183580585,4.883091659214967,5.27104596606033,{"v":1.4000000000000001,"d":"1.40"},17.8,19.7,25.7,null,0,343,391,536,null,0,6.442201120776372,7.321401284497683,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14210341",14,210,1,34,15,0,26,30,39.42528035678237,849,3877,4247,4614,1.362,1.1,1.1,1.1,127,834,914,993,22,143,157,171,0.17848166959925352,4.902211303954255,5.783903162516914,6.728430354268965,220,252,274,0.98,0.98,0.98,220,252,274,95,108,118,{"$f":"(AK40/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":220},{"$f":"(AL40/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":252},{"$f":"(AM40/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":274},2.376420213167923,2.982187616780782,3.4883928981649275,{"v":2.1,"d":"2.10"},17.8,19.7,25.7,null,0,343,391,536,null,0,6.442201120776372,7.321401284497683,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2,null,14,null,14,null,26]
["14210421",14,210,1,42,20,0,26,30,39.42528035678237,1052,4579,4990,5404,1.362,1.1,1.1,1.1,157,985,1074,1163,27,169,185,200,0.5870598263489678,7.295292342669215,8.263290170445247,9.200332914234806,187,210,224,0.98,0.98,0.98,187,210,224,80,90,96,{"$f":"(AK41/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":187},{"$f":"(AL41/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":210},{"$f":"(AM41/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":224},2.607770331586274,3.065995446195145,3.3504386203708574,{"v":2.8000000000000003,"d":"2.80"},17.8,19.7,25.7,null,0,343,391,536,null,0,6.442201120776372,7.321401284497683,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2,null,18,null,18,null,34]
["14230261",14,230,1,26,10,0,26,30,40.00519982655924,717,3345,3658,4100,1.362,1.1,1.1,1.1,107,720,787,882,18,124,135,152,0.45179229181305136,8.000637891279508,9.081273938606051,10.837746264750775,223,244,259,0.98,0.98,0.98,223,244,259,96,105,111,{"$f":"(AK42/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":223},{"$f":"(AL42/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":244},{"$f":"(AM42/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":259},5.463551215658938,6.244098192554035,6.783223054435348,{"v":1.5333333333333334,"d":"1.53"},{"v":20,"d":"20.0"},22.2,29.3,null,0,385,438,613,null,0,6.324513728106023,7.18539965060231,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2,null,26,null,23,null,42]
["14230341",14,230,1,34,15,0,26,30,40.00519982655924,945,4338,4772,5248,1.362,1.1,1.1,1.1,141,934,1027,1129,24,161,177,194,0.22921485084638143,6.654143748710284,7.869428329691268,9.256834835626135,239,275,304,0.98,0.98,0.98,239,275,304,103,118,131,{"$f":"(AK43/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":239},{"$f":"(AL43/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":275},{"$f":"(AM43/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":304},3.017756535900421,3.8388413522783282,4.619011033058954,{"v":2.3000000000000003,"d":"2.30"},{"v":20,"d":"20.0"},22.2,29.3,null,0,385,438,613,null,0,6.324513728106023,7.18539965060231,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2,null,34,null,30]
["14230421",14,230,1,42,20,0,26,30,40.00519982655924,1171,5126,5609,6144,1.362,1.1,1.1,1.1,175,1103,1207,1322,30,190,208,227,0.7474110513904848,9.437157397852099,10.69001126095627,12.058049904943474,210,237,256,0.98,0.98,0.98,210,237,256,90,102,110,{"$f":"(AK44/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":210},{"$f":"(AL44/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":237},{"$f":"(AM44/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":256},3.376819167062962,4.010599274200589,4.449235717012153,{"v":3.066666666666667,"d":"3.07"},{"v":20,"d":"20.0"},22.2,29.3,null,0,385,438,613,null,0,6.324513728106023,7.18539965060231,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2,null,42,null,38]
["14250261",14,250,1,26,10,0,26,30,40.516725051033056,788,3738,4095,4634,1.362,1.1,1.1,1.1,118,804,881,997,20,138,152,171,0.5773809135233472,10.247674318365489,11.835157042556968,14.106784434765684,243,265,{"v":284.90000000000003,"d":"285"},0.98,0.98,0.98,243,265,285,104,114,123,{"$f":"(AK45/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":243},{"$f":"(AL45/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":265},{"$f":"(AM45/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":285},6.722992655758085,7.7085405326854906,8.632724225288523,{"v":1.6666666666666667,"d":"1.67"},22.2,24.6,{"v":33,"d":"33.0"},null,0,426,485,689,null,0,6.222353975468644,7.068105048220597,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14250341",14,250,1,34,15,0,26,30,40.516725051033056,1039,4789,5287,5880,1.362,1.1,1.1,1.1,155,1031,1138,1265,27,177,196,218,0.3082081832264361,8.586697582157463,10.28530609997675,12.416727170435347,257,298,334,0.98,0.98,0.98,257,298,334,111,128,144,{"$f":"(AK46/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":257},{"$f":"(AL46/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":298},{"$f":"(AM46/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":334},3.7595448053823985,4.838013745647644,5.959442471291788,{"v":2.5,"d":"2.50"},22.2,24.6,{"v":33,"d":"33.0"},null,0,426,485,689,null,0,6.222353975468644,7.068105048220597,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14250421",14,250,1,42,20,0,26,30,40.516725051033056,1287,5662,6217,6883,1.362,1.1,1.1,1.1,192,1218,1338,1481,33,209,230,255,0.9304916266992453,11.746016322380719,13.401319066679408,15.44811806721727,231,263,288,0.98,0.98,0.98,231,263,288,99,113,124,{"$f":"(AK47/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":231},{"$f":"(AL47/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":263},{"$f":"(AM47/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":288},4.2035243629565215,5.041362301501329,5.727949776824413,{"v":3.3333333333333335,"d":"3.33"},22.2,24.6,{"v":33,"d":"33.0"},null,0,426,485,689,null,0,6.222353975468644,7.068105048220597,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14270261",14,270,1,26,10,0,26,30,40.974299956639804,860,4089,4491,5134,1.362,1.1,1.1,1.1,128,880,966,1105,22,151,166,190,0.7217032283588841,12.706951843561585,14.633316120705594,17.89615466336172,262,287,{"v":310.8,"d":"311"},0.98,0.98,0.98,262,287,311,113,123,134,{"$f":"(AK48/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":262},{"$f":"(AL48/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":287},{"$f":"(AM48/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":311},8.249820885521348,9.360791581637296,10.63509481474571,{"v":1.8,"d":"1.80"},24.4,{"v":27,"d":"27.0"},36.7,null,0,467,531,766,null,0,6.132190146726926,6.965185380004039,10,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2,null,70,null,70,null,70]
["14270341",14,270,1,34,15,0,26,30,40.974299956639804,1133,5230,5794,6511,1.362,1.1,1.1,1.1,169,1126,1247,1401,29,194,214,241,0.3791124058747006,10.943650304091044,13.019260285539815,16.06681110371226,275,321,365,0.98,0.98,0.98,275,321,365,118,138,157,{"$f":"(AK49/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":275},{"$f":"(AL49/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":321},{"$f":"(AM49/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":365},4.539738260505129,5.9891086899505135,7.524978414023191,{"v":2.7,"d":"2.70"},24.4,{"v":27,"d":"27.0"},36.7,null,0,467,531,766,null,0,6.132190146726926,6.965185380004039,10,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2,null,80,null,80,null,80]
["14270421",14,270,1,42,20,0,26,30,40.974299956639804,1404,6188,6816,7622,1.362,1.1,1.1,1.1,210,1332,1467,1640,36,229,252,282,1.137088557799719,14.437600721292856,16.471066452181475,19.230974366685224,253,288,321,0.98,0.98,0.98,253,288,321,109,124,138,{"$f":"(AK50/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":253},{"$f":"(AL50/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":288},{"$f":"(AM50/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":321},5.201776705273755,6.209981185103384,7.193511728744068,{"v":3.6,"d":"3.60"},24.4,{"v":27,"d":"27.0"},36.7,null,0,467,531,766,null,0,6.132190146726926,6.965185380004039,10,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2,null,90,null,90,null,90]
["14290261",14,290,1,26,10,0,26,30,38.12842680822206,931,4434,4881,5556,1.362,1.1,1.1,1.1,139,954,1050,1196,24,164,181,206,0.8855882514752468,15.48803184258451,17.940392044756468,21.7560522983848,280,308,{"v":341.08750000000003,"d":"341"},0.98,0.98,0.98,280,308,341,120,132,147,{"$f":"(AK51/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":280},{"$f":"(AL51/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":308},{"$f":"(AM51/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":341},9.72448095537559,11.208108539319399,13.157603018115477,{"v":1.9333333333333333,"d":"1.93"},26.5,29.4,36.8,null,0,506,576,757,null,0,6.0515594714640155,6.87363114546986,9,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2,null,100,null,100,null,100]
["14290341",14,290,1,34,15,0,26,30,38.12842680822206,1227,5665,6295,7138,1.362,1.1,1.1,1.1,183,1219,1355,1536,31,210,233,264,0.4596260269960454,13.56176252546608,16.30047092944978,20.33361557989624,292,343,403,0.98,0.98,0.98,292,343,403,126,147,173,{"$f":"(AK52/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":292},{"$f":"(AL52/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":343},{"$f":"(AM52/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":403},5.492030247267677,7.214284956260687,9.623957351948448,{"v":2.9,"d":"2.90"},26.5,29.4,36.8,null,0,506,576,757,null,0,6.0515594714640155,6.87363114546986,9,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2,null,110,null,110,null,110]
["14290421",14,290,1,42,20,0,26,30,38.12842680822206,1520,6706,7407,8350,1.362,1.1,1.1,1.1,227,1443,1594,1797,39,248,274,309,1.3679461297523074,17.357340058999846,19.91082828284496,23.495648219704844,273,313,359,0.98,0.98,0.98,273,313,359,117,135,154,{"$f":"(AK53/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":273},{"$f":"(AL53/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":313},{"$f":"(AM53/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":359},6.178577206518133,7.520960737415887,9.012941212598458,{"v":3.8666666666666667,"d":"3.87"},26.5,29.4,36.8,null,0,506,576,757,null,0,6.0515594714640155,6.87363114546986,9,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2,null,120,null,120,null,120]
["14310261",14,310,1,26,10,0,26,30,35.03251241711607,1006,4779,5272,5800,1.362,1.1,1.1,1.1,150,1028,1135,1248,26,177,195,215,1.0698295908785274,18.603564169501706,21.49190562126489,24.858284842947842,299,329,{"v":358.4,"d":"358"},0.98,0.98,0.98,299,329,358,129,141,154,{"$f":"(AK54/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":299},{"$f":"(AL54/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":329},{"$f":"(AM54/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":358},11.612221876387986,13.257473734020033,15.11899262569165,{"v":2.066666666666667,"d":"2.07"},28.7,31.8,36.4,null,0,546,621,733,null,0,5.978678811957965,6.791272142530232,8,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2,null,130,null,130,null,130]
["14310341",14,310,1,34,15,0,26,30,{"v":35.03251241711607,"d":"35.0"},1325,6097,6793,7495,1.362,1.1,1.1,1.1,198,1312,1462,1613,34,226,251,277,0.5801054496745601,16.548294775837526,19.924532001426694,23.7215660665786,309,365,417,0.98,0.98,0.98,309,365,417,133,157,179,{"$f":"(AK55/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":309},{"$f":"(AL55/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":365},{"$f":"(AM55/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":417},6.476336927145092,8.685695248360709,10.954141077262884,{"v":3.1,"d":"3.10"},28.7,31.8,36.4,null,0,546,621,733,null,0,5.978678811957965,6.791272142530232,8,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2,null,150,null,150,null,150]
["14310421",14,310,1,42,20,0,26,30,{"v":35.03251241711607,"d":"35.0"},1642,7222,7997,8779,1.362,1.1,1.1,1.1,245,1554,1721,1889,42,267,296,325,1.6237714325261459,20.591518791810564,23.731587723879333,26.99094937502187,294,338,380,0.98,0.98,0.98,294,338,380,126,145,163,{"$f":"(AK56/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":294},{"$f":"(AL56/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":338},{"$f":"(AM56/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":380},7.333456821027489,8.894185115673213,10.445783553000176,{"v":4.133333333333334,"d":"4.13"},28.7,31.8,36.4,null,0,546,621,733,null,0,5.978678811957965,6.791272142530232,8,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2,null,170,null,170,null,170]
[{"$f":"CONCATENATE(B57,C57,E57,D57)","v":"970142"},9,70,2,14,{"$f":"IF($E57=14,4,IF($E57=18,9,IF($E57=26,9,IF($E57=34,14,IF($E57=42,19,)))))","v":4},0,0,0,{"v":0,"d":"0.0"},76,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K57*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O57),0)","v":11},{"$f":"ROUND(L57*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P57),0)","v":0},{"$f":"ROUND(M57*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q57),0)","v":0},{"$f":"ROUND(N57*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R57),0)","v":0},{"$f":"ROUND(S57*3600/(4186*ABS($M$1-$M$2)),0)","v":2},{"$f":"ROUND(T57*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U57*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V57*3600/(4186*ABS($M$1-$M$2)),0)","v":0},2.4998470803170997E-3,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE57*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH57),0)","v":0},{"$f":"ROUND(AF57*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI57),0)","v":0},{"$f":"ROUND(AG57*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ57),0)","v":0},{"$f":"ROUND(AK57*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL57*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM57*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK57/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL57/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM57/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.11666666666666667,"d":"0.12"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1,null,190,null,190,null,190]
["970182",9,70,2,18,{"$f":"IF($E58=14,4,IF($E58=18,9,IF($E58=26,9,IF($E58=34,14,IF($E58=42,19,)))))","v":9},0,0,0,{"v":0,"d":"0.0"},90,0,0,0,1.362,1.1,1.1,1.1,13,0,0,0,2,0,0,0,{"$f":"0.0098*(($BM58*(W58^$BO58)*($C58-14.4)*$BP58)+($BN58*W58*W58))","v":3.1012048654778792E-3},0,{"$f":"0.0098*(($BM58*(Y58^$BO58)*($C58-14.4)*$BP58)+($BN58*Y58*Y58))","v":0},{"$f":"0.0098*(($BM58*(Z58^$BO58)*($C58-14.4)*$BP58)+($BN58*Z58*Z58))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK58/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL58/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM58/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.23333333333333334,"d":"0.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2,null,210,null,210,null,210]
["970262",9,70,2,26,9,0,0,0,{"v":0,"d":"0.0"},119,0,0,0,1.362,1.1,1.1,1.1,18,0,0,0,3,0,0,0,6.4730267114827406E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK59/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL59/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM59/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.23333333333333334,"d":"0.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2,null,230,null,230,null,230]
["970342",9,70,2,34,14,0,0,0,{"v":0,"d":"0.0"},154,0,0,0,1.362,1.1,1.1,1.1,23,0,0,0,4,0,0,0,0.033277998999107175,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK60/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL60/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM60/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.35000000000000003,"d":"0.35"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3,null,250,null,250,null,250]
["970422",9,70,2,42,19,0,0,0,{"v":0,"d":"0.0"},222,0,0,0,1.362,1.1,1.1,1.1,33,0,0,0,6,0,0,0,0.10928752307846887,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK61/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL61/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM61/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4666666666666667,"d":"0.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1,null,270,null,270,null,270]
["980142",9,80,2,14,4,0,0,0,{"v":0,"d":"0.0"},95,0,0,0,1.362,1.1,1.1,1.1,14,0,0,0,2,0,0,0,2.9471127422446355E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK62/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL62/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM62/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.13333333333333333,"d":"0.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1,null,290,null,290,null,290]
["980182",9,80,2,18,9,0,0,0,{"v":0,"d":"0.0"},113,0,0,0,1.362,1.1,1.1,1.1,17,0,0,0,3,0,0,0,7.630927336835948E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK63/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL63/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM63/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.26666666666666666,"d":"0.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2,null,310,null,310,null,310]
["980262",9,80,2,26,9,0,0,0,{"v":0,"d":"0.0"},148,0,0,0,1.362,1.1,1.1,1.1,22,0,0,0,4,0,0,0,0.012862019153558217,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK64/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL64/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM64/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.26666666666666666,"d":"0.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2,null,330,null,330]
["980342",9,80,2,34,14,0,0,0,{"v":0,"d":"0.0"},193,0,0,0,1.362,1.1,1.1,1.1,29,0,0,0,5,0,0,0,0.05479458090694347,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK65/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL65/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM65/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3,null,370,null,370]
["980422",9,80,2,42,19,0,0,0,{"v":0,"d":"0.0"},278,0,0,0,1.362,1.1,1.1,1.1,41,0,0,0,7,0,0,0,0.16459449411510485,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK66/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL66/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM66/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5333333333333333,"d":"0.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1,null,410,null,410]
["990142",9,90,2,14,4,0,0,0,{"v":0,"d":"0.0"},114,0,0,0,1.362,1.1,1.1,1.1,17,0,0,0,3,0,0,0,0.006829581822298132,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK67/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL67/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM67/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.15000000000000002,"d":"0.15"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1,null,450,null,450]
["990182",9,90,2,18,9,0,0,0,{"v":0,"d":"0.0"},135,0,0,0,1.362,1.1,1.1,1.1,20,0,0,0,3,0,0,0,0.008788827962189157,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK68/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL68/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM68/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.30000000000000004,"d":"0.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2,null,490,null,490]
["990262",9,90,2,26,9,0,0,0,{"v":0,"d":"0.0"},178,0,0,0,1.362,1.1,1.1,1.1,27,0,0,0,5,0,0,0,0.02220790314848095,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK69/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL69/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM69/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.30000000000000004,"d":"0.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2,null,"Type,ww","Liter/cm","k1","k2","x","t"]
["990342",9,90,2,34,14,0,0,0,{"v":0,"d":"0.0"},231,0,0,0,1.362,1.1,1.1,1.1,34,0,0,0,6,0,0,0,0.08291273655798917,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK70/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL70/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM70/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3,null,4,{"$f":"BS71/2","v":{"v":1.6666666666666668E-3,"d":"0.0017"}},{"v":1.3823338826853E-3,"d":"1.38E-03"},{"v":0.00033290816326531,"d":"3.33E-04"},1.723172227894,1]
["990422",9,90,2,42,19,0,0,0,{"v":0,"d":"0.0"},333,0,0,0,1.362,1.1,1.1,1.1,50,0,0,0,9,0,0,0,0.2825921202379186,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK71/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL71/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM71/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6000000000000001,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1,null,5,{"$f":"BS72","v":{"v":3.3333333333333335E-3,"d":"0.0033"}},{"v":0.00080534470601597,"d":"8.05E-04"},{"v":0.00039795050474944,"d":"3.98E-04"},1.813864715518,2]
["9100142",9,100,2,14,4,0,0,0,{"v":0,"d":"0.0"},133,0,0,0,1.362,1.1,1.1,1.1,20,0,0,0,3,0,0,0,0.007729081732655027,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK72/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL72/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM72/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.16666666666666669,"d":"0.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1,null,9,{"$f":"BS73/2","v":{"v":3.3333333333333335E-3,"d":"0.0033"}},{"v":0.00080534470601597,"d":"8.05E-04"},{"v":0.00039795050474944,"d":"3.98E-04"},1.813864715518,2]
["9100182",9,100,2,18,9,0,0,0,{"v":0,"d":"0.0"},158,0,0,0,1.362,1.1,1.1,1.1,24,0,0,0,4,0,0,0,0.016764342481123313,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK73/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL73/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM73/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F73=$BR$70,$C73*$BS$70,IF($F73=$BR$71,$C73*$BS$71,IF($F73=$BR$72,$C73*$BS$72,IF($F73=$BR$73,$C73*$BS$73,IF($F73=$BR$74,$C73*$BS$74,IF($F73=$BR$75,$C73*$BS$75,IF($F73=$BR$76,$C73*$BS$76,IF($F73=$BR$77,$C73*$BS$77,IF($F73=$BR$78,$C73*$BS$78,IF($F73=$BR$79,$C73*$BS$79,IF($F73=$BR$80,$C73*$BS$80,)))))))))))","v":{"v":0.33333333333333337,"d":"0.33"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2,null,10,{"$f":"0.4/60","v":{"v":0.006666666666666667,"d":"0.0067"}},{"v":0.0014501879713726,"d":"1.45E-03"},{"v":0.00037831632653061,"d":"3.78E-04"},1.4868910444209,2]
["9100262",9,100,2,26,9,0,0,0,{"v":0,"d":"0.0"},207,0,0,0,1.362,1.1,1.1,1.1,31,0,0,0,5,0,0,0,0.0251325599308642,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK74/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL74/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM74/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM74*(AN74^$BO74)*($C74-14.4)*$BP74)+($BN74*AN74*AN74))","v":0},0,0,{"v":0.33333333333333337,"d":"0.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F74=$BR$70,$BT$70,IF($F74=$BR$71,$BT$71,IF($F74=$BR$72,$BT$72,IF($F74=$BR$73,$BT$73,IF($F74=$BR$74,$BT$74,IF($F74=$BR$75,$BT$75,IF($F74=$BR$76,$BT$76,IF($F74=$BR$77,$BT$77,IF($F74=$BR$78,$BT$78,IF($F74=$BR$79,$BT$79,IF($F74=$BR$80,$BT$80,)))))))))))","v":0.00080534470601597},{"$f":"IF($F74=$BR$70,$BU$70,IF($F74=$BR$71,$BU$71,IF($F74=$BR$72,$BU$72,IF($F74=$BR$73,$BU$73,IF($F74=$BR$74,$BU$74,IF($F74=$BR$75,$BU$75,IF($F74=$BR$76,$BU$76,IF($F74=$BR$77,$BU$77,IF($F74=$BR$78,$BU$78,IF($F74=$BR$79,$BU$79,IF($F74=$BR$80,$BU$80,)))))))))))","v":0.00039795050474944},{"$f":"IF($F74=$BR$70,$BV$70,IF($F74=$BR$71,$BV$71,IF($F74=$BR$72,$BV$72,IF($F74=$BR$73,$BV$73,IF($F74=$BR$74,$BV$74,IF($F74=$BR$75,$BV$75,IF($F74=$BR$76,$BV$76,IF($F74=$BR$77,$BV$77,IF($F74=$BR$78,$BV$78,IF($F74=$BR$79,$BV$79,IF($F74=$BR$80,$BV$80,)))))))))))","v":1.813864715518},{"$f":"IF($F74=$BR$70,$BW$70,IF($F74=$BR$71,$BW$71,IF($F74=$BR$72,$BW$72,IF($F74=$BR$73,$BW$73,IF($F74=$BR$74,$BW$74,IF($F74=$BR$75,$BW$75,IF($F74=$BR$76,$BW$76,IF($F74=$BR$77,$BW$77,IF($F74=$BR$78,$BW$78,IF($F74=$BR$79,$BW$79,IF($F74=$BR$80,$BW$80,)))))))))))","v":2},null,11,{"$f":"BS73*2","v":{"v":0.013333333333333334,"d":"0.0133"}},{"v":0.0045081108686135,"d":"4.51E-03"},{"v":0.00061577708006279,"d":"6.16E-04"},1.2776043744342,4]
["9100342",9,100,2,34,14,0,0,0,{"v":0,"d":"0.0"},269,0,0,0,1.362,1.1,1.1,1.1,40,0,0,0,7,0,0,0,0.1181852251031021,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK75/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL75/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM75/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3,null,14,{"$f":"BS76/2","v":{"v":0.005,"d":"0.0050"}},{"v":0.00255823982887,"d":"2.56E-03"},{"v":0.00056161694684148,"d":"5.62E-04"},1.4942747715062,3]
["9100422",9,100,2,42,19,0,0,0,{"v":0,"d":"0.0"},388,0,0,0,1.362,1.1,1.1,1.1,58,0,0,0,10,0,0,0,0.37806768715965605,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK76/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL76/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM76/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6666666666666667,"d":"0.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1,null,15,{"$f":"BS73*1.5","v":{"v":0.01,"d":"0.0100"}},{"v":0.00019563320356262,"d":"1.96E-04"},{"v":4.4708458846471E-4,"d":"4.47E-04"},1.766459432507,2]
["9110142",9,110,2,14,4,0,0,0,{"v":0,"d":"0.0"},152,0,0,0,1.362,1.1,1.1,1.1,23,0,0,0,4,0,0,0,0.014169445844370371,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK77/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL77/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM77/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.18333333333333335,"d":"0.18"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1,null,16,{"$f":"BS73*3","v":{"v":0.02,"d":"0.0200"}},{"v":2.3534468911758E-5,"d":"2.35E-05"},{"v":0.0012798185941044,"d":"1.28E-03"},2.1754508297045,4]
["9110182",9,110,2,18,9,0,0,0,{"v":0,"d":"0.0"},180,0,0,0,1.362,1.1,1.1,1.1,27,0,0,0,5,0,0,0,0.028057216713247447,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK78/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL78/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM78/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3666666666666667,"d":"0.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2,null,19,{"$f":"BS79/2","v":{"v":0.006666666666666667,"d":"0.0067"}},{"v":0.011616292894075,"d":"1.16E-02"},{"v":0.0016553227470232,"d":"1.66E-03"},1.5869346821791,1]
["9110262",9,110,2,26,9,0,0,0,{"v":0,"d":"0.0"},237,0,0,0,1.362,1.1,1.1,1.1,35,0,0,0,6,0,0,0,0.03905896637940668,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK79/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL79/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM79/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3666666666666667,"d":"0.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2,null,20,{"$f":"BS73*2","v":{"v":0.013333333333333334,"d":"0.0133"}},{"v":1.6730950035507E-3,"d":"1.67E-03"},{"v":0.00032929523945446,"d":"3.29E-04"},1.3691788367472,2]
["9110342",9,110,2,34,14,0,0,0,{"v":0,"d":"0.0"},307,0,0,0,1.362,1.1,1.1,1.1,46,0,0,0,8,0,0,0,0.16112448616671515,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK80/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL80/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM80/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.55,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3,null,21,{"$f":"BS73*4","v":{"v":0.02666666666666667,"d":"0.0267"}},{"v":1.2120276898534E-4,"d":"1.21E-04"},{"v":0.00051547245615298,"d":"5.15E-04"},1.8622089337321,4]
["9110422",9,110,2,42,19,0,0,0,{"v":0,"d":"0.0"},445,0,0,0,1.362,1.1,1.1,1.1,66,0,0,0,11,0,0,0,0.4910358862505484,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK81/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL81/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM81/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7333333333333334,"d":"0.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9120142",9,120,2,14,4,0,0,0,{"v":0,"d":"0.0"},172,0,0,0,1.362,1.1,1.1,1.1,26,0,0,0,4,0,0,0,0.01564614520047606,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK82/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL82/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM82/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.2,"d":"0.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9120182",9,120,2,18,9,0,0,0,{"v":0,"d":"0.0"},203,0,0,0,1.362,1.1,1.1,1.1,30,0,0,0,5,0,0,0,0.030981873495630696,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK83/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL83/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM83/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9120262",9,120,2,26,9,0,0,0,{"v":0,"d":"0.0"},267,0,0,0,1.362,1.1,1.1,1.1,40,0,0,0,7,0,0,0,0.05704958475569953,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK84/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL84/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM84/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9120342",9,120,2,34,14,0,0,0,{"v":0,"d":"0.0"},346,0,0,0,1.362,1.1,1.1,1.1,52,0,0,0,9,0,0,0,0.21221024098891197,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK85/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL85/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM85/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9120422",9,120,2,42,19,0,0,0,{"v":0,"d":"0.0"},500,0,0,0,1.362,1.1,1.1,1.1,75,0,0,0,13,0,0,0,0.7069688951569888,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK86/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL86/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM86/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9130142",9,130,2,14,4,0,0,0,{"v":0,"d":"0.0"},190,0,0,0,1.362,1.1,1.1,1.1,28,0,0,0,5,0,0,0,0.02515665608799953,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK87/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL87/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM87/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.21666666666666667,"d":"0.22"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9130182",9,130,2,18,9,0,0,0,{"v":0,"d":"0.0"},225,0,0,0,1.362,1.1,1.1,1.1,34,0,0,0,6,0,0,0,0.04720092651357636,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK88/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL88/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM88/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.43333333333333335,"d":"0.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9130262",9,130,2,26,9,0,0,0,{"v":0,"d":"0.0"},296,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K89*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O89),0)","v":44},0,0,0,{"$f":"ROUND(S89*3600/(4186*ABS($M$1-$M$2)),0)","v":8},0,0,0,0.0795506150193772,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK89/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL89/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM89/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.43333333333333335,"d":"0.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9130342",9,130,2,34,14,0,0,0,{"v":0,"d":"0.0"},385,0,0,0,1.362,1.1,1.1,1.1,57,0,0,0,10,0,0,0,0.27189499021265695,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK90/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL90/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM90/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.65,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9130422",9,130,2,42,19,0,0,0,{"v":0,"d":"0.0"},555,0,0,0,1.362,1.1,1.1,1.1,83,0,0,0,14,0,0,0,0.8703047159072181,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK91/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL91/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM91/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8666666666666667,"d":"0.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9150142",9,150,2,14,4,0,0,0,{"v":0,"d":"0.0"},229,0,0,0,1.362,1.1,1.1,1.1,34,0,0,0,6,0,0,0,0.040387979706302785,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK92/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL92/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM92/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9150182",9,150,2,18,9,0,0,0,{"v":0,"d":"0.0"},271,0,0,0,1.362,1.1,1.1,1.1,40,0,0,0,7,0,0,0,0.07320256456346057,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK93/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL93/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM93/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9150262",9,150,2,26,9,0,0,0,{"v":0,"d":"0.0"},356,0,0,0,1.362,1.1,1.1,1.1,53,0,0,0,9,0,0,0,0.11549252835977776,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK94/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL94/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM94/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9150342",9,150,2,34,14,0,0,0,{"v":0,"d":"0.0"},462,0,0,0,1.362,1.1,1.1,1.1,69,0,0,0,12,0,0,0,0.41875916107887057,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK95/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL95/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM95/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9150422",9,150,2,42,19,0,0,0,{"v":0,"d":"0.0"},666,0,0,0,1.362,1.1,1.1,1.1,99,0,0,0,17,0,0,0,1.3888771840766918,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK96/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL96/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM96/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9170142",9,170,2,14,4,0,0,0,{"v":0,"d":"0.0"},267,0,0,0,1.362,1.1,1.1,1.1,40,0,0,0,7,0,0,0,0.06042943264252265,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK97/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL97/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM97/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.2833333333333333,"d":"0.28"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9170182",9,170,2,18,9,0,0,0,{"v":0,"d":"0.0"},316,0,0,0,1.362,1.1,1.1,1.1,47,0,0,0,8,0,0,0,0.1069904144874735,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK98/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL98/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM98/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5666666666666667,"d":"0.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9170262",9,170,2,26,9,0,0,0,{"v":0,"d":"0.0"},415,0,0,0,1.362,1.1,1.1,1.1,62,0,0,0,11,0,0,0,0.19066418462238746,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK99/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL99/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM99/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5666666666666667,"d":"0.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9170342",9,170,2,34,14,0,0,0,{"v":0,"d":"0.0"},538,0,0,0,1.362,1.1,1.1,1.1,80,0,0,0,14,0,0,0,0.6049278044286743,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK100/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL100/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM100/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.85,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9170422",9,170,2,42,19,0,0,0,{"v":0,"d":"0.0"},778,0,0,0,1.362,1.1,1.1,1.1,116,0,0,0,20,0,0,0,2.062156247240507,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK101/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL101/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM101/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1333333333333333,"d":"1.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9190142",9,190,2,14,4,0,0,0,{"v":0,"d":"0.0"},304,0,0,0,1.362,1.1,1.1,1.1,45,0,0,0,8,0,0,0,0.08582247217399967,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK102/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL102/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM102/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3166666666666667,"d":"0.32"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9190182",9,190,2,18,9,0,0,0,{"v":0,"d":"0.0"},360,0,0,0,1.362,1.1,1.1,1.1,54,0,0,0,9,0,0,0,0.14946793698783312,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK103/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL103/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM103/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6333333333333334,"d":"0.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9190262",9,190,2,26,9,0,0,0,{"v":0,"d":"0.0"},474,0,0,0,1.362,1.1,1.1,1.1,71,0,0,0,12,0,0,0,0.2518955482976295,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK104/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL104/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM104/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6333333333333334,"d":"0.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9190342",9,190,2,34,14,0,0,0,{"v":0,"d":"0.0"},615,0,0,0,1.362,1.1,1.1,1.1,92,0,0,0,16,0,0,0,0.8333627851761785,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK105/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL105/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM105/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9500000000000001,"d":"0.95"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9190422",9,190,2,42,19,0,0,0,{"v":0,"d":"0.0"},888,0,0,0,1.362,1.1,1.1,1.1,133,0,0,0,23,0,0,0,2.9045329409913916,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK106/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL106/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM106/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2666666666666668,"d":"1.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9210142",9,210,2,14,4,0,0,0,{"v":0,"d":"0.0"},342,0,0,0,1.362,1.1,1.1,1.1,51,0,0,0,9,0,0,0,0.11708826199462927,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK107/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL107/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM107/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.35000000000000003,"d":"0.35"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9210182",9,210,2,18,9,0,0,0,{"v":0,"d":"0.0"},406,0,0,0,1.362,1.1,1.1,1.1,61,0,0,0,10,0,0,0,0.20151748691134386,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK108/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL108/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM108/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9210262",9,210,2,26,9,0,0,0,{"v":0,"d":"0.0"},534,0,0,0,1.362,1.1,1.1,1.1,80,0,0,0,14,0,0,0,0.3710424038503834,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK109/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL109/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM109/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9210342",9,210,2,34,14,0,0,0,{"v":0,"d":"0.0"},692,0,0,0,1.362,1.1,1.1,1.1,103,0,0,0,18,0,0,0,1.1068269964550952,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK110/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL110/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM110/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.05,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9210422",9,210,2,42,19,0,0,0,{"v":0,"d":"0.0"},1000,0,0,0,1.362,1.1,1.1,1.1,149,0,0,0,26,0,0,0,3.929582658734965,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK111/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL111/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM111/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4000000000000001,"d":"1.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9230142",9,230,2,14,4,0,0,0,{"v":0,"d":"0.0"},381,0,0,0,1.362,1.1,1.1,1.1,57,0,0,0,10,0,0,0,0.15473077132339433,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK112/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL112/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM112/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.38333333333333336,"d":"0.38"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9230182",9,230,2,18,9,0,0,0,{"v":0,"d":"0.0"},451,0,0,0,1.362,1.1,1.1,1.1,67,0,0,0,12,0,0,0,0.3091470199480457,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK113/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL113/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM113/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7666666666666667,"d":"0.77"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9230262",9,230,2,26,9,0,0,0,{"v":0,"d":"0.0"},593,0,0,0,1.362,1.1,1.1,1.1,89,0,0,0,15,0,0,0,0.46342576374914596,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK114/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL114/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM114/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7666666666666667,"d":"0.77"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9230342",9,230,2,34,14,0,0,0,{"v":0,"d":"0.0"},769,0,0,0,1.362,1.1,1.1,1.1,115,0,0,0,20,0,0,0,1.4279195707385046,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK115/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL115/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM115/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1500000000000001,"d":"1.15"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9230422",9,230,2,42,19,0,0,0,{"v":0,"d":"0.0"},1111,0,0,0,1.362,1.1,1.1,1.1,166,0,0,0,29,0,0,0,5.150204288927729,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK116/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL116/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM116/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5333333333333334,"d":"1.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9250142",9,250,2,14,4,0,0,0,{"v":0,"d":"0.0"},419,0,0,0,1.362,1.1,1.1,1.1,63,0,0,0,11,0,0,0,0.1992391184829101,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK117/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL117/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM117/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4166666666666667,"d":"0.42"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9250182",9,250,2,18,9,0,0,0,{"v":0,"d":"0.0"},496,0,0,0,1.362,1.1,1.1,1.1,74,0,0,0,13,0,0,0,0.390561305195186,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK118/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL118/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM118/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8333333333333334,"d":"0.83"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9250262",9,250,2,26,9,0,0,0,{"v":0,"d":"0.0"},652,0,0,0,1.362,1.1,1.1,1.1,97,0,0,0,17,0,0,0,0.6354071204801046,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK119/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL119/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM119/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8333333333333334,"d":"0.83"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9250342",9,250,2,34,14,0,0,0,{"v":0,"d":"0.0"},846,0,0,0,1.362,1.1,1.1,1.1,126,0,0,0,22,0,0,0,1.7991017961144635,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK120/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL120/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM120/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9250422",9,250,2,42,19,0,0,0,{"v":0,"d":"0.0"},1221,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K121*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O121),0)","v":182},0,0,0,{"$f":"ROUND(S121*3600/(4186*ABS($M$1-$M$2)),0)","v":31},0,0,0,6.255272280879525,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK121/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL121/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM121/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6666666666666667,"d":"1.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9270142",9,270,2,14,{"$f":"IF($E122=14,4,IF($E122=18,9,IF($E122=26,9,IF($E122=34,14,IF($E122=42,19,)))))","v":4},0,0,0,{"v":0,"d":"0.0"},457,0,0,0,1.362,1.1,1.1,1.1,68,0,0,0,12,0,0,0,{"$f":"0.0098*(($BM122*(W122^$BO122)*($C122-14.4)*$BP122)+($BN122*W122*W122))","v":0.25108939883030007},0,{"$f":"0.0098*(($BM122*(Y122^$BO122)*($C122-14.4)*$BP122)+($BN122*Y122*Y122))","v":0},{"$f":"0.0098*(($BM122*(Z122^$BO122)*($C122-14.4)*$BP122)+($BN122*Z122*Z122))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK122/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL122/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM122/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9270182",9,270,2,18,9,0,0,0,{"v":0,"d":"0.0"},541,0,0,0,1.362,1.1,1.1,1.1,81,0,0,0,14,0,0,0,0.48462461873408297,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK123/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL123/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM123/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9270262",9,270,2,26,9,0,0,0,{"v":0,"d":"0.0"},711,0,0,0,1.362,1.1,1.1,1.1,106,0,0,0,18,0,0,0,0.7645600081027294,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK124/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL124/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM124/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9270342",9,270,2,34,14,0,0,0,{"v":0,"d":"0.0"},923,0,0,0,1.362,1.1,1.1,1.1,138,0,0,0,24,0,0,0,2.2227168473725714,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK125/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL125/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM125/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.35,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9270422",9,270,2,42,19,0,0,0,{"v":0,"d":"0.0"},1333,0,0,0,1.362,1.1,1.1,1.1,199,0,0,0,34,0,0,0,7.856865228202791,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK126/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL126/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM126/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.8,"d":"1.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9290142",9,290,2,14,4,0,0,0,{"v":0,"d":"0.0"},495,0,0,0,1.362,1.1,1.1,1.1,74,0,0,0,13,0,0,0,0.3107461461676084,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK127/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL127/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM127/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.48333333333333334,"d":"0.48"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9290182",9,290,2,18,9,0,0,0,{"v":0,"d":"0.0"},586,0,0,0,1.362,1.1,1.1,1.1,87,0,0,0,15,0,0,0,0.5921497756840737,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK128/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL128/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM128/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9666666666666667,"d":"0.97"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9290262",9,290,2,26,9,0,0,0,{"v":0,"d":"0.0"},771,0,0,0,1.362,1.1,1.1,1.1,115,0,0,0,20,0,0,0,0.9979043924787302,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK129/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL129/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM129/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9666666666666667,"d":"0.97"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9290342",9,290,2,34,14,0,0,0,{"v":0,"d":"0.0"},1000,0,0,0,1.362,1.1,1.1,1.1,149,0,0,0,26,0,0,0,2.7010052197234917,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK130/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL130/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM130/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9290422",9,290,2,42,19,0,0,0,{"v":0,"d":"0.0"},1444,0,0,0,1.362,1.1,1.1,1.1,216,0,0,0,37,0,0,0,9.687312492125066,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK131/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL131/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM131/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.9333333333333333,"d":"1.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9310142",9,310,2,14,4,0,0,0,{"v":0,"d":"0.0"},533,0,0,0,1.362,1.1,1.1,1.1,80,0,0,0,14,0,0,0,0.3786635249694434,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK132/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL132/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM132/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5166666666666667,"d":"0.52"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9310182",9,310,2,18,9,0,0,0,{"v":0,"d":"0.0"},631,0,0,0,1.362,1.1,1.1,1.1,94,0,0,0,16,0,0,0,0.7139385050261753,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK133/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL133/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM133/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0333333333333334,"d":"1.03"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9310262",9,310,2,26,9,0,0,0,{"v":0,"d":"0.0"},830,0,0,0,1.362,1.1,1.1,1.1,124,0,0,0,21,0,0,0,1.1692530493701028,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK134/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL134/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM134/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0333333333333334,"d":"1.03"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9310342",9,310,2,34,14,0,0,0,{"v":0,"d":"0.0"},1076,0,0,0,1.362,1.1,1.1,1.1,161,0,0,0,28,0,0,0,3.2361170711188967,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK135/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL135/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM135/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.55,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9310422",9,310,2,42,19,0,0,0,{"v":0,"d":"0.0"},1555,0,0,0,1.362,1.1,1.1,1.1,232,0,0,0,40,0,0,0,11.757700670882393,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK136/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL136/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM136/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.066666666666667,"d":"2.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9330142",9,330,2,14,4,0,0,0,{"v":0,"d":"0.0"},571,0,0,0,1.362,1.1,1.1,1.1,85,0,0,0,15,0,0,0,0.45528631952161647,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK137/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL137/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM137/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F137=$BR$70,$C137*$BS$70,IF($F137=$BR$71,$C137*$BS$71,IF($F137=$BR$72,$C137*$BS$72,IF($F137=$BR$73,$C137*$BS$73,IF($F137=$BR$74,$C137*$BS$74,IF($F137=$BR$75,$C137*$BS$75,IF($F137=$BR$76,$C137*$BS$76,IF($F137=$BR$77,$C137*$BS$77,IF($F137=$BR$78,$C137*$BS$78,IF($F137=$BR$79,$C137*$BS$79,IF($F137=$BR$80,$C137*$BS$80,)))))))))))","v":0.55},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9330182",9,330,2,18,9,0,0,0,{"v":0,"d":"0.0"},676,0,0,0,1.362,1.1,1.1,1.1,101,0,0,0,17,0,0,0,0.8507823480049105,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK138/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL138/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM138/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM138*(AN138^$BO138)*($C138-14.4)*$BP138)+($BN138*AN138*AN138))","v":0},0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F138=$BR$70,$BT$70,IF($F138=$BR$71,$BT$71,IF($F138=$BR$72,$BT$72,IF($F138=$BR$73,$BT$73,IF($F138=$BR$74,$BT$74,IF($F138=$BR$75,$BT$75,IF($F138=$BR$76,$BT$76,IF($F138=$BR$77,$BT$77,IF($F138=$BR$78,$BT$78,IF($F138=$BR$79,$BT$79,IF($F138=$BR$80,$BT$80,)))))))))))","v":0.00080534470601597},{"$f":"IF($F138=$BR$70,$BU$70,IF($F138=$BR$71,$BU$71,IF($F138=$BR$72,$BU$72,IF($F138=$BR$73,$BU$73,IF($F138=$BR$74,$BU$74,IF($F138=$BR$75,$BU$75,IF($F138=$BR$76,$BU$76,IF($F138=$BR$77,$BU$77,IF($F138=$BR$78,$BU$78,IF($F138=$BR$79,$BU$79,IF($F138=$BR$80,$BU$80,)))))))))))","v":0.00039795050474944},{"$f":"IF($F138=$BR$70,$BV$70,IF($F138=$BR$71,$BV$71,IF($F138=$BR$72,$BV$72,IF($F138=$BR$73,$BV$73,IF($F138=$BR$74,$BV$74,IF($F138=$BR$75,$BV$75,IF($F138=$BR$76,$BV$76,IF($F138=$BR$77,$BV$77,IF($F138=$BR$78,$BV$78,IF($F138=$BR$79,$BV$79,IF($F138=$BR$80,$BV$80,)))))))))))","v":1.813864715518},{"$f":"IF($F138=$BR$70,$BW$70,IF($F138=$BR$71,$BW$71,IF($F138=$BR$72,$BW$72,IF($F138=$BR$73,$BW$73,IF($F138=$BR$74,$BW$74,IF($F138=$BR$75,$BW$75,IF($F138=$BR$76,$BW$76,IF($F138=$BR$77,$BW$77,IF($F138=$BR$78,$BW$78,IF($F138=$BR$79,$BW$79,IF($F138=$BR$80,$BW$80,)))))))))))","v":2}]
["9330262",9,330,2,26,9,0,0,0,{"v":0,"d":"0.0"},889,0,0,0,1.362,1.1,1.1,1.1,133,0,0,0,23,0,0,0,1.4722242250147157,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK139/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL139/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM139/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9330342",9,330,2,34,14,0,0,0,{"v":0,"d":"0.0"},1154,0,0,0,1.362,1.1,1.1,1.1,172,0,0,0,30,0,0,0,3.830122276084769,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK140/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL140/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM140/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6500000000000001,"d":"1.65"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9330422",9,330,2,42,19,0,0,0,{"v":0,"d":"0.0"},1666,0,0,0,1.362,1.1,1.1,1.1,249,0,0,0,43,0,0,0,14.07876691332578,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK141/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL141/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM141/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.2,"d":"2.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9350142",9,350,2,14,4,0,0,0,{"v":0,"d":"0.0"},609,0,0,0,1.362,1.1,1.1,1.1,91,0,0,0,16,0,0,0,0.5410507663410987,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK142/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL142/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM142/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5833333333333334,"d":"0.58"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9350182",9,350,2,18,9,0,0,0,{"v":0,"d":"0.0"},722,0,0,0,1.362,1.1,1.1,1.1,108,0,0,0,19,0,0,0,1.1068750871400044,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK143/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL143/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM143/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1666666666666667,"d":"1.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9350262",9,350,2,26,9,0,0,0,{"v":0,"d":"0.0"},948,0,0,0,1.362,1.1,1.1,1.1,141,0,0,0,24,0,0,0,1.6910388953309536,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK144/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL144/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM144/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1666666666666667,"d":"1.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9350342",9,350,2,34,14,0,0,0,{"v":0,"d":"0.0"},1231,0,0,0,1.362,1.1,1.1,1.1,184,0,0,0,32,0,0,0,4.485018744265233,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK145/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL145/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM145/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9350422",9,350,2,42,19,0,0,0,{"v":0,"d":"0.0"},1777,0,0,0,1.362,1.1,1.1,1.1,265,0,0,0,46,0,0,0,16.66093391095744,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK146/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL146/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM146/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.3333333333333335,"d":"2.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9370142",9,370,2,14,4,0,0,0,{"v":0,"d":"0.0"},647,0,0,0,1.362,1.1,1.1,1.1,97,0,0,0,17,0,0,0,0.6363852633181388,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK147/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL147/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM147/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6166666666666667,"d":"0.62"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9370182",9,370,2,18,9,0,0,0,{"v":0,"d":"0.0"},767,0,0,0,1.362,1.1,1.1,1.1,114,0,0,0,20,0,0,0,1.287119030069474,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK148/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL148/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM148/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2333333333333334,"d":"1.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9370262",9,370,2,26,9,0,0,0,{"v":0,"d":"0.0"},1008,0,0,0,1.362,1.1,1.1,1.1,150,0,0,0,26,0,0,0,2.0716809842061146,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK149/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL149/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM149/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2333333333333334,"d":"1.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9370342",9,370,2,34,14,0,0,0,{"v":0,"d":"0.0"},1307,0,0,0,1.362,1.1,1.1,1.1,195,0,0,0,34,0,0,0,5.202739395986066,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK150/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL150/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM150/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.85,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9370422",9,370,2,42,19,0,0,0,{"v":0,"d":"0.0"},1888,0,0,0,1.362,1.1,1.1,1.1,282,0,0,0,49,0,0,0,19.514339305610036,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK151/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL151/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM151/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.466666666666667,"d":"2.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9390142",9,390,2,14,4,0,0,0,{"v":0,"d":"0.0"},685,0,0,0,1.362,1.1,1.1,1.1,102,0,0,0,18,0,0,0,0.7417109802707712,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK152/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL152/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM152/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.65,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9390182",9,390,2,18,9,0,0,0,{"v":0,"d":"0.0"},811,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K153*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O153),0)","v":121},0,0,0,{"$f":"ROUND(S153*3600/(4186*ABS($M$1-$M$2)),0)","v":21},0,0,0,1.48522955461467,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK153/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL153/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM153/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9390262",9,390,2,26,9,0,0,0,{"v":0,"d":"0.0"},1067,0,0,0,1.362,1.1,1.1,1.1,159,0,0,0,27,0,0,0,2.3431007765101963,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK154/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL154/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM154/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9390342",9,390,2,34,14,0,0,0,{"v":0,"d":"0.0"},1385,0,0,0,1.362,1.1,1.1,1.1,207,0,0,0,36,0,0,0,5.9851580799980715,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK155/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL155/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM155/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.95,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9390422",9,390,2,42,19,0,0,0,{"v":0,"d":"0.0"},1999,0,0,0,1.362,1.1,1.1,1.1,298,0,0,0,51,0,0,0,21.96123478546851,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK156/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL156/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM156/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.6,"d":"2.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9410142",9,410,2,14,4,0,0,0,{"v":0,"d":"0.0"},723,0,0,0,1.362,1.1,1.1,1.1,108,0,0,0,19,0,0,0,0.8574423895154929,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK157/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL157/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM157/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6833333333333333,"d":"0.68"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9410182",9,410,2,18,9,0,0,0,{"v":0,"d":"0.0"},856,0,0,0,1.362,1.1,1.1,1.1,128,0,0,0,22,0,0,0,1.7019594878432558,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK158/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL158/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM158/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3666666666666667,"d":"1.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9410262",9,410,2,26,9,0,0,0,{"v":0,"d":"0.0"},1126,0,0,0,1.362,1.1,1.1,1.1,168,0,0,0,29,0,0,0,2.8092709392926634,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK159/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL159/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM159/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3666666666666667,"d":"1.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9410342",9,410,2,34,14,0,0,0,{"v":0,"d":"0.0"},1461,0,0,0,1.362,1.1,1.1,1.1,218,0,0,0,37,0,0,0,6.567010689307354,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK160/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL160/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM160/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.05,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9410422",9,410,2,42,19,0,0,0,{"v":0,"d":"0.0"},2111,0,0,0,1.362,1.1,1.1,1.1,315,0,0,0,54,0,0,0,25.32547515847159,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK161/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL161/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM161/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.7333333333333334,"d":"2.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9430142",9,430,2,14,4,0,0,0,{"v":0,"d":"0.0"},761,0,0,0,1.362,1.1,1.1,1.1,114,0,0,0,20,0,0,0,0.9839877307227323,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK162/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL162/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM162/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7166666666666667,"d":"0.72"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9430182",9,430,2,18,9,0,0,0,{"v":0,"d":"0.0"},902,0,0,0,1.362,1.1,1.1,1.1,135,0,0,0,23,0,0,0,1.938054760505208,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK163/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL163/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM163/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4333333333333333,"d":"1.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9430262",9,430,2,26,9,0,0,0,{"v":0,"d":"0.0"},1186,0,0,0,1.362,1.1,1.1,1.1,177,0,0,0,30,0,0,0,3.13832222889272,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK164/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL164/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM164/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4333333333333333,"d":"1.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9430342",9,430,2,34,14,0,0,0,{"v":0,"d":"0.0"},1538,0,0,0,1.362,1.1,1.1,1.1,230,0,0,0,40,0,0,0,7.751319326142405,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK165/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL165/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM165/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.15,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9430422",9,430,2,42,19,0,0,0,{"v":0,"d":"0.0"},2221,0,0,0,1.362,1.1,1.1,1.1,332,0,0,0,57,0,0,0,28.98799814319772,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK166/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL166/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM166/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8666666666666667,"d":"2.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9450142",9,450,2,14,4,0,0,0,{"v":0,"d":"0.0"},800,0,0,0,1.362,1.1,1.1,1.1,119,0,0,0,20,0,0,0,1.0312775637700244,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK167/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL167/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM167/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9450182",9,450,2,18,9,0,0,0,{"v":0,"d":"0.0"},947,0,0,0,1.362,1.1,1.1,1.1,141,0,0,0,24,0,0,0,2.1942547905400547,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK168/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL168/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM168/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9450262",9,450,2,26,9,0,0,0,{"v":0,"d":"0.0"},1245,0,0,0,1.362,1.1,1.1,1.1,186,0,0,0,32,0,0,0,3.6977153576410617,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK169/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL169/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM169/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9450342",9,450,2,34,14,0,0,0,{"v":0,"d":"0.0"},1615,0,0,0,1.362,1.1,1.1,1.1,241,0,0,0,41,0,0,0,8.429379830603802,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK170/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL170/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM170/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9450422",9,450,2,42,19,0,0,0,{"v":0,"d":"0.0"},2332,0,0,0,1.362,1.1,1.1,1.1,348,0,0,0,60,0,0,0,32.95805828813813,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK171/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL171/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM171/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3,"d":"3.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9470142",9,470,2,14,4,0,0,0,{"v":0,"d":"0.0"},838,0,0,0,1.362,1.1,1.1,1.1,125,0,0,0,22,0,0,0,1.2711244201970322,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK172/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL172/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM172/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7833333333333334,"d":"0.78"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9470182",9,470,2,18,9,0,0,0,{"v":0,"d":"0.0"},992,0,0,0,1.362,1.1,1.1,1.1,148,0,0,0,25,0,0,0,2.471292829051116,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK173/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL173/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM173/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5666666666666669,"d":"1.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9470262",9,470,2,26,9,0,0,0,{"v":0,"d":"0.0"},1304,0,0,0,1.362,1.1,1.1,1.1,195,0,0,0,34,0,0,0,4.31688971084337,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK174/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL174/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM174/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5666666666666669,"d":"1.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9470342",9,470,2,34,14,0,0,0,{"v":0,"d":"0.0"},1692,0,0,0,1.362,1.1,1.1,1.1,253,0,0,0,44,0,0,0,9.797488375812694,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK175/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL175/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM175/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.35,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9470422",9,470,2,42,19,0,0,0,{"v":0,"d":"0.0"},2444,0,0,0,1.362,1.1,1.1,1.1,365,0,0,0,63,{"$f":"ROUND(T176*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U176*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V176*3600/(4186*ABS($M$1-$M$2)),0)","v":0},37.24471814484071,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK176/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL176/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM176/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1333333333333337,"d":"3.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9490142",9,490,2,14,4,0,0,0,{"v":0,"d":"0.0"},875,0,0,0,1.362,1.1,1.1,1.1,131,0,0,0,23,0,0,0,1.4325045548170292,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK177/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL177/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM177/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8166666666666668,"d":"0.82"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9490182",9,490,2,18,9,0,0,0,{"v":0,"d":"0.0"},1037,0,0,0,1.362,1.1,1.1,1.1,155,0,0,0,27,0,0,0,2.966172591876055,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK178/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL178/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM178/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6333333333333335,"d":"1.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9490262",9,490,2,26,9,0,0,0,{"v":0,"d":"0.0"},1363,0,0,0,1.362,1.1,1.1,1.1,203,0,0,0,35,0,0,0,4.749493910273141,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK179/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL179/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM179/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6333333333333335,"d":"1.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9490342",9,490,2,34,14,0,0,0,{"v":0,"d":"0.0"},1769,0,0,0,1.362,1.1,1.1,1.1,264,0,0,0,45,0,0,0,10.576502469455393,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK180/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL180/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM180/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9490422",9,490,2,42,19,0,0,0,{"v":0,"d":"0.0"},2555,0,0,0,1.362,1.1,1.1,1.1,381,0,0,0,66,0,0,0,41.856861234550756,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK181/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL181/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM181/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.266666666666667,"d":"3.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["1170142",11,70,2,14,4,0,0,0,{"v":0,"d":"0.0"},87,0,0,0,1.362,1.1,1.1,1.1,13,0,0,0,2,0,0,0,2.4998470803170997E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK182/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL182/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM182/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.11666666666666667,"d":"0.12"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["1170182",11,70,2,18,9,0,0,0,{"v":0,"d":"0.0"},104,0,0,0,1.362,1.1,1.1,1.1,16,0,0,0,3,0,0,0,6.4730267114827406E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK183/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL183/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM183/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.23333333333333334,"d":"0.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1170262",11,70,2,26,9,0,0,0,{"v":0,"d":"0.0"},140,0,0,0,1.362,1.1,1.1,1.1,21,0,0,0,4,0,0,0,0.010910857489775673,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK184/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL184/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM184/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.23333333333333334,"d":"0.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1170342",11,70,2,34,14,0,0,0,{"v":0,"d":"0.0"},182,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K185*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O185),0)","v":27},0,0,0,{"$f":"ROUND(S185*3600/(4186*ABS($M$1-$M$2)),0)","v":5},0,0,0,0.046462723474783835,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK185/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL185/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM185/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.35000000000000003,"d":"0.35"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["1170422",11,70,2,42,{"$f":"IF($E186=14,4,IF($E186=18,9,IF($E186=26,9,IF($E186=34,14,IF($E186=42,19,)))))","v":19},0,0,0,{"v":0,"d":"0.0"},255,0,0,0,1.362,1.1,1.1,1.1,38,0,0,0,7,0,0,0,{"$f":"0.0098*(($BM186*(W186^$BO186)*($C186-14.4)*$BP186)+($BN186*W186*W186))","v":0.1396250416559609},0,{"$f":"0.0098*(($BM186*(Y186^$BO186)*($C186-14.4)*$BP186)+($BN186*Y186*Y186))","v":0},{"$f":"0.0098*(($BM186*(Z186^$BO186)*($C186-14.4)*$BP186)+($BN186*Z186*Z186))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK186/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL186/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM186/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4666666666666667,"d":"0.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["1180142",11,80,2,14,4,0,0,0,{"v":0,"d":"0.0"},109,0,0,0,1.362,1.1,1.1,1.1,16,0,0,0,3,0,0,0,0.005930081911941236,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK187/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL187/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM187/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.13333333333333333,"d":"0.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["1180182",11,80,2,18,9,0,0,0,{"v":0,"d":"0.0"},129,0,0,0,1.362,1.1,1.1,1.1,19,0,0,0,3,0,0,0,7.630927336835948E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK188/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL188/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM188/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.26666666666666666,"d":"0.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1180262",11,80,2,26,9,0,0,0,{"v":0,"d":"0.0"},175,0,0,0,1.362,1.1,1.1,1.1,26,0,0,0,4,0,0,0,0.012862019153558217,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK189/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL189/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM189/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.26666666666666666,"d":"0.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1180342",11,80,2,34,14,0,0,0,{"v":0,"d":"0.0"},227,0,0,0,1.362,1.1,1.1,1.1,34,0,0,0,6,0,0,0,0.07197165215334056,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK190/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL190/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM190/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["1180422",11,80,2,42,19,0,0,0,{"v":0,"d":"0.0"},319,0,0,0,1.362,1.1,1.1,1.1,48,0,0,0,8,0,0,0,0.20349964395370287,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK191/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL191/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM191/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5333333333333333,"d":"0.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["1190142",11,90,2,14,4,0,0,0,{"v":0,"d":"0.0"},131,0,0,0,1.362,1.1,1.1,1.1,20,0,0,0,3,0,0,0,0.006829581822298132,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK192/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL192/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM192/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.15000000000000002,"d":"0.15"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["1190182",11,90,2,18,9,0,0,0,{"v":0,"d":"0.0"},155,0,0,0,1.362,1.1,1.1,1.1,23,0,0,0,4,0,0,0,0.014813180817340765,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK193/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL193/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM193/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.30000000000000004,"d":"0.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1190262",11,90,2,26,9,0,0,0,{"v":0,"d":"0.0"},210,0,0,0,1.362,1.1,1.1,1.1,31,0,0,0,5,0,0,0,0.02220790314848095,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK194/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL194/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM194/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.30000000000000004,"d":"0.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1190342",11,90,2,34,14,0,0,0,{"v":0,"d":"0.0"},272,0,0,0,1.362,1.1,1.1,1.1,41,0,0,0,7,0,0,0,0.10441004558847257,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK195/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL195/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM195/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["1190422",11,90,2,42,19,0,0,0,{"v":0,"d":"0.0"},383,0,0,0,1.362,1.1,1.1,1.1,57,0,0,0,10,0,0,0,0.33409041252559374,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK196/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL196/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM196/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6000000000000001,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11100142",11,100,2,14,4,0,0,0,{"v":0,"d":"0.0"},153,0,0,0,1.362,1.1,1.1,1.1,23,0,0,0,4,0,0,0,0.012692746488264683,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK197/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL197/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM197/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.16666666666666669,"d":"0.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11100182",11,100,2,18,9,0,0,0,{"v":0,"d":"0.0"},181,0,0,0,1.362,1.1,1.1,1.1,27,0,0,0,5,0,0,0,0.0251325599308642,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK198/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL198/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM198/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.33333333333333337,"d":"0.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11100262",11,100,2,26,9,0,0,0,{"v":0,"d":"0.0"},245,0,0,0,1.362,1.1,1.1,1.1,37,0,0,0,6,0,0,0,0.034987986312321834,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK199/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL199/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM199/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.33333333333333337,"d":"0.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11100342",11,100,2,34,14,0,0,0,{"v":0,"d":"0.0"},317,0,0,0,1.362,1.1,1.1,1.1,47,0,0,0,8,0,0,0,0.1443073062485503,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK200/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL200/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM200/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11100422",11,100,2,42,19,0,0,0,{"v":0,"d":"0.0"},447,0,0,0,1.362,1.1,1.1,1.1,67,0,0,0,12,0,0,0,0.505092315185515,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK201/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL201/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM201/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F201=$BR$70,$C201*$BS$70,IF($F201=$BR$71,$C201*$BS$71,IF($F201=$BR$72,$C201*$BS$72,IF($F201=$BR$73,$C201*$BS$73,IF($F201=$BR$74,$C201*$BS$74,IF($F201=$BR$75,$C201*$BS$75,IF($F201=$BR$76,$C201*$BS$76,IF($F201=$BR$77,$C201*$BS$77,IF($F201=$BR$78,$C201*$BS$78,IF($F201=$BR$79,$C201*$BS$79,IF($F201=$BR$80,$C201*$BS$80,)))))))))))","v":{"v":0.6666666666666667,"d":"0.67"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11110142",11,110,2,14,4,0,0,0,{"v":0,"d":"0.0"},175,0,0,0,1.362,1.1,1.1,1.1,26,0,0,0,4,0,0,0,0.014169445844370371,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK202/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL202/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM202/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM202*(AN202^$BO202)*($C202-14.4)*$BP202)+($BN202*AN202*AN202))","v":0},0,0,{"v":0.18333333333333335,"d":"0.18"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F202=$BR$70,$BT$70,IF($F202=$BR$71,$BT$71,IF($F202=$BR$72,$BT$72,IF($F202=$BR$73,$BT$73,IF($F202=$BR$74,$BT$74,IF($F202=$BR$75,$BT$75,IF($F202=$BR$76,$BT$76,IF($F202=$BR$77,$BT$77,IF($F202=$BR$78,$BT$78,IF($F202=$BR$79,$BT$79,IF($F202=$BR$80,$BT$80,)))))))))))","v":1.3823338826853E-3},{"$f":"IF($F202=$BR$70,$BU$70,IF($F202=$BR$71,$BU$71,IF($F202=$BR$72,$BU$72,IF($F202=$BR$73,$BU$73,IF($F202=$BR$74,$BU$74,IF($F202=$BR$75,$BU$75,IF($F202=$BR$76,$BU$76,IF($F202=$BR$77,$BU$77,IF($F202=$BR$78,$BU$78,IF($F202=$BR$79,$BU$79,IF($F202=$BR$80,$BU$80,)))))))))))","v":0.00033290816326531},{"$f":"IF($F202=$BR$70,$BV$70,IF($F202=$BR$71,$BV$71,IF($F202=$BR$72,$BV$72,IF($F202=$BR$73,$BV$73,IF($F202=$BR$74,$BV$74,IF($F202=$BR$75,$BV$75,IF($F202=$BR$76,$BV$76,IF($F202=$BR$77,$BV$77,IF($F202=$BR$78,$BV$78,IF($F202=$BR$79,$BV$79,IF($F202=$BR$80,$BV$80,)))))))))))","v":1.723172227894},{"$f":"IF($F202=$BR$70,$BW$70,IF($F202=$BR$71,$BW$71,IF($F202=$BR$72,$BW$72,IF($F202=$BR$73,$BW$73,IF($F202=$BR$74,$BW$74,IF($F202=$BR$75,$BW$75,IF($F202=$BR$76,$BW$76,IF($F202=$BR$77,$BW$77,IF($F202=$BR$78,$BW$78,IF($F202=$BR$79,$BW$79,IF($F202=$BR$80,$BW$80,)))))))))))","v":1}]
["11110182",11,110,2,18,9,0,0,0,{"v":0,"d":"0.0"},207,0,0,0,1.362,1.1,1.1,1.1,31,0,0,0,5,0,0,0,0.028057216713247447,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK203/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL203/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM203/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3666666666666667,"d":"0.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11110262",11,110,2,26,9,0,0,0,{"v":0,"d":"0.0"},279,0,0,0,1.362,1.1,1.1,1.1,42,0,0,0,7,0,0,0,0.051665258153112514,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK204/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL204/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM204/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3666666666666667,"d":"0.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11110342",11,110,2,34,14,0,0,0,{"v":0,"d":"0.0"},363,0,0,0,1.362,1.1,1.1,1.1,54,0,0,0,9,0,0,0,0.19215679122977283,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK205/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL205/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM205/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.55,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11110422",11,110,2,42,19,0,0,0,{"v":0,"d":"0.0"},510,0,0,0,1.362,1.1,1.1,1.1,76,0,0,0,13,0,0,0,0.6402806991699274,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK206/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL206/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM206/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7333333333333334,"d":"0.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11120142",11,120,2,14,4,0,0,0,{"v":0,"d":"0.0"},197,0,0,0,1.362,1.1,1.1,1.1,29,0,0,0,5,0,0,0,0.022987530345093,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK207/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL207/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM207/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.2,"d":"0.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11120182",11,120,2,18,9,0,0,0,{"v":0,"d":"0.0"},233,0,0,0,1.362,1.1,1.1,1.1,35,0,0,0,6,0,0,0,0.04312994644649151,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK208/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL208/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM208/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11120262",11,120,2,26,9,0,0,0,{"v":0,"d":"0.0"},314,0,0,0,1.362,1.1,1.1,1.1,47,0,0,0,8,0,0,0,0.07269066515235312,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK209/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL209/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM209/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11120342",11,120,2,34,14,0,0,0,{"v":0,"d":"0.0"},409,0,0,0,1.362,1.1,1.1,1.1,61,0,0,0,{"$f":"ROUND(S210*3600/(4186*ABS($M$1-$M$2)),0)","v":10},0,0,0,0.248422273464841,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK210/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL210/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM210/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11120422",11,120,2,42,19,0,0,0,{"v":0,"d":"0.0"},574,0,0,0,1.362,1.1,1.1,1.1,86,0,0,0,15,0,0,0,0.8874165292349688,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK211/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL211/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM211/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11130142",11,130,2,14,4,0,0,0,{"v":0,"d":"0.0"},218,0,0,0,1.362,1.1,1.1,1.1,33,0,0,0,6,0,0,0,0.03444837355493069,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK212/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL212/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM212/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.21666666666666667,"d":"0.22"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11130182",11,130,2,18,9,0,0,0,{"v":0,"d":"0.0"},259,0,0,0,1.362,1.1,1.1,1.1,39,0,0,0,7,0,0,0,0.06243391135828655,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK213/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL213/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM213/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.43333333333333335,"d":"0.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11130262",11,130,2,26,9,0,0,0,{"v":0,"d":"0.0"},349,0,0,0,1.362,1.1,1.1,1.1,52,0,0,0,9,0,0,0,0.09850482404575009,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK214/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL214/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM214/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.43333333333333335,"d":"0.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11130342",11,130,2,34,14,0,0,0,{"v":0,"d":"0.0"},454,0,0,0,1.362,1.1,1.1,1.1,68,0,0,0,12,0,0,0,0.357112168860067,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK215/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL215/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM215/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.65,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11130422",11,130,2,42,19,0,0,0,{"v":0,"d":"0.0"},638,0,0,0,1.362,1.1,1.1,1.1,95,{"$f":"ROUND(L216*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P216),0)","v":0},{"$f":"ROUND(M216*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q216),0)","v":0},{"$f":"ROUND(N216*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R216),0)","v":0},16,0,0,0,1.075946637015705,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK216/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL216/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM216/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8666666666666667,"d":"0.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11150142",11,150,2,14,4,0,0,0,{"v":0,"d":"0.0"},262,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K217*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O217),0)","v":39},0,0,0,7,0,0,0,0.05268270126173568,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK217/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL217/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM217/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11150182",11,150,2,18,9,0,0,0,{"v":0,"d":"0.0"},310,0,0,0,1.362,1.1,1.1,1.1,46,0,0,0,8,0,0,0,0.09327051475342535,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK218/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL218/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM218/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11150262",11,150,2,26,9,0,0,0,{"v":0,"d":"0.0"},420,0,0,0,1.362,1.1,1.1,1.1,63,0,0,0,11,0,0,0,0.16621787422214895,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK219/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL219/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM219/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11150342",11,150,2,34,14,0,0,0,{"v":0,"d":"0.0"},544,0,0,0,1.362,1.1,1.1,1.1,81,0,0,0,14,0,0,0,0.527312245225952,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK220/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL220/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM220/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11150422",11,150,2,42,19,0,0,0,{"v":0,"d":"0.0"},766,0,0,0,1.362,1.1,1.1,1.1,114,0,0,0,20,0,0,0,1.797931648002438,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK221/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL221/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM221/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11170142",11,170,2,14,4,0,0,0,{"v":0,"d":"0.0"},306,0,0,0,1.362,1.1,1.1,1.1,46,0,0,0,8,0,0,0,0.07607148445486532,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK222/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL222/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM222/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.2833333333333333,"d":"0.28"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11170182",11,170,2,18,9,0,0,0,{"v":0,"d":"0.0"},363,0,0,0,1.362,1.1,1.1,1.1,54,0,0,0,9,0,0,0,0.13248023267380543,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK223/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL223/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM223/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5666666666666667,"d":"0.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11170262",11,170,2,26,9,0,0,0,{"v":0,"d":"0.0"},489,0,0,0,1.362,1.1,1.1,1.1,73,0,0,0,13,0,0,0,0.2581666635757564,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK224/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL224/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM224/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5666666666666667,"d":"0.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11170342",11,170,2,34,14,0,0,0,{"v":0,"d":"0.0"},636,0,0,0,1.362,1.1,1.1,1.1,95,0,0,0,16,0,0,0,0.7386072270235654,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK225/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL225/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM225/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.85,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11170422",11,170,2,42,19,0,0,0,{"v":0,"d":"0.0"},893,0,0,0,1.362,1.1,1.1,1.1,133,0,0,0,23,0,0,0,2.5746979276877155,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK226/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL226/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM226/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1333333333333333,"d":"1.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11190142",11,190,2,14,4,0,0,0,{"v":0,"d":"0.0"},349,0,0,0,1.362,1.1,1.1,1.1,52,0,0,0,9,0,0,0,0.10514306777227453,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK227/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL227/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM227/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3166666666666667,"d":"0.32"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11190182",11,190,2,18,9,0,0,0,{"v":0,"d":"0.0"},414,0,0,0,1.362,1.1,1.1,1.1,62,0,0,0,11,0,0,0,0.21511049502262594,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK228/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL228/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM228/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6333333333333334,"d":"0.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11190262",11,190,2,26,9,0,0,0,{"v":0,"d":"0.0"},559,0,0,0,1.362,1.1,1.1,1.1,83,0,0,0,14,0,0,0,0.33318166555581685,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK229/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL229/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM229/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6333333333333334,"d":"0.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11190342",11,190,2,34,14,0,0,0,{"v":0,"d":"0.0"},726,0,0,0,1.362,1.1,1.1,1.1,108,0,0,0,19,0,0,0,1.0775164283349221,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK230/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL230/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM230/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9500000000000001,"d":"0.95"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11190422",11,190,2,42,19,0,0,0,{"v":0,"d":"0.0"},1021,0,0,0,1.362,1.1,1.1,1.1,152,0,0,0,26,0,0,0,3.5289061273852225,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK231/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL231/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM231/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2666666666666668,"d":"1.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11210142",11,210,2,14,4,0,0,0,{"v":0,"d":"0.0"},393,0,0,0,1.362,1.1,1.1,1.1,59,0,0,0,10,0,0,0,0.14040753186853402,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK232/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL232/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM232/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.35000000000000003,"d":"0.35"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11210182",11,210,2,18,9,0,0,0,{"v":0,"d":"0.0"},466,0,0,0,1.362,1.1,1.1,1.1,70,0,0,0,12,0,0,0,0.2805212841228376,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK233/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL233/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM233/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11210262",11,210,2,26,9,0,0,0,{"v":0,"d":"0.0"},629,0,0,0,1.362,1.1,1.1,1.1,94,0,0,0,16,0,0,0,0.47275442965409814,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK234/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL234/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM234/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11210342",11,210,2,34,14,0,0,0,{"v":0,"d":"0.0"},817,0,0,0,1.362,1.1,1.1,1.1,122,0,0,0,21,0,0,0,1.3937130567605476,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK235/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL235/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM235/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.05,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11210422",11,210,2,42,19,0,0,0,{"v":0,"d":"0.0"},1148,0,0,0,1.362,1.1,1.1,1.1,171,0,0,0,29,0,0,0,4.67371435850924,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK236/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL236/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM236/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4000000000000001,"d":"1.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11230142",11,230,2,14,4,0,0,0,{"v":0,"d":"0.0"},437,0,0,0,1.362,1.1,1.1,1.1,65,0,0,0,11,0,0,0,0.18235929199879208,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK237/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL237/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM237/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.38333333333333336,"d":"0.38"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11230182",11,230,2,18,9,0,0,0,{"v":0,"d":"0.0"},518,0,0,0,1.362,1.1,1.1,1.1,77,0,0,0,13,0,0,0,0.3574626447903286,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK238/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL238/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM238/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7666666666666667,"d":"0.77"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11230262",11,230,2,26,9,0,0,0,{"v":0,"d":"0.0"},699,0,0,0,1.362,1.1,1.1,1.1,104,0,0,0,18,0,0,0,0.6451082967318298,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK239/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL239/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM239/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7666666666666667,"d":"0.77"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11230342",11,230,2,34,14,0,0,0,{"v":0,"d":"0.0"},908,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K240*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O240),0)","v":136},0,0,0,23,0,0,0,1.7597542979096725,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK240/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL240/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM240/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1500000000000001,"d":"1.15"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11230422",11,230,2,42,19,0,0,0,{"v":0,"d":"0.0"},1276,0,0,0,1.362,1.1,1.1,1.1,190,0,0,0,33,0,0,0,6.323242778500345,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK241/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL241/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM241/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5333333333333334,"d":"1.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11250142",11,250,2,14,4,0,0,0,{"v":0,"d":"0.0"},480,0,0,0,1.362,1.1,1.1,1.1,72,0,0,0,12,0,0,0,0.23147910158223278,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK242/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL242/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM242/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4166666666666667,"d":"0.42"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11250182",11,250,2,18,9,0,0,0,{"v":0,"d":"0.0"},569,0,0,0,1.362,1.1,1.1,1.1,85,0,0,0,15,0,0,0,0.5063337677274552,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK243/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL243/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM243/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8333333333333334,"d":"0.83"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11250262",11,250,2,26,9,0,0,0,{"v":0,"d":"0.0"},769,0,0,0,1.362,1.1,1.1,1.1,115,0,0,0,20,0,0,0,0.8532970736833582,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK244/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL244/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM244/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8333333333333334,"d":"0.83"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11250342",11,250,2,34,14,0,0,0,{"v":0,"d":"0.0"},998,0,0,0,1.362,1.1,1.1,1.1,149,0,0,0,26,0,0,0,2.309527045590827,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK245/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL245/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM245/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11250422",11,250,2,42,19,0,0,0,{"v":0,"d":"0.0"},1404,0,0,0,1.362,1.1,1.1,1.1,210,0,0,0,36,0,0,0,7.931804345367134,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK246/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL246/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM246/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6666666666666667,"d":"1.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11270142",11,270,2,14,4,0,0,0,{"v":0,"d":"0.0"},524,0,0,0,1.362,1.1,1.1,1.1,78,0,0,0,13,0,0,0,0.28823563937024926,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK247/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL247/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM247/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11270182",11,270,2,18,9,0,0,0,{"v":0,"d":"0.0"},622,0,0,0,1.362,1.1,1.1,1.1,93,0,0,0,16,0,0,0,0.6174648748773444,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK248/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL248/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM248/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11270262",11,270,2,26,9,0,0,0,{"v":0,"d":"0.0"},839,0,0,0,1.362,1.1,1.1,1.1,125,0,0,0,22,0,0,0,1.100316236930015,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK249/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL249/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM249/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11270342",11,270,2,34,{"$f":"IF($E250=14,4,IF($E250=18,9,IF($E250=26,9,IF($E250=34,14,IF($E250=42,19,)))))","v":14},0,0,0,{"v":0,"d":"0.0"},1090,0,0,0,1.362,1.1,1.1,1.1,163,0,0,0,28,0,0,0,{"$f":"0.0098*(($BM250*(W250^$BO250)*($C250-14.4)*$BP250)+($BN250*W250*W250))","v":2.7987960892795294},0,{"$f":"0.0098*(($BM250*(Y250^$BO250)*($C250-14.4)*$BP250)+($BN250*Y250*Y250))","v":0},{"$f":"0.0098*(($BM250*(Z250^$BO250)*($C250-14.4)*$BP250)+($BN250*Z250*Z250))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK250/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL250/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM250/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.35,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11270422",11,270,2,42,19,0,0,0,{"v":0,"d":"0.0"},1531,0,0,0,1.362,1.1,1.1,1.1,229,0,0,0,39,0,0,0,9.76941007992649,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK251/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL251/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM251/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.8,"d":"1.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11290142",11,290,2,14,4,0,0,0,{"v":0,"d":"0.0"},568,0,0,0,1.362,1.1,1.1,1.1,85,0,0,0,15,0,0,0,0.3976751335873178,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK252/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL252/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM252/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.48333333333333334,"d":"0.48"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11290182",11,290,2,18,9,0,0,0,{"v":0,"d":"0.0"},673,0,0,0,1.362,1.1,1.1,1.1,100,0,0,0,17,0,0,0,0.7430947342425075,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK253/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL253/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM253/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9666666666666667,"d":"0.97"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11290262",11,290,2,26,9,0,0,0,{"v":0,"d":"0.0"},909,0,0,0,1.362,1.1,1.1,1.1,136,0,0,0,23,0,0,0,1.2858920108185188,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK254/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL254/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM254/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9666666666666667,"d":"0.97"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11290342",11,290,2,34,14,0,0,0,{"v":0,"d":"0.0"},1180,0,0,0,1.362,1.1,1.1,1.1,176,0,0,0,30,0,0,0,3.3453100055380482,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK255/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL255/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM255/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11290422",11,290,2,42,19,0,0,0,{"v":0,"d":"0.0"},1659,0,0,0,1.362,1.1,1.1,1.1,248,0,0,0,43,0,0,0,12.298187428650852,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK256/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL256/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM256/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.9333333333333333,"d":"1.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11310142",11,310,2,14,4,0,0,0,{"v":0,"d":"0.0"},612,0,0,0,1.362,1.1,1.1,1.1,91,0,0,0,16,0,0,0,0.4766627369798236,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK257/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL257/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM257/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5166666666666667,"d":"0.52"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11310182",11,310,2,18,9,0,0,0,{"v":0,"d":"0.0"},725,0,0,0,1.362,1.1,1.1,1.1,108,0,0,0,19,0,0,0,0.9751149896615416,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK258/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL258/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM258/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0333333333333334,"d":"1.03"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11310262",11,310,2,26,9,0,0,0,{"v":0,"d":"0.0"},978,0,0,0,1.362,1.1,1.1,1.1,146,0,0,0,25,0,0,0,1.604267233894127,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK259/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL259/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM259/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0333333333333334,"d":"1.03"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11310342",11,310,2,34,14,0,0,0,{"v":0,"d":"0.0"},1271,0,0,0,1.362,1.1,1.1,1.1,190,0,0,0,33,0,0,0,4.137135341481443,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK260/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL260/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM260/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.55,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11310422",11,310,2,42,19,0,0,0,{"v":0,"d":"0.0"},1786,0,0,0,1.362,1.1,1.1,1.1,267,0,0,0,46,0,0,0,14.679216650621687,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK261/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL261/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM261/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.066666666666667,"d":"2.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11330142",11,330,2,14,4,0,0,0,{"v":0,"d":"0.0"},655,0,0,0,1.362,1.1,1.1,1.1,98,0,0,0,17,0,0,0,0.5649069280180107,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK262/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL262/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM262/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.55,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11330182",11,330,2,18,9,0,0,0,{"v":0,"d":"0.0"},777,0,0,0,1.362,1.1,1.1,1.1,116,0,0,0,20,0,0,0,1.1425117112741021,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK263/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL263/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM263/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11330262",11,330,2,26,9,0,0,0,{"v":0,"d":"0.0"},1048,0,0,0,1.362,1.1,1.1,1.1,156,0,0,0,27,0,0,0,1.9692576872906808,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK264/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL264/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM264/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11330342",11,330,2,34,14,0,0,0,{"v":0,"d":"0.0"},1362,0,0,0,1.362,1.1,1.1,1.1,203,0,0,0,35,0,0,0,4.822753599922877,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK265/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL265/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM265/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F265=$BR$70,$C265*$BS$70,IF($F265=$BR$71,$C265*$BS$71,IF($F265=$BR$72,$C265*$BS$72,IF($F265=$BR$73,$C265*$BS$73,IF($F265=$BR$74,$C265*$BS$74,IF($F265=$BR$75,$C265*$BS$75,IF($F265=$BR$76,$C265*$BS$76,IF($F265=$BR$77,$C265*$BS$77,IF($F265=$BR$78,$C265*$BS$78,IF($F265=$BR$79,$C265*$BS$79,IF($F265=$BR$80,$C265*$BS$80,)))))))))))","v":{"v":1.6500000000000001,"d":"1.65"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11330422",11,330,2,42,19,0,0,0,{"v":0,"d":"0.0"},1914,0,0,0,1.362,1.1,1.1,1.1,286,0,0,0,49,0,0,0,17.323631781151413,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK266/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL266/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM266/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM266*(AN266^$BO266)*($C266-14.4)*$BP266)+($BN266*AN266*AN266))","v":0},0,0,{"v":2.2,"d":"2.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F266=$BR$70,$BT$70,IF($F266=$BR$71,$BT$71,IF($F266=$BR$72,$BT$72,IF($F266=$BR$73,$BT$73,IF($F266=$BR$74,$BT$74,IF($F266=$BR$75,$BT$75,IF($F266=$BR$76,$BT$76,IF($F266=$BR$77,$BT$77,IF($F266=$BR$78,$BT$78,IF($F266=$BR$79,$BT$79,IF($F266=$BR$80,$BT$80,)))))))))))","v":0.011616292894075},{"$f":"IF($F266=$BR$70,$BU$70,IF($F266=$BR$71,$BU$71,IF($F266=$BR$72,$BU$72,IF($F266=$BR$73,$BU$73,IF($F266=$BR$74,$BU$74,IF($F266=$BR$75,$BU$75,IF($F266=$BR$76,$BU$76,IF($F266=$BR$77,$BU$77,IF($F266=$BR$78,$BU$78,IF($F266=$BR$79,$BU$79,IF($F266=$BR$80,$BU$80,)))))))))))","v":0.0016553227470232},{"$f":"IF($F266=$BR$70,$BV$70,IF($F266=$BR$71,$BV$71,IF($F266=$BR$72,$BV$72,IF($F266=$BR$73,$BV$73,IF($F266=$BR$74,$BV$74,IF($F266=$BR$75,$BV$75,IF($F266=$BR$76,$BV$76,IF($F266=$BR$77,$BV$77,IF($F266=$BR$78,$BV$78,IF($F266=$BR$79,$BV$79,IF($F266=$BR$80,$BV$80,)))))))))))","v":1.5869346821791},{"$f":"IF($F266=$BR$70,$BW$70,IF($F266=$BR$71,$BW$71,IF($F266=$BR$72,$BW$72,IF($F266=$BR$73,$BW$73,IF($F266=$BR$74,$BW$74,IF($F266=$BR$75,$BW$75,IF($F266=$BR$76,$BW$76,IF($F266=$BR$77,$BW$77,IF($F266=$BR$78,$BW$78,IF($F266=$BR$79,$BW$79,IF($F266=$BR$80,$BW$80,)))))))))))","v":1}]
["11350142",11,350,2,14,4,0,0,0,{"v":0,"d":"0.0"},699,0,0,0,1.362,1.1,1.1,1.1,104,0,0,0,18,0,0,0,0.662834097387835,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK267/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL267/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM267/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5833333333333334,"d":"0.58"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11350182",11,350,2,18,9,0,0,0,{"v":0,"d":"0.0"},828,0,0,0,1.362,1.1,1.1,1.1,124,0,0,0,21,0,0,0,1.3272413019923863,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK268/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL268/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM268/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1666666666666667,"d":"1.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11350262",11,350,2,26,9,0,0,0,{"v":0,"d":"0.0"},1119,0,0,0,1.362,1.1,1.1,1.1,167,0,0,0,29,0,0,0,2.383690892150709,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK269/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL269/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM269/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1666666666666667,"d":"1.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11350342",11,350,2,34,14,0,0,0,{"v":0,"d":"0.0"},1452,0,0,0,1.362,1.1,1.1,1.1,217,0,0,0,37,0,0,0,5.572145786775736,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK270/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL270/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM270/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11350422",11,350,2,42,19,0,0,0,{"v":0,"d":"0.0"},2042,0,0,0,1.362,1.1,1.1,1.1,305,0,0,0,52,0,0,0,20.241512881129434,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK271/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL271/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM271/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.3333333333333335,"d":"2.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11370142",11,370,2,14,4,0,0,0,{"v":0,"d":"0.0"},743,0,0,0,1.362,1.1,1.1,1.1,111,0,0,0,19,0,0,0,0.7708635596858172,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK272/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL272/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM272/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6166666666666667,"d":"0.62"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11370182",11,370,2,18,9,0,0,0,{"v":0,"d":"0.0"},881,0,0,0,1.362,1.1,1.1,1.1,131,0,0,0,23,0,0,{"$f":"ROUND(V273*3600/(4186*ABS($M$1-$M$2)),0)","v":0},1.6585564392109127,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK273/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL273/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM273/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2333333333333334,"d":"1.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11370262",11,370,2,26,9,0,0,0,{"v":0,"d":"0.0"},1188,0,0,0,1.362,1.1,1.1,1.1,177,0,0,0,{"$f":"ROUND(S274*3600/(4186*ABS($M$1-$M$2)),0)","v":30},{"$f":"ROUND(T274*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U274*3600/(4186*ABS($M$1-$M$2)),0)","v":0},0,2.685750673728019,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK274/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL274/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM274/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2333333333333334,"d":"1.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11370342",11,370,2,34,14,0,0,0,{"v":0,"d":"0.0"},1544,0,0,0,1.362,1.1,1.1,1.1,230,0,0,0,40,0,0,0,6.633535903753193,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK275/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL275/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM275/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.85,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11370422",11,370,2,42,19,0,0,0,{"v":0,"d":"0.0"},2169,0,0,0,1.362,1.1,1.1,1.1,324,0,0,0,56,0,0,0,24.123062162221235,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK276/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL276/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM276/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.466666666666667,"d":"2.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11390142",11,390,2,14,4,0,0,0,{"v":0,"d":"0.0"},786,0,0,0,1.362,1.1,1.1,1.1,117,0,0,0,20,0,0,0,0.8894080646281478,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK277/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL277/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM277/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.65,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11390182",11,390,2,18,9,0,0,0,{"v":0,"d":"0.0"},932,0,0,0,1.362,1.1,1.1,1.1,139,0,0,0,24,0,0,0,1.8923252534145938,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK278/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL278/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM278/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11390262",11,390,2,26,9,0,0,0,{"v":0,"d":"0.0"},1258,0,0,0,1.362,1.1,1.1,1.1,188,0,0,0,32,0,0,0,3.1889382440410894,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK279/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL279/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM279/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11390342",11,390,2,34,14,0,0,0,{"v":0,"d":"0.0"},1634,0,0,0,1.362,1.1,1.1,1.1,244,0,0,0,42,0,0,0,7.536235935503717,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK280/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL280/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM280/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.95,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11390422",11,390,2,42,19,0,0,0,{"v":0,"d":"0.0"},2297,0,0,0,1.362,1.1,1.1,1.1,343,0,0,0,59,0,0,0,27.677869363912034,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK281/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL281/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM281/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.6,"d":"2.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11410142",11,410,2,14,4,0,0,0,{"v":0,"d":"0.0"},830,0,0,0,1.362,1.1,1.1,1.1,124,0,0,0,21,0,0,0,1.0188742459048594,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK282/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL282/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM282/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6833333333333333,"d":"0.68"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11410182",11,410,2,18,9,0,0,0,{"v":0,"d":"0.0"},984,0,0,0,1.362,1.1,1.1,1.1,147,0,0,0,25,0,0,0,2.146158230867245,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK283/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL283/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM283/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3666666666666667,"d":"1.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11410262",11,410,2,26,9,0,0,0,{"v":0,"d":"0.0"},1328,0,0,0,1.362,1.1,1.1,1.1,198,0,0,0,34,0,0,0,3.748972931761039,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK284/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL284/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM284/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3666666666666667,"d":"1.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11410342",11,410,2,34,14,0,0,0,{"v":0,"d":"0.0"},1725,0,0,0,1.362,1.1,1.1,1.1,257,0,0,0,44,0,0,0,8.508616611571648,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK285/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL285/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM285/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.05,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11410422",11,410,2,42,19,0,0,0,{"v":0,"d":"0.0"},2424,0,0,0,1.362,1.1,1.1,1.1,362,0,0,0,62,0,0,0,31.536829648248872,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK286/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL286/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM286/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.7333333333333334,"d":"2.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11430142",11,430,2,14,4,0,0,0,{"v":0,"d":"0.0"},874,0,0,0,1.362,1.1,1.1,1.1,130,0,0,0,22,0,0,0,1.159663018072622,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK287/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL287/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM287/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7166666666666667,"d":"0.72"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11430182",11,430,2,18,9,0,0,0,{"v":0,"d":"0.0"},1036,0,0,0,1.362,1.1,1.1,1.1,155,0,0,0,27,0,0,0,2.5923295026565403,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK288/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL288/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM288/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4333333333333333,"d":"1.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11430262",11,430,2,26,9,0,0,0,{"v":0,"d":"0.0"},1398,0,0,0,1.362,1.1,1.1,1.1,209,0,0,0,36,0,0,0,4.368560628829961,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK289/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL289/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM289/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4333333333333333,"d":"1.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11430342",11,430,2,34,14,0,0,0,{"v":0,"d":"0.0"},1816,0,0,0,1.362,1.1,1.1,1.1,271,0,0,0,47,0,0,0,9.864461228652981,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK290/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL290/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM290/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.15,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11430422",11,430,2,42,19,0,0,0,{"v":0,"d":"0.0"},2552,0,0,0,1.362,1.1,1.1,1.1,381,0,0,0,66,0,0,0,36.585263569344576,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK291/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL291/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM291/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8666666666666667,"d":"2.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11450142",11,450,2,14,4,0,0,0,{"v":0,"d":"0.0"},917,0,0,0,1.362,1.1,1.1,1.1,137,0,0,0,24,0,0,0,1.4120398132145129,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK292/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL292/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM292/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11450182",11,450,2,18,9,0,0,0,{"v":0,"d":"0.0"},1087,0,0,0,1.362,1.1,1.1,1.1,162,0,0,0,28,0,0,0,2.9022339379111846,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK293/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL293/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM293/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11450262",11,450,2,26,9,0,0,0,{"v":0,"d":"0.0"},1468,0,0,0,1.362,1.1,1.1,1.1,219,0,0,0,38,0,0,0,5.050379452042899,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK294/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL294/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM294/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11450342",11,450,2,34,14,0,0,0,{"v":0,"d":"0.0"},1906,0,0,0,1.362,1.1,1.1,1.1,284,0,0,0,49,0,0,0,11.003116713825555,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK295/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL295/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM295/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11450422",11,450,2,42,19,0,0,0,{"v":0,"d":"0.0"},2680,0,0,0,1.362,1.1,1.1,1.1,400,0,0,0,69,0,0,0,41.146306509756855,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK296/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL296/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM296/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3,"d":"3.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11470142",11,470,2,14,4,0,0,0,{"v":0,"d":"0.0"},961,0,0,0,1.362,1.1,1.1,1.1,143,0,0,0,25,0,0,0,1.5844312990375478,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK297/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL297/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM297/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7833333333333334,"d":"0.78"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11470182",11,470,2,18,9,0,0,0,{"v":0,"d":"0.0"},1140,0,0,0,1.362,1.1,1.1,1.1,170,0,0,0,29,0,0,0,3.2348509864346173,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK298/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL298/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM298/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5666666666666669,"d":"1.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11470262",11,470,2,26,9,0,0,0,{"v":0,"d":"0.0"},1537,0,0,0,1.362,1.1,1.1,1.1,229,0,0,0,39,0,0,0,5.5368539217238775,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK299/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL299/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM299/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5666666666666669,"d":"1.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11470342",11,470,2,34,14,0,0,0,{"v":0,"d":"0.0"},1998,0,0,0,1.362,1.1,1.1,1.1,298,0,0,0,51,0,0,0,12.216886318343574,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK300/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL300/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM300/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.35,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11470422",11,470,2,42,19,0,0,0,{"v":0,"d":"0.0"},2807,0,0,0,1.362,1.1,1.1,1.1,419,0,0,0,72,0,0,0,46.04014638832283,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK301/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL301/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM301/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1333333333333337,"d":"3.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["11490142",11,490,2,14,4,0,0,0,{"v":0,"d":"0.0"},1005,0,0,0,1.362,1.1,1.1,1.1,150,0,0,0,26,0,0,0,1.7695598738459763,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK302/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL302/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM302/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8166666666666668,"d":"0.82"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["11490182",11,490,2,18,9,0,0,0,{"v":0,"d":"0.0"},1191,0,0,0,1.362,1.1,1.1,1.1,178,0,0,{"$f":"ROUND(N303*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R303),0)","v":0},31,0,0,0,3.81096875424071,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK303/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL303/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM303/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6333333333333335,"d":"1.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11490262",11,490,2,26,9,0,0,0,{"v":0,"d":"0.0"},1608,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K304*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O304),0)","v":240},{"$f":"ROUND(L304*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P304),0)","v":0},{"$f":"ROUND(M304*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q304),0)","v":0},0,41,0,0,0,6.328511583070077,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK304/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL304/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM304/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6333333333333335,"d":"1.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["11490342",11,490,2,34,14,0,0,0,{"v":0,"d":"0.0"},2088,0,0,0,1.362,1.1,1.1,1.1,312,0,0,0,54,0,0,0,13.89008218145171,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK305/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL305/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM305/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["11490422",11,490,2,42,19,0,0,0,{"v":0,"d":"0.0"},2935,0,0,0,1.362,1.1,1.1,1.1,438,0,0,0,75,0,0,0,51.27536785366567,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK306/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL306/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM306/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.266666666666667,"d":"3.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["1470142",14,70,2,14,{"$f":"IF($E307=14,5,IF($E307=26,10,IF($E307=34,15,IF($E307=42,20,))))","v":5},0,0,0,{"v":0,"d":"0.0"},99,0,0,0,1.362,1.1,1.1,1.1,15,0,0,0,3,0,0,0,6.4730267114827406E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK307/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL307/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM307/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.23333333333333334,"d":"0.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1470262",14,70,2,26,{"$f":"IF($E308=14,5,IF($E308=26,10,IF($E308=34,15,IF($E308=42,20,))))","v":10},0,0,0,{"v":0,"d":"0.0"},172,0,0,0,1.362,1.1,1.1,1.1,26,0,0,0,4,0,0,0,0.012474492861344375,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK308/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL308/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM308/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4666666666666667,"d":"0.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1470342",14,70,2,34,15,0,0,0,{"v":0,"d":"0.0"},235,0,0,0,1.362,1.1,1.1,1.1,35,0,0,0,6,0,0,0,0.005208367161684071,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK309/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL309/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM309/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["1470422",14,70,2,42,20,0,0,0,{"v":0,"d":"0.0"},317,0,0,0,1.362,1.1,1.1,1.1,47,0,0,0,8,0,0,0,0.03163644583066969,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK310/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL310/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM310/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9333333333333333,"d":"0.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["1480142",14,80,2,14,5,0,0,0,{"v":0,"d":"0.0"},124,0,0,0,1.362,1.1,1.1,1.1,19,0,0,0,3,0,0,0,7.630927336835948E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK311/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL311/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM311/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.26666666666666666,"d":"0.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
[{"$f":"CONCATENATE(B312,C312,E312,D312)","v":"1480262"},14,80,2,26,10,0,0,0,{"v":0,"d":"0.0"},215,0,0,0,1.362,1.1,1.1,1.1,32,0,0,0,6,0,0,0,0.026901125524058062,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE312*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH312),0)","v":0},{"$f":"ROUND(AF312*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI312),0)","v":0},{"$f":"ROUND(AG312*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ312),0)","v":0},{"$f":"ROUND(AK312*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL312*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM312*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK312/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL312/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM312/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5333333333333333,"d":"0.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1480342",14,80,2,34,15,0,0,0,{"v":0,"d":"0.0"},294,0,0,0,1.362,1.1,1.1,1.1,44,0,0,0,8,0,0,0,0.010185863580687435,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK313/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL313/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM313/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["1480422",14,80,2,42,20,0,0,0,{"v":0,"d":"0.0"},396,0,0,0,1.362,1.1,1.1,1.1,59,0,0,0,10,0,0,0,{"$f":"0.0098*(($BM314*(W314^$BO314)*($C314-14.4)*$BP314)+($BN314*W314*W314))","v":0.05065646652322561},0,{"$f":"0.0098*(($BM314*(Y314^$BO314)*($C314-14.4)*$BP314)+($BN314*Y314*Y314))","v":0},{"$f":"0.0098*(($BM314*(Z314^$BO314)*($C314-14.4)*$BP314)+($BN314*Z314*Z314))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK314/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL314/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM314/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0666666666666667,"d":"1.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["1490142",14,90,2,14,5,0,0,0,{"v":0,"d":"0.0"},149,0,0,0,1.362,1.1,1.1,1.1,22,0,0,0,4,0,0,0,0.014813180817340765,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK315/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL315/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM315/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.30000000000000004,"d":"0.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1490262",14,90,2,26,10,0,0,0,{"v":0,"d":"0.0"},258,0,0,0,1.362,1.1,1.1,1.1,39,0,0,0,7,0,0,0,0.038976231269433524,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK316/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL316/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM316/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6000000000000001,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1490342",14,90,2,34,15,0,0,0,{"v":0,"d":"0.0"},353,0,0,0,1.362,1.1,1.1,1.1,53,0,0,0,9,0,0,0,0.014410551604897005,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK317/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL317/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM317/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["1490422",14,90,2,42,20,0,0,0,{"v":0,"d":"0.0"},475,0,0,0,1.362,1.1,1.1,1.1,71,0,0,0,12,0,0,0,0.07491913985338658,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK318/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL318/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM318/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2000000000000002,"d":"1.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14100142",14,100,2,14,5,0,0,0,{"v":0,"d":"0.0"},174,0,0,0,1.362,1.1,1.1,1.1,26,0,0,0,4,0,0,0,0.016764342481123313,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK319/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL319/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM319/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.33333333333333337,"d":"0.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14100262",14,100,2,26,10,0,0,0,{"v":0,"d":"0.0"},301,0,0,0,1.362,1.1,1.1,1.1,45,0,0,0,8,0,0,0,0.053810845185502394,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK320/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL320/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM320/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6666666666666667,"d":"0.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14100342",14,100,2,34,15,0,0,0,{"v":0,"d":"0.0"},411,0,0,0,1.362,1.1,1.1,1.1,61,0,0,0,10,0,0,0,0.01960857205245291,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK321/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL321/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM321/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14100422",14,100,2,42,20,0,0,0,{"v":0,"d":"0.0"},555,0,0,0,1.362,1.1,1.1,1.1,83,0,0,0,14,0,0,0,0.1047454451276107,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK322/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL322/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM322/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3333333333333335,"d":"1.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14110142",14,110,2,14,5,0,0,0,{"v":0,"d":"0.0"},198,0,0,0,1.362,1.1,1.1,1.1,30,0,0,0,5,0,0,0,0.028057216713247447,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK323/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL323/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM323/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3666666666666667,"d":"0.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14110262",14,110,2,26,10,0,0,0,{"v":0,"d":"0.0"},345,0,0,0,1.362,1.1,1.1,1.1,51,0,0,0,9,0,0,0,0.07158444572576048,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK324/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL324/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM324/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7333333333333334,"d":"0.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14110342",14,110,2,34,15,0,0,0,{"v":0,"d":"0.0"},470,0,0,0,1.362,1.1,1.1,1.1,70,0,0,0,12,0,0,0,0.03017609091374174,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK325/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL325/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM325/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14110422",14,110,2,42,20,0,0,0,{"v":0,"d":"0.0"},633,0,0,0,1.362,1.1,1.1,1.1,94,0,0,0,16,0,0,0,0.140427661064783,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK326/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL326/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM326/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4666666666666668,"d":"1.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14120142",14,120,2,14,5,0,0,0,{"v":0,"d":"0.0"},223,0,0,0,1.362,1.1,1.1,1.1,33,0,0,0,6,0,0,0,0.04312994644649151,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK327/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL327/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM327/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14120262",14,120,2,26,10,0,0,0,{"v":0,"d":"0.0"},388,0,0,0,1.362,1.1,1.1,1.1,58,0,0,0,10,0,0,0,0.09246559738077666,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK328/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL328/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM328/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14120342",14,120,2,34,15,0,0,0,{"v":0,"d":"0.0"},529,0,0,0,1.362,1.1,1.1,1.1,79,0,0,0,14,0,0,0,0.04370880048019538,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK329/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL329/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM329/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F329=$BR$70,$C329*$BS$70,IF($F329=$BR$71,$C329*$BS$71,IF($F329=$BR$72,$C329*$BS$72,IF($F329=$BR$73,$C329*$BS$73,IF($F329=$BR$74,$C329*$BS$74,IF($F329=$BR$75,$C329*$BS$75,IF($F329=$BR$76,$C329*$BS$76,IF($F329=$BR$77,$C329*$BS$77,IF($F329=$BR$78,$C329*$BS$78,IF($F329=$BR$79,$C329*$BS$79,IF($F329=$BR$80,$C329*$BS$80,)))))))))))","v":{"v":1.2,"d":"1.20"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14120422",14,120,2,42,20,0,0,0,{"v":0,"d":"0.0"},713,0,0,0,1.362,1.1,1.1,1.1,106,0,0,0,18,0,0,0,0.182235125642486,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK330/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL330/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM330/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM330*(AN330^$BO330)*($C330-14.4)*$BP330)+($BN330*AN330*AN330))","v":0},0,0,{"v":1.6,"d":"1.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F330=$BR$70,$BT$70,IF($F330=$BR$71,$BT$71,IF($F330=$BR$72,$BT$72,IF($F330=$BR$73,$BT$73,IF($F330=$BR$74,$BT$74,IF($F330=$BR$75,$BT$75,IF($F330=$BR$76,$BT$76,IF($F330=$BR$77,$BT$77,IF($F330=$BR$78,$BT$78,IF($F330=$BR$79,$BT$79,IF($F330=$BR$80,$BT$80,)))))))))))","v":1.6730950035507E-3},{"$f":"IF($F330=$BR$70,$BU$70,IF($F330=$BR$71,$BU$71,IF($F330=$BR$72,$BU$72,IF($F330=$BR$73,$BU$73,IF($F330=$BR$74,$BU$74,IF($F330=$BR$75,$BU$75,IF($F330=$BR$76,$BU$76,IF($F330=$BR$77,$BU$77,IF($F330=$BR$78,$BU$78,IF($F330=$BR$79,$BU$79,IF($F330=$BR$80,$BU$80,)))))))))))","v":0.00032929523945446},{"$f":"IF($F330=$BR$70,$BV$70,IF($F330=$BR$71,$BV$71,IF($F330=$BR$72,$BV$72,IF($F330=$BR$73,$BV$73,IF($F330=$BR$74,$BV$74,IF($F330=$BR$75,$BV$75,IF($F330=$BR$76,$BV$76,IF($F330=$BR$77,$BV$77,IF($F330=$BR$78,$BV$78,IF($F330=$BR$79,$BV$79,IF($F330=$BR$80,$BV$80,)))))))))))","v":1.3691788367472},{"$f":"IF($F330=$BR$70,$BW$70,IF($F330=$BR$71,$BW$71,IF($F330=$BR$72,$BW$72,IF($F330=$BR$73,$BW$73,IF($F330=$BR$74,$BW$74,IF($F330=$BR$75,$BW$75,IF($F330=$BR$76,$BW$76,IF($F330=$BR$77,$BW$77,IF($F330=$BR$78,$BW$78,IF($F330=$BR$79,$BW$79,IF($F330=$BR$80,$BW$80,)))))))))))","v":2}]
["14130142",14,130,2,14,5,0,0,0,{"v":0,"d":"0.0"},248,0,0,0,1.362,1.1,1.1,1.1,37,0,0,0,6,0,0,0,0.04720092651357636,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK331/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL331/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM331/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.43333333333333335,"d":"0.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14130262",14,130,2,26,10,0,0,0,{"v":0,"d":"0.0"},431,0,0,0,1.362,1.1,1.1,1.1,64,0,0,0,11,0,0,0,0.11661370499829944,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK332/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL332/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM332/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8666666666666667,"d":"0.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14130342",14,130,2,34,15,0,0,0,{"v":0,"d":"0.0"},587,0,0,0,1.362,1.1,1.1,1.1,88,0,0,0,15,0,0,0,0.05397338747807479,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK333/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL333/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM333/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14130422",14,130,2,42,20,0,0,0,{"v":0,"d":"0.0"},792,0,0,0,1.362,1.1,1.1,1.1,118,0,0,0,20,0,0,0,0.23041835167355365,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK334/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL334/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM334/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.7333333333333334,"d":"1.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14150142",14,150,2,14,5,0,0,0,{"v":0,"d":"0.0"},298,0,0,0,1.362,1.1,1.1,1.1,44,0,0,0,8,0,0,0,0.09327051475342535,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK335/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL335/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM335/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14150262",14,150,2,26,10,0,0,0,{"v":0,"d":"0.0"},516,0,0,0,1.362,1.1,1.1,1.1,77,0,0,0,13,0,0,0,0.17531029636491535,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK336/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL336/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM336/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14150342",14,150,2,34,15,0,0,0,{"v":0,"d":"0.0"},705,0,0,0,1.362,1.1,1.1,1.1,105,0,0,0,18,0,0,{"$f":"ROUND(V337*3600/(4186*ABS($M$1-$M$2)),0)","v":0},0.08719173065208868,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK337/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL337/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM337/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14150422",14,150,2,42,20,0,0,0,{"v":0,"d":"0.0"},950,0,0,0,1.362,1.1,1.1,1.1,142,0,0,0,{"$f":"ROUND(S338*3600/(4186*ABS($M$1-$M$2)),0)","v":24},{"$f":"ROUND(T338*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U338*3600/(4186*ABS($M$1-$M$2)),0)","v":0},0,0.3468375885819408,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK338/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL338/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM338/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2,"d":"2.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14170142",14,170,2,14,5,0,0,0,{"v":0,"d":"0.0"},347,0,0,0,1.362,1.1,1.1,1.1,52,0,0,0,9,0,0,0,0.13248023267380543,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK339/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL339/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM339/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5666666666666667,"d":"0.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14170262",14,170,2,26,10,0,0,0,{"v":0,"d":"0.0"},603,0,0,0,1.362,1.1,1.1,1.1,90,0,0,0,15,0,0,0,0.24881011485076113,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK340/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL340/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM340/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1333333333333333,"d":"1.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14170342",14,170,2,34,15,0,0,0,{"v":0,"d":"0.0"},822,0,0,0,1.362,1.1,1.1,1.1,123,0,0,0,21,0,0,0,0.13115972001833867,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK341/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL341/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM341/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.7,"d":"1.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14170422",14,170,2,42,20,0,0,0,{"v":0,"d":"0.0"},1108,0,0,0,1.362,1.1,1.1,1.1,165,0,0,0,28,0,0,0,0.4914124563508791,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK342/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL342/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM342/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.2666666666666666,"d":"2.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14190142",14,190,2,14,5,0,0,0,{"v":0,"d":"0.0"},397,0,0,0,1.362,1.1,1.1,1.1,59,0,0,0,10,0,0,0,0.18095230333090526,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK343/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL343/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM343/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6333333333333334,"d":"0.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14190262",14,190,2,26,10,0,0,0,{"v":0,"d":"0.0"},689,0,0,0,1.362,1.1,1.1,1.1,103,0,0,0,18,0,0,0,0.36819469221879325,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK344/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL344/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM344/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2666666666666668,"d":"1.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14190342",14,190,2,34,15,0,0,0,{"v":0,"d":"0.0"},940,0,0,0,1.362,1.1,1.1,1.1,140,0,0,0,24,0,0,0,0.1871571239889759,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK345/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL345/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM345/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.9000000000000001,"d":"1.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14190422",14,190,2,42,20,0,0,0,{"v":0,"d":"0.0"},1267,0,0,0,1.362,1.1,1.1,1.1,189,0,0,0,33,0,0,0,0.6944193035978685,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK346/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL346/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM346/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.5333333333333337,"d":"2.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14210142",14,210,2,14,5,0,0,0,{"v":0,"d":"0.0"},446,0,0,0,1.362,1.1,1.1,1.1,67,0,0,0,12,0,0,0,0.2805212841228376,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK347/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL347/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM347/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14210262",14,210,2,26,10,0,0,0,{"v":0,"d":"0.0"},775,0,0,0,1.362,1.1,1.1,1.1,116,0,0,0,20,0,0,0,0.4796053764226092,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK348/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL348/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM348/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4000000000000001,"d":"1.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14210342",14,210,2,34,15,0,0,0,{"v":0,"d":"0.0"},1057,0,0,0,1.362,1.1,1.1,1.1,158,0,0,0,27,0,0,0,0.25642310317388495,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK349/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL349/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM349/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.1,"d":"2.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14210422",14,210,2,42,20,0,0,0,{"v":0,"d":"0.0"},1425,0,0,0,1.362,1.1,1.1,1.1,213,0,0,0,37,0,0,0,0.9045248850913218,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK350/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL350/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM350/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8000000000000003,"d":"2.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14230142",14,230,2,14,5,0,0,0,{"v":0,"d":"0.0"},496,0,0,0,1.362,1.1,1.1,1.1,74,0,0,0,13,0,0,0,0.3574626447903286,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK351/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL351/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM351/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7666666666666667,"d":"0.77"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14230262",14,230,2,26,10,0,0,0,{"v":0,"d":"0.0"},861,0,0,0,1.362,1.1,1.1,1.1,129,0,0,0,22,0,0,0,0.609041444578151,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK352/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL352/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM352/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5333333333333334,"d":"1.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14230342",14,230,2,34,15,0,0,0,{"v":0,"d":"0.0"},1175,0,0,0,1.362,1.1,1.1,1.1,175,0,0,0,30,0,0,0,0.34016222089904613,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK353/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL353/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM353/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.3000000000000003,"d":"2.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14230422",14,230,2,42,20,0,0,0,{"v":0,"d":"0.0"},1583,0,0,0,1.362,1.1,1.1,1.1,236,0,0,0,41,0,0,0,1.1472902530997895,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK354/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL354/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM354/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.066666666666667,"d":"3.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14250142",14,250,2,14,5,0,0,0,{"v":0,"d":"0.0"},546,0,0,0,1.362,1.1,1.1,1.1,81,0,0,0,14,0,0,0,0.4467638804395164,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK355/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL355/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM355/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8333333333333334,"d":"0.83"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14250262",14,250,2,26,10,0,0,0,{"v":0,"d":"0.0"},947,0,0,0,1.362,1.1,1.1,1.1,141,0,0,0,24,0,0,0,0.7573657940768075,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK356/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL356/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM356/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6666666666666667,"d":"1.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14250342",14,250,2,34,15,0,0,0,{"v":0,"d":"0.0"},1292,0,0,0,1.362,1.1,1.1,1.1,193,0,0,0,33,0,0,0,0.4395490119763462,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK357/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL357/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM357/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.5,"d":"2.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14250422",14,250,2,42,20,0,0,0,{"v":0,"d":"0.0"},1742,0,0,0,1.362,1.1,1.1,1.1,260,0,0,0,45,0,0,0,1.4239450396110673,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK358/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL358/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM358/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.3333333333333335,"d":"3.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14270142",14,270,2,14,5,0,0,0,{"v":0,"d":"0.0"},595,0,0,0,1.362,1.1,1.1,1.1,89,0,0,0,15,0,0,0,0.5492417717057644,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK359/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL359/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM359/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14270262",14,270,2,26,10,0,0,0,{"v":0,"d":"0.0"},1034,0,0,0,1.362,1.1,1.1,1.1,154,0,0,0,26,0,0,0,0.9254015366324477,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK360/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL360/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM360/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.8,"d":"1.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14270342",14,270,2,34,15,0,0,0,{"v":0,"d":"0.0"},1409,0,0,0,1.362,1.1,1.1,1.1,210,0,0,0,36,0,0,0,0.5557315626984591,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK361/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL361/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM361/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.7,"d":"2.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14270422",14,270,2,42,20,0,0,0,{"v":0,"d":"0.0"},1900,0,0,0,1.362,1.1,1.1,1.1,284,0,0,0,49,0,0,0,1.735646743999081,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK362/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL362/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM362/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.6,"d":"3.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14290142",14,290,2,14,5,0,0,0,{"v":0,"d":"0.0"},645,0,0,0,1.362,1.1,1.1,1.1,96,0,0,0,17,0,0,0,0.7430947342425075,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK363/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL363/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM363/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9666666666666667,"d":"0.97"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14290262",14,290,2,26,10,0,0,0,{"v":0,"d":"0.0"},1119,0,0,0,1.362,1.1,1.1,1.1,167,0,0,0,29,0,0,0,1.1736574966755882,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK364/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL364/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM364/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.9333333333333333,"d":"1.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14290342",14,290,2,34,15,0,0,0,{"v":0,"d":"0.0"},1527,0,0,0,1.362,1.1,1.1,1.1,228,0,0,0,39,0,0,0,0.6898343849472528,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK365/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL365/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM365/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.9,"d":"2.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14290422",14,290,2,42,20,0,0,0,{"v":0,"d":"0.0"},2058,0,0,0,1.362,1.1,1.1,1.1,307,0,0,0,53,0,0,0,2.083490757889303,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK366/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL366/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM366/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.8666666666666667,"d":"3.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14310142",14,310,2,14,5,0,0,0,{"v":0,"d":"0.0"},694,0,0,0,1.362,1.1,1.1,1.1,104,0,0,0,18,0,0,0,0.8840117194736292,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK367/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL367/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM367/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0333333333333334,"d":"1.03"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14310262",14,310,2,26,10,0,0,0,{"v":0,"d":"0.0"},1206,0,0,0,1.362,1.1,1.1,1.1,180,0,0,0,31,0,0,0,1.3899265044299594,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK368/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL368/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM368/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.066666666666667,"d":"2.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14310342",14,310,2,34,15,0,0,0,{"v":0,"d":"0.0"},1644,0,0,0,1.362,1.1,1.1,1.1,245,0,0,0,42,0,0,0,0.8429607698254645,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK369/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL369/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM369/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1,"d":"3.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14310422",14,310,2,42,20,0,0,0,{"v":0,"d":"0.0"},2217,0,0,0,1.362,1.1,1.1,1.1,331,0,0,0,57,0,0,0,2.468518316122651,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK370/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL370/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM370/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.133333333333334,"d":"4.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14330142",14,330,2,14,5,0,0,0,{"v":0,"d":"0.0"},744,0,0,0,1.362,1.1,1.1,1.1,111,0,0,0,19,0,0,0,1.040995038400773,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK371/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL371/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM371/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14330262",14,330,2,26,{"$f":"IF($E372=14,5,IF($E372=26,10,IF($E372=34,15,IF($E372=42,20,))))","v":10},0,0,0,{"v":0,"d":"0.0"},1292,0,0,0,1.362,1.1,1.1,1.1,193,0,0,0,33,0,0,0,1.628396929103065,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK372/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL372/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM372/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.2,"d":"2.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14330342",14,330,2,34,15,0,0,0,{"v":0,"d":"0.0"},1762,0,0,0,1.362,1.1,1.1,1.1,263,0,0,0,45,0,0,0,1.0161947471826447,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK373/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL373/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM373/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.3000000000000003,"d":"3.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14330422",14,330,2,42,20,0,0,0,{"v":0,"d":"0.0"},2375,0,0,0,1.362,1.1,1.1,1.1,354,0,0,0,61,0,0,0,2.8917229234133024,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK374/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL374/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM374/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.4,"d":"4.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14350142",14,350,2,14,5,0,0,0,{"v":0,"d":"0.0"},794,0,0,0,1.362,1.1,1.1,1.1,119,0,0,0,20,0,0,0,1.214815370671788,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK375/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL375/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM375/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1666666666666667,"d":"1.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14350262",14,350,2,26,10,0,0,0,{"v":0,"d":"0.0"},1377,0,0,0,1.362,1.1,1.1,1.1,206,0,0,0,35,0,0,0,1.8897670298211189,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK376/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL376/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM376/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.3333333333333335,"d":"2.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14350342",14,350,2,34,15,0,0,0,{"v":0,"d":"0.0"},1880,0,0,0,1.362,1.1,1.1,1.1,281,0,0,0,48,0,0,0,1.2106027400026835,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK377/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL377/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM377/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.5,"d":"3.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14350422",14,350,2,42,20,0,0,0,{"v":0,"d":"0.0"},2533,0,0,0,1.362,1.1,1.1,1.1,378,0,0,0,65,0,0,0,{"$f":"0.0098*(($BM378*(W378^$BO378)*($C378-14.4)*$BP378)+($BN378*W378*W378))","v":3.3540556329986537},0,{"$f":"0.0098*(($BM378*(Y378^$BO378)*($C378-14.4)*$BP378)+($BN378*Y378*Y378))","v":0},{"$f":"0.0098*(($BM378*(Z378^$BO378)*($C378-14.4)*$BP378)+($BN378*Z378*Z378))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK378/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL378/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM378/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.666666666666667,"d":"4.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14370142",14,370,2,14,5,0,0,0,{"v":0,"d":"0.0"},843,0,0,0,1.362,1.1,1.1,1.1,126,0,0,0,22,0,0,0,1.5300614161537585,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK379/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL379/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM379/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2333333333333334,"d":"1.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14370262",14,370,2,26,10,0,0,0,{"v":0,"d":"0.0"},1464,0,0,0,1.362,1.1,1.1,1.1,219,0,0,0,38,0,0,0,2.2627519844441517,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK380/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL380/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM380/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.466666666666667,"d":"2.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14370342",14,370,2,34,15,0,0,0,{"v":0,"d":"0.0"},1997,0,0,0,1.362,1.1,1.1,1.1,298,0,0,0,51,0,0,0,1.4272349780191318,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK381/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL381/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM381/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.7,"d":"3.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14370422",14,370,2,42,20,0,0,0,{"v":0,"d":"0.0"},2692,0,0,0,1.362,1.1,1.1,1.1,402,0,0,0,69,0,0,0,3.8564294425443095,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK382/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL382/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM382/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.933333333333334,"d":"4.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14390142",14,390,2,14,5,0,0,0,{"v":0,"d":"0.0"},893,0,0,0,1.362,1.1,1.1,1.1,133,0,0,0,23,0,0,0,1.751722546309011,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK383/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL383/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM383/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14390262",14,390,2,26,10,0,0,0,{"v":0,"d":"0.0"},1550,0,0,0,1.362,1.1,1.1,1.1,231,0,0,0,40,0,0,0,2.579256810384885,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK384/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL384/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM384/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.6,"d":"2.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14390342",14,390,2,34,15,0,0,0,{"v":0,"d":"0.0"},2115,0,0,0,1.362,1.1,1.1,1.1,316,0,0,0,54,0,0,0,1.6671267182234404,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK385/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL385/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM385/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.9,"d":"3.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14390422",14,390,2,42,20,0,0,0,{"v":0,"d":"0.0"},2850,0,0,0,1.362,1.1,1.1,1.1,425,0,0,0,73,0,0,0,4.399722999012772,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK386/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL386/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM386/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":5.2,"d":"5.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14410142",14,410,2,14,5,0,0,0,{"v":0,"d":"0.0"},942,0,0,0,1.362,1.1,1.1,1.1,141,0,0,0,24,0,0,0,1.9929684324564143,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK387/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL387/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM387/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3666666666666667,"d":"1.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14410262",14,410,2,26,10,0,0,0,{"v":0,"d":"0.0"},1636,0,0,0,1.362,1.1,1.1,1.1,244,0,0,0,42,0,0,0,2.9208214373110297,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK388/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL388/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM388/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.7333333333333334,"d":"2.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14410342",14,410,2,34,15,0,0,0,{"v":0,"d":"0.0"},2232,0,0,0,1.362,1.1,1.1,1.1,333,0,0,0,57,0,0,0,1.931299308281275,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK389/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL389/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM389/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.1,"d":"4.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14410422",14,410,2,42,20,0,0,0,{"v":0,"d":"0.0"},3008,0,0,0,1.362,1.1,1.1,1.1,449,0,0,0,77,0,0,0,4.984783754065478,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK390/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL390/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM390/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":5.466666666666667,"d":"5.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14430142",14,430,2,14,5,0,0,0,{"v":0,"d":"0.0"},992,0,0,0,1.362,1.1,1.1,1.1,148,0,0,0,25,0,0,0,2.2545364302618687,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK391/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL391/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM391/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4333333333333333,"d":"1.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14430262",14,430,2,26,10,0,0,0,{"v":0,"d":"0.0"},1722,0,0,0,1.362,1.1,1.1,1.1,257,0,0,0,44,0,0,0,3.2880624737548576,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK392/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL392/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM392/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8666666666666667,"d":"2.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14430342",14,430,2,34,15,0,0,0,{"v":0,"d":"0.0"},2349,0,0,0,1.362,1.1,1.1,1.1,351,0,0,0,60,0,0,0,2.220761120552108,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK393/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL393/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM393/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F393=$BR$70,$C393*$BS$70,IF($F393=$BR$71,$C393*$BS$71,IF($F393=$BR$72,$C393*$BS$72,IF($F393=$BR$73,$C393*$BS$73,IF($F393=$BR$74,$C393*$BS$74,IF($F393=$BR$75,$C393*$BS$75,IF($F393=$BR$76,$C393*$BS$76,IF($F393=$BR$77,$C393*$BS$77,IF($F393=$BR$78,$C393*$BS$78,IF($F393=$BR$79,$C393*$BS$79,IF($F393=$BR$80,$C393*$BS$80,)))))))))))","v":{"v":4.3,"d":"4.30"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14430422",14,430,2,42,20,0,0,0,{"v":0,"d":"0.0"},3167,0,0,0,1.362,1.1,1.1,1.1,473,0,0,0,81,0,0,0,5.612430676530627,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK394/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL394/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM394/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM394*(AN394^$BO394)*($C394-14.4)*$BP394)+($BN394*AN394*AN394))","v":0},0,0,{"v":5.733333333333333,"d":"5.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F394=$BR$70,$BT$70,IF($F394=$BR$71,$BT$71,IF($F394=$BR$72,$BT$72,IF($F394=$BR$73,$BT$73,IF($F394=$BR$74,$BT$74,IF($F394=$BR$75,$BT$75,IF($F394=$BR$76,$BT$76,IF($F394=$BR$77,$BT$77,IF($F394=$BR$78,$BT$78,IF($F394=$BR$79,$BT$79,IF($F394=$BR$80,$BT$80,)))))))))))","v":1.6730950035507E-3},{"$f":"IF($F394=$BR$70,$BU$70,IF($F394=$BR$71,$BU$71,IF($F394=$BR$72,$BU$72,IF($F394=$BR$73,$BU$73,IF($F394=$BR$74,$BU$74,IF($F394=$BR$75,$BU$75,IF($F394=$BR$76,$BU$76,IF($F394=$BR$77,$BU$77,IF($F394=$BR$78,$BU$78,IF($F394=$BR$79,$BU$79,IF($F394=$BR$80,$BU$80,)))))))))))","v":0.00032929523945446},{"$f":"IF($F394=$BR$70,$BV$70,IF($F394=$BR$71,$BV$71,IF($F394=$BR$72,$BV$72,IF($F394=$BR$73,$BV$73,IF($F394=$BR$74,$BV$74,IF($F394=$BR$75,$BV$75,IF($F394=$BR$76,$BV$76,IF($F394=$BR$77,$BV$77,IF($F394=$BR$78,$BV$78,IF($F394=$BR$79,$BV$79,IF($F394=$BR$80,$BV$80,)))))))))))","v":1.3691788367472},{"$f":"IF($F394=$BR$70,$BW$70,IF($F394=$BR$71,$BW$71,IF($F394=$BR$72,$BW$72,IF($F394=$BR$73,$BW$73,IF($F394=$BR$74,$BW$74,IF($F394=$BR$75,$BW$75,IF($F394=$BR$76,$BW$76,IF($F394=$BR$77,$BW$77,IF($F394=$BR$78,$BW$78,IF($F394=$BR$79,$BW$79,IF($F394=$BR$80,$BW$80,)))))))))))","v":2}]
["14450142",14,450,2,14,5,0,0,0,{"v":0,"d":"0.0"},1042,0,0,0,1.362,1.1,1.1,1.1,156,0,0,0,27,0,0,0,2.7169438657297116,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK395/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL395/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM395/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14450262",14,450,2,26,10,0,0,0,{"v":0,"d":"0.0"},1808,0,0,0,1.362,1.1,1.1,1.1,270,0,0,0,46,0,0,0,3.6815812889765698,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK396/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL396/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM396/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3,"d":"3.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14450342",14,450,2,34,15,0,0,0,{"v":0,"d":"0.0"},2467,0,0,0,1.362,1.1,1.1,1.1,368,0,0,0,63,0,0,0,2.536508378341598,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK397/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL397/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM397/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.5,"d":"4.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14450422",14,450,2,42,20,0,0,0,{"v":0,"d":"0.0"},3325,0,0,0,1.362,1.1,1.1,1.1,496,0,0,0,85,0,0,0,6.283456603446941,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK398/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL398/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM398/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6,"d":"6.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14470142",14,470,2,14,5,0,0,0,{"v":0,"d":"0.0"},1091,0,0,0,1.362,1.1,1.1,1.1,163,0,0,0,28,0,0,0,3.035345802217571,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK399/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL399/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM399/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5666666666666669,"d":"1.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14470262",14,470,2,26,10,0,0,0,{"v":0,"d":"0.0"},1895,0,0,0,1.362,1.1,1.1,1.1,283,0,0,0,49,0,0,0,4.229767077732525,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK400/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL400/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM400/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1333333333333337,"d":"3.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14470342",14,470,2,34,15,0,0,0,{"v":0,"d":"0.0"},2584,0,0,0,1.362,1.1,1.1,1.1,386,0,0,0,66,0,0,0,2.879525891512923,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK401/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL401/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM401/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.7,"d":"4.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14470422",14,470,2,42,20,0,0,0,{"v":0,"d":"0.0"},3483,0,0,0,1.362,1.1,1.1,1.1,520,0,0,0,89,0,0,0,6.998630292975797,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK402/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL402/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM402/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6.2666666666666675,"d":"6.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["14490142",14,490,2,14,5,0,0,0,{"v":0,"d":"0.0"},1141,0,0,0,1.362,1.1,1.1,1.1,170,0,0,0,29,0,0,0,3.3767110021486024,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK403/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL403/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM403/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6333333333333335,"d":"1.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["14490262",14,490,2,26,10,0,0,0,{"v":0,"d":"0.0"},1980,0,0,0,1.362,1.1,1.1,1.1,296,0,0,0,51,0,0,0,4.685842570490673,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK404/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL404/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM404/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.266666666666667,"d":"3.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["14490342",14,490,2,34,15,0,0,0,{"v":0,"d":"0.0"},2702,0,0,0,1.362,1.1,1.1,1.1,403,0,0,0,69,0,0,0,3.250787715185223,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK405/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL405/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM405/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.9,"d":"4.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["14490422",14,490,2,42,20,0,0,0,{"v":0,"d":"0.0"},3642,0,0,0,1.362,1.1,1.1,1.1,544,0,0,0,94,0,0,0,7.873342468625221,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK406/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL406/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM406/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6.533333333333334,"d":"6.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["1970262",19,70,2,26,{"$f":"IF($E407=26,10,IF($E407=34,15,IF($E407=42,20,)))","v":10},0,0,0,{"v":0,"d":"0.0"},196,0,0,0,1.362,1.1,1.1,1.1,29,0,0,0,5,0,0,0,0.017392739210067683,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK407/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL407/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM407/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4666666666666667,"d":"0.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1970342",19,70,2,34,{"$f":"IF($E408=26,10,IF($E408=34,15,IF($E408=42,20,)))","v":15},0,0,0,{"v":0,"d":"0.0"},265,0,0,0,1.362,1.1,1.1,1.1,40,0,0,0,7,0,0,0,0.006846084047172233,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK408/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL408/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM408/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["1970422",19,70,2,42,20,0,0,0,{"v":0,"d":"0.0"},363,0,0,0,1.362,1.1,1.1,1.1,54,0,0,0,9,0,0,0,0.03719146314941046,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK409/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL409/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM409/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9333333333333333,"d":"0.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["1980262",19,80,2,26,10,0,0,0,{"v":0,"d":"0.0"},245,0,0,0,1.362,1.1,1.1,1.1,37,0,0,0,6,0,0,0,0.026901125524058062,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK410/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL410/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM410/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5333333333333333,"d":"0.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1980342",19,80,2,34,15,0,0,0,{"v":0,"d":"0.0"},332,0,0,0,1.362,1.1,1.1,1.1,50,0,0,0,9,0,0,0,0.012551337866990428,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK411/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL411/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM411/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
[{"$f":"CONCATENATE(B412,C412,E412,D412)","v":"1980422"},19,80,2,42,20,0,0,0,{"v":0,"d":"0.0"},455,0,0,0,1.362,1.1,1.1,1.1,68,0,0,0,12,0,0,0,0.0650706691640389,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE412*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH412),0)","v":0},{"$f":"ROUND(AF412*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI412),0)","v":0},{"$f":"ROUND(AG412*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ412),0)","v":0},{"$f":"ROUND(AK412*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL412*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM412*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK412/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL412/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM412/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0666666666666667,"d":"1.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["1990262",19,90,2,26,10,0,0,0,{"v":0,"d":"0.0"},293,0,0,0,1.362,1.1,1.1,1.1,44,0,0,0,8,0,0,0,0.04755225112177548,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK413/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL413/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM413/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6000000000000001,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1990342",19,90,2,34,15,0,0,0,{"v":0,"d":"0.0"},397,0,0,0,1.362,1.1,1.1,1.1,59,0,0,0,10,0,0,0,0.017369035936126105,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK414/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL414/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM414/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["1990422",19,90,2,42,20,0,0,0,{"v":0,"d":"0.0"},546,0,0,0,1.362,1.1,1.1,1.1,81,0,0,0,14,0,0,0,0.09258271909587396,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK415/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL415/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM415/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2000000000000002,"d":"1.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19100262",19,100,2,26,10,0,0,0,{"v":0,"d":"0.0"},342,0,0,0,1.362,1.1,1.1,1.1,51,0,0,0,9,0,0,0,0.06412794591135038,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK416/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL416/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM416/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6666666666666667,"d":"0.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19100342",19,100,2,34,15,0,0,0,{"v":0,"d":"0.0"},463,0,0,0,1.362,1.1,1.1,1.1,69,0,0,0,12,0,0,0,0.027085592467873506,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK417/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL417/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM417/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19100422",19,100,2,42,20,0,0,0,{"v":0,"d":"0.0"},636,0,0,0,1.362,1.1,1.1,1.1,95,0,0,0,16,0,0,0,0.12582499106812614,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK418/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL418/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM418/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3333333333333335,"d":"1.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19110262",19,110,2,26,10,0,0,0,{"v":0,"d":"0.0"},392,0,0,0,1.362,1.1,1.1,1.1,59,0,0,0,10,0,0,0,0.08374449440911218,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK419/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL419/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM419/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7333333333333334,"d":"0.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19110342",19,110,2,34,15,0,0,0,{"v":0,"d":"0.0"},530,0,0,0,1.362,1.1,1.1,1.1,79,0,0,0,14,0,0,0,0.03965103150266958,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK420/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL420/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM420/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19110422",19,110,2,42,20,0,0,0,{"v":0,"d":"0.0"},728,0,0,0,1.362,1.1,1.1,1.1,109,0,0,0,19,0,0,0,0.1778000502722003,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK421/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL421/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM421/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4666666666666668,"d":"1.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19120262",19,120,2,26,10,0,0,0,{"v":0,"d":"0.0"},440,0,0,0,1.362,1.1,1.1,1.1,66,0,0,0,11,0,0,0,0.10656482113166454,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK422/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL422/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM422/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19120342",19,120,2,34,15,0,0,0,{"v":0,"d":"0.0"},596,0,0,0,1.362,1.1,1.1,1.1,89,0,0,0,15,0,0,0,0.049389688000522014,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK423/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL423/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM423/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2,"d":"1.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19120422",19,120,2,42,20,0,0,0,{"v":0,"d":"0.0"},818,0,0,0,1.362,1.1,1.1,1.1,122,0,0,0,21,0,0,0,0.22518975054830898,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK424/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL424/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM424/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6,"d":"1.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19130262",19,130,2,26,10,0,0,0,{"v":0,"d":"0.0"},489,0,0,0,1.362,1.1,1.1,1.1,73,0,0,0,13,0,0,0,0.14954573458542933,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK425/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL425/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM425/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8666666666666667,"d":"0.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19130342",19,130,2,34,15,0,0,0,{"v":0,"d":"0.0"},662,0,0,0,1.362,1.1,1.1,1.1,99,0,0,0,17,0,0,0,0.06736518523692822,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK426/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL426/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM426/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19130422",19,130,2,42,20,0,0,0,{"v":0,"d":"0.0"},909,0,0,0,1.362,1.1,1.1,1.1,136,0,0,0,23,0,0,0,0.2791563101998274,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK427/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL427/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM427/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.7333333333333334,"d":"1.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19150262",19,150,2,26,10,0,0,0,{"v":0,"d":"0.0"},587,0,0,0,1.362,1.1,1.1,1.1,88,0,0,0,15,0,0,0,0.21693660233780984,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK428/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL428/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM428/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19150342",19,150,2,34,15,0,0,0,{"v":0,"d":"0.0"},795,0,0,0,1.362,1.1,1.1,1.1,119,0,0,0,20,0,0,0,0.10507034434108192,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK429/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL429/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM429/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19150422",19,150,2,42,20,0,0,0,{"v":0,"d":"0.0"},1091,0,0,0,1.362,1.1,1.1,1.1,163,0,0,0,28,0,0,0,0.42857409964559595,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK430/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL430/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM430/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2,"d":"2.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19170262",19,170,2,26,10,0,0,0,{"v":0,"d":"0.0"},685,0,0,0,1.362,1.1,1.1,1.1,102,0,0,0,18,0,0,0,0.32639589242166417,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK431/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL431/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM431/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1333333333333333,"d":"1.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19170342",19,170,2,34,15,0,0,0,{"v":0,"d":"0.0"},927,0,0,0,1.362,1.1,1.1,1.1,138,0,0,0,24,0,0,0,0.16612826056027313,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK432/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL432/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM432/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.7,"d":"1.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19170422",19,170,2,42,20,0,0,0,{"v":0,"d":"0.0"},1273,0,0,0,1.362,1.1,1.1,1.1,190,0,0,0,33,0,0,0,0.615728529230743,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK433/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL433/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM433/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.2666666666666666,"d":"2.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19190262",19,190,2,26,10,0,0,0,{"v":0,"d":"0.0"},782,0,0,0,1.362,1.1,1.1,1.1,117,0,0,0,20,0,0,0,0.4307176078722401,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK434/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL434/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM434/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2666666666666668,"d":"1.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19190342",19,190,2,34,15,0,0,0,{"v":0,"d":"0.0"},1059,0,0,0,1.362,1.1,1.1,1.1,158,0,0,0,27,0,0,0,0.2305305631476093,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK435/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL435/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM435/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.9000000000000001,"d":"1.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19190422",19,190,2,42,20,0,0,0,{"v":0,"d":"0.0"},1455,0,0,0,1.362,1.1,1.1,1.1,217,0,0,0,37,0,0,0,0.8124894051015719,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK436/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL436/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM436/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.5333333333333337,"d":"2.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19210262",19,210,2,26,10,0,0,0,{"v":0,"d":"0.0"},881,0,0,0,1.362,1.1,1.1,1.1,131,0,0,0,23,0,0,{"$f":"ROUND(V437*3600/(4186*ABS($M$1-$M$2)),0)","v":0},0.5905204565764357,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK437/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL437/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM437/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4000000000000001,"d":"1.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19210342",19,210,2,34,15,0,0,0,{"v":0,"d":"0.0"},1192,0,0,0,1.362,1.1,1.1,1.1,178,0,0,0,{"$f":"ROUND(S438*3600/(4186*ABS($M$1-$M$2)),0)","v":31},{"$f":"ROUND(T438*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U438*3600/(4186*ABS($M$1-$M$2)),0)","v":0},0,0.32742995333601566,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK438/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL438/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM438/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.1,"d":"2.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19210422",19,210,2,42,20,0,0,0,{"v":0,"d":"0.0"},1637,0,0,0,1.362,1.1,1.1,1.1,244,0,0,0,42,0,0,0,1.0763834623425705,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK439/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL439/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM439/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8000000000000003,"d":"2.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19230262",19,230,2,26,10,0,0,0,{"v":0,"d":"0.0"},978,0,0,0,1.362,1.1,1.1,1.1,146,0,0,0,25,0,0,0,0.7366849535864659,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK440/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL440/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM440/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5333333333333334,"d":"1.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19230342",19,230,2,34,15,0,0,0,{"v":0,"d":"0.0"},1324,0,0,0,1.362,1.1,1.1,1.1,198,0,0,0,34,0,0,0,0.42447878721481413,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK441/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL441/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM441/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.3000000000000003,"d":"2.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19230422",19,230,2,42,20,0,0,0,{"v":0,"d":"0.0"},1819,0,0,0,1.362,1.1,1.1,1.1,272,0,0,0,47,0,0,0,{"$f":"0.0098*(($BM442*(W442^$BO442)*($C442-14.4)*$BP442)+($BN442*W442*W442))","v":1.3837878135401982},0,{"$f":"0.0098*(($BM442*(Y442^$BO442)*($C442-14.4)*$BP442)+($BN442*Y442*Y442))","v":0},{"$f":"0.0098*(($BM442*(Z442^$BO442)*($C442-14.4)*$BP442)+($BN442*Z442*Z442))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK442/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL442/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM442/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.066666666666667,"d":"3.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19250262",19,250,2,26,10,0,0,0,{"v":0,"d":"0.0"},1076,0,0,0,1.362,1.1,1.1,1.1,161,0,0,0,28,0,0,0,0.9526843891537767,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK443/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL443/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM443/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6666666666666667,"d":"1.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19250342",19,250,2,34,15,0,0,0,{"v":0,"d":"0.0"},1457,0,0,0,1.362,1.1,1.1,1.1,217,0,0,0,37,0,0,0,0.53815379468308,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK444/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL444/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM444/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.5,"d":"2.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19250422",19,250,2,42,20,0,0,0,{"v":0,"d":"0.0"},2001,0,0,0,1.362,1.1,1.1,1.1,299,0,0,0,51,0,0,0,1.6907613133214068,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK445/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL445/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM445/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.3333333333333335,"d":"3.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19270262",19,270,2,26,10,0,0,0,{"v":0,"d":"0.0"},1174,0,0,0,1.362,1.1,1.1,1.1,175,0,0,0,30,0,0,0,1.1450566861245886,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK446/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL446/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM446/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.8,"d":"1.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19270342",19,270,2,34,15,0,0,0,{"v":0,"d":"0.0"},1590,0,0,0,1.362,1.1,1.1,1.1,237,0,0,0,41,0,0,0,0.6994777632096597,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK447/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL447/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM447/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.7,"d":"2.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19270422",19,270,2,42,20,0,0,0,{"v":0,"d":"0.0"},2182,0,0,0,1.362,1.1,1.1,1.1,326,0,0,0,56,0,0,0,2.0846494613185826,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK448/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL448/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM448/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.6,"d":"3.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19290262",19,290,2,26,10,0,0,0,{"v":0,"d":"0.0"},1271,0,0,0,1.362,1.1,1.1,1.1,190,0,0,0,33,0,0,0,1.422521205199001,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK449/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL449/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM449/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.9333333333333333,"d":"1.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19290342",19,290,2,34,15,0,0,0,{"v":0,"d":"0.0"},1721,0,0,0,1.362,1.1,1.1,1.1,257,0,0,0,44,0,0,0,0.8538981947959675,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK450/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL450/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM450/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.9,"d":"2.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19290422",19,290,2,42,20,0,0,0,{"v":0,"d":"0.0"},2365,0,0,0,1.362,1.1,1.1,1.1,353,0,0,0,61,0,0,0,2.5267400452041255,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK451/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL451/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM451/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.8666666666666667,"d":"3.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19310262",19,310,2,26,10,0,0,0,{"v":0,"d":"0.0"},1370,0,0,0,1.362,1.1,1.1,1.1,204,0,0,0,35,0,0,0,1.6650679425361228,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK452/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL452/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM452/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.066666666666667,"d":"2.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19310342",19,310,2,34,15,0,0,0,{"v":0,"d":"0.0"},1854,0,0,0,1.362,1.1,1.1,1.1,277,0,0,0,48,0,0,0,1.0675147867651602,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK453/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL453/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM453/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1,"d":"3.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19310422",19,310,2,42,20,0,0,0,{"v":0,"d":"0.0"},2547,0,0,0,1.362,1.1,1.1,1.1,380,0,0,0,65,0,0,0,2.955912466895074,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK454/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL454/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM454/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.133333333333334,"d":"4.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19330262",19,330,2,26,10,0,0,0,{"v":0,"d":"0.0"},1467,0,0,0,1.362,1.1,1.1,1.1,219,0,0,0,38,0,0,0,2.008826410265957,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK455/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL455/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM455/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.2,"d":"2.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19330342",19,330,2,34,15,0,0,0,{"v":0,"d":"0.0"},1987,0,0,0,1.362,1.1,1.1,1.1,297,0,0,0,51,0,0,0,1.267973011621372,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK456/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL456/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM456/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.3000000000000003,"d":"3.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19330422",19,330,2,42,20,0,0,0,{"v":0,"d":"0.0"},2728,0,0,0,1.362,1.1,1.1,1.1,407,0,0,0,70,0,0,0,3.4926379534901506,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK457/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL457/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM457/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F457=$BR$70,$C457*$BS$70,IF($F457=$BR$71,$C457*$BS$71,IF($F457=$BR$72,$C457*$BS$72,IF($F457=$BR$73,$C457*$BS$73,IF($F457=$BR$74,$C457*$BS$74,IF($F457=$BR$75,$C457*$BS$75,IF($F457=$BR$76,$C457*$BS$76,IF($F457=$BR$77,$C457*$BS$77,IF($F457=$BR$78,$C457*$BS$78,IF($F457=$BR$79,$C457*$BS$79,IF($F457=$BR$80,$C457*$BS$80,)))))))))))","v":{"v":4.4,"d":"4.40"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19350262",19,350,2,26,10,0,0,0,{"v":0,"d":"0.0"},1565,0,0,0,1.362,1.1,1.1,1.1,234,0,0,0,40,0,0,0,2.3052073098114154,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK458/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL458/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM458/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM458*(AN458^$BO458)*($C458-14.4)*$BP458)+($BN458*AN458*AN458))","v":0},0,0,{"v":2.3333333333333335,"d":"2.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F458=$BR$70,$BT$70,IF($F458=$BR$71,$BT$71,IF($F458=$BR$72,$BT$72,IF($F458=$BR$73,$BT$73,IF($F458=$BR$74,$BT$74,IF($F458=$BR$75,$BT$75,IF($F458=$BR$76,$BT$76,IF($F458=$BR$77,$BT$77,IF($F458=$BR$78,$BT$78,IF($F458=$BR$79,$BT$79,IF($F458=$BR$80,$BT$80,)))))))))))","v":0.0014501879713726},{"$f":"IF($F458=$BR$70,$BU$70,IF($F458=$BR$71,$BU$71,IF($F458=$BR$72,$BU$72,IF($F458=$BR$73,$BU$73,IF($F458=$BR$74,$BU$74,IF($F458=$BR$75,$BU$75,IF($F458=$BR$76,$BU$76,IF($F458=$BR$77,$BU$77,IF($F458=$BR$78,$BU$78,IF($F458=$BR$79,$BU$79,IF($F458=$BR$80,$BU$80,)))))))))))","v":0.00037831632653061},{"$f":"IF($F458=$BR$70,$BV$70,IF($F458=$BR$71,$BV$71,IF($F458=$BR$72,$BV$72,IF($F458=$BR$73,$BV$73,IF($F458=$BR$74,$BV$74,IF($F458=$BR$75,$BV$75,IF($F458=$BR$76,$BV$76,IF($F458=$BR$77,$BV$77,IF($F458=$BR$78,$BV$78,IF($F458=$BR$79,$BV$79,IF($F458=$BR$80,$BV$80,)))))))))))","v":1.4868910444209},{"$f":"IF($F458=$BR$70,$BW$70,IF($F458=$BR$71,$BW$71,IF($F458=$BR$72,$BW$72,IF($F458=$BR$73,$BW$73,IF($F458=$BR$74,$BW$74,IF($F458=$BR$75,$BW$75,IF($F458=$BR$76,$BW$76,IF($F458=$BR$77,$BW$77,IF($F458=$BR$78,$BW$78,IF($F458=$BR$79,$BW$79,IF($F458=$BR$80,$BW$80,)))))))))))","v":2}]
["19350342",19,350,2,34,15,0,0,0,{"v":0,"d":"0.0"},2119,0,0,0,1.362,1.1,1.1,1.1,316,0,0,0,54,0,0,0,1.4909445593996062,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK459/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL459/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM459/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.5,"d":"3.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19350422",19,350,2,42,20,0,0,0,{"v":0,"d":"0.0"},2910,0,0,0,1.362,1.1,1.1,1.1,434,0,0,0,75,0,0,0,4.081582798403194,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK460/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL460/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM460/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.666666666666667,"d":"4.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19370262",19,370,2,26,10,0,0,0,{"v":0,"d":"0.0"},1663,0,0,0,1.362,1.1,1.1,1.1,248,0,0,0,43,0,0,0,2.719742390419653,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK461/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL461/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM461/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.466666666666667,"d":"2.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19370342",19,370,2,34,15,0,0,0,{"v":0,"d":"0.0"},2252,0,0,0,1.362,1.1,1.1,1.1,336,0,0,0,58,0,0,0,1.7917267510891295,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK462/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL462/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM462/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.7,"d":"3.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19370422",19,370,2,42,20,0,0,0,{"v":0,"d":"0.0"},3092,0,0,0,1.362,1.1,1.1,1.1,462,0,0,0,79,0,0,0,4.643197622107749,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK463/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL463/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM463/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.933333333333334,"d":"4.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19390262",19,390,2,26,10,0,0,0,{"v":0,"d":"0.0"},1760,0,0,0,1.362,1.1,1.1,1.1,263,0,0,0,45,0,0,0,3.0733713264696716,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK464/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL464/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM464/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.6,"d":"2.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19390342",19,390,2,34,15,0,0,0,{"v":0,"d":"0.0"},2384,0,0,0,1.362,1.1,1.1,1.1,356,0,0,0,61,0,0,0,2.0681123840696243,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK465/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL465/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM465/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.9,"d":"3.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19390422",19,390,2,42,20,0,0,0,{"v":0,"d":"0.0"},3274,0,0,0,1.362,1.1,1.1,1.1,489,0,0,0,84,0,0,0,5.333873465499114,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK466/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL466/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM466/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":5.2,"d":"5.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19410262",19,410,2,26,10,0,0,0,{"v":0,"d":"0.0"},1859,0,0,0,1.362,1.1,1.1,1.1,277,0,0,0,48,0,0,0,3.562883906013579,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK467/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL467/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM467/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.7333333333333334,"d":"2.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19410342",19,410,2,34,15,0,0,0,{"v":0,"d":"0.0"},2516,0,0,0,1.362,1.1,1.1,1.1,376,0,0,0,65,0,0,0,2.4361581489357453,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK468/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL468/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM468/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.1,"d":"4.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19410422",19,410,2,42,20,0,0,0,{"v":0,"d":"0.0"},3456,0,0,0,1.362,1.1,1.1,1.1,516,0,0,0,89,0,0,0,6.080315742504732,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK469/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL469/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM469/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":5.466666666666667,"d":"5.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19430262",19,430,2,26,10,0,0,0,{"v":0,"d":"0.0"},1956,0,0,0,1.362,1.1,1.1,1.1,292,0,0,0,50,0,0,0,3.9769720891030724,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK470/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL470/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM470/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8666666666666667,"d":"2.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19430342",19,430,2,34,15,0,0,0,{"v":0,"d":"0.0"},2649,0,0,0,1.362,1.1,1.1,1.1,395,0,0,0,68,0,0,0,2.7708558786877235,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK471/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL471/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM471/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.3,"d":"4.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19430422",19,430,2,42,{"$f":"IF($E472=26,10,IF($E472=34,15,IF($E472=42,20,)))","v":20},0,0,0,{"v":0,"d":"0.0"},3638,0,0,0,1.362,1.1,1.1,1.1,543,0,0,0,93,0,0,0,6.783409696775025,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK472/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL472/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM472/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":5.733333333333333,"d":"5.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19450262",19,450,2,26,10,0,0,0,{"v":0,"d":"0.0"},2054,0,0,0,1.362,1.1,1.1,1.1,307,0,0,0,53,0,0,0,4.545427923638345,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK473/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL473/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM473/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3,"d":"3.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19450342",19,450,2,34,15,0,0,0,{"v":0,"d":"0.0"},2781,0,0,0,1.362,1.1,1.1,1.1,415,0,0,0,71,0,0,0,3.1335113847214515,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK474/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL474/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM474/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.5,"d":"4.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19450422",19,450,2,42,20,0,0,0,{"v":0,"d":"0.0"},3820,0,0,0,1.362,1.1,1.1,1.1,570,0,0,0,98,0,0,0,7.637918220607638,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK475/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL475/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM475/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6,"d":"6.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19470262",19,470,2,26,10,0,0,0,{"v":0,"d":"0.0"},2152,0,0,0,1.362,1.1,1.1,1.1,321,0,0,0,55,0,0,0,5.023015771024925,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE476*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH476),0)","v":0},{"$f":"ROUND(AF476*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI476),0)","v":0},{"$f":"ROUND(AG476*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ476),0)","v":0},{"$f":"ROUND(AK476*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL476*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM476*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK476/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL476/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM476/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1333333333333337,"d":"3.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19470342",19,470,2,34,15,0,0,0,{"v":0,"d":"0.0"},2914,0,0,0,1.362,1.1,1.1,1.1,435,0,0,0,75,0,0,0,3.6097516026799545,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK477/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL477/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM477/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.7,"d":"4.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19470422",19,470,2,42,20,0,0,0,{"v":0,"d":"0.0"},4001,0,0,0,1.362,1.1,1.1,1.1,597,0,0,0,103,0,0,0,8.55139060673361,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK478/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL478/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM478/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6.2666666666666675,"d":"6.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["19490262",19,490,2,26,10,0,0,0,{"v":0,"d":"0.0"},2250,0,0,0,1.362,1.1,1.1,1.1,336,0,0,0,58,0,0,0,5.6741805499403934,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK479/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL479/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM479/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.266666666666667,"d":"3.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["19490342",19,490,2,34,15,0,0,0,{"v":0,"d":"0.0"},3046,0,0,0,1.362,1.1,1.1,1.1,455,0,0,0,78,0,0,0,4.0376213351218855,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK480/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL480/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM480/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.9,"d":"4.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["19490422",19,490,2,42,20,0,0,0,{"v":0,"d":"0.0"},4184,0,0,0,1.362,1.1,1.1,1.1,625,0,0,0,108,0,0,0,9.524867809879517,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK481/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL481/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM481/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6.533333333333334,"d":"6.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
[{"$f":"CONCATENATE(B482,C482,E482,D482)","v":"970143"},9,70,3,14,{"$f":"IF($E482=14,4,IF($E482=18,9,IF($E482=23,9,IF($E482=30,14,IF($E482=38,19,)))))","v":4},0,0,0,{"v":0,"d":"0.0"},84,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K482*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O482),0)","v":13},{"$f":"ROUND(L482*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P482),0)","v":0},{"$f":"ROUND(M482*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q482),0)","v":0},{"$f":"ROUND(N482*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R482),0)","v":0},{"$f":"ROUND(S482*3600/(4186*ABS($M$1-$M$2)),0)","v":2},{"$f":"ROUND(T482*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U482*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V482*3600/(4186*ABS($M$1-$M$2)),0)","v":0},2.4998470803170997E-3,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE482*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH482),0)","v":0},{"$f":"ROUND(AF482*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI482),0)","v":0},{"$f":"ROUND(AG482*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ482),0)","v":0},{"$f":"ROUND(AK482*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL482*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM482*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK482/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL482/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM482/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.11666666666666667,"d":"0.12"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["970183",9,70,3,18,{"$f":"IF($E483=14,4,IF($E483=18,9,IF($E483=23,9,IF($E483=30,14,IF($E483=38,19,)))))","v":9},0,0,0,{"v":0,"d":"0.0"},109.2,0,0,0,1.362,1.1,1.1,1.1,16,0,0,0,3,0,0,0,6.4730267114827406E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK483/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL483/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM483/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.23333333333333334,"d":"0.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["970233",9,70,3,23,9,0,0,0,{"v":0,"d":"0.0"},132.4,0,0,0,1.362,1.1,1.1,1.1,20,0,0,0,3,0,0,0,6.4730267114827406E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK484/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL484/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM484/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.23333333333333334,"d":"0.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["970303",9,70,3,30,14,0,0,0,{"v":0,"d":"0.0"},174.4,0,0,0,1.362,1.1,1.1,1.1,26,0,0,0,4,0,0,0,0.033277998999107175,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK485/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL485/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM485/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.35000000000000003,"d":"0.35"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["970383",9,70,3,38,19,0,0,0,{"v":0,"d":"0.0"},229.60000000000002,0,0,0,1.362,1.1,1.1,1.1,34,0,0,0,6,0,0,0,0.10928752307846887,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK486/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL486/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM486/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4666666666666667,"d":"0.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["980143",9,80,3,14,4,0,0,0,{"v":0,"d":"0.0"},105,0,0,0,1.362,1.1,1.1,1.1,16,0,0,0,3,0,0,0,0.005930081911941236,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK487/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL487/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM487/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.13333333333333333,"d":"0.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["980183",9,80,3,18,9,0,0,0,{"v":0,"d":"0.0"},136.5,0,0,0,1.362,1.1,1.1,1.1,20,0,0,0,3,0,0,0,7.630927336835948E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK488/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL488/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM488/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.26666666666666666,"d":"0.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["980233",9,80,3,23,9,0,0,0,{"v":0,"d":"0.0"},165.5,0,0,0,1.362,1.1,1.1,1.1,25,0,0,0,4,0,0,0,0.012862019153558217,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK489/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL489/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM489/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.26666666666666666,"d":"0.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["980303",9,80,3,30,14,0,0,0,{"v":0,"d":"0.0"},218,0,0,0,1.362,1.1,1.1,1.1,33,0,0,0,6,0,0,0,0.07197165215334056,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK490/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL490/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM490/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["980383",9,80,3,38,19,0,0,0,{"v":0,"d":"0.0"},287,0,0,0,1.362,1.1,1.1,1.1,43,0,0,0,7,0,0,0,0.16459449411510485,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK491/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL491/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM491/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5333333333333333,"d":"0.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["990143",9,90,3,14,4,0,0,0,{"v":0,"d":"0.0"},126,0,0,0,1.362,1.1,1.1,1.1,19,0,0,0,3,0,0,0,0.006829581822298132,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK492/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL492/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM492/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.15000000000000002,"d":"0.15"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["990183",9,90,3,18,9,0,0,0,{"v":0,"d":"0.0"},163.79999999999998,0,0,0,1.362,1.1,1.1,1.1,24,0,0,0,4,0,0,0,0.014813180817340765,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK493/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL493/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM493/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.30000000000000004,"d":"0.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["990233",9,90,3,23,9,0,0,0,{"v":0,"d":"0.0"},198.6,0,0,0,1.362,1.1,1.1,1.1,30,0,0,0,5,0,0,0,0.02220790314848095,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK494/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL494/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM494/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.30000000000000004,"d":"0.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["990303",9,90,3,30,14,0,0,0,{"v":0,"d":"0.0"},261.59999999999997,0,0,0,1.362,1.1,1.1,1.1,39,0,0,0,7,0,0,0,0.10441004558847257,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK495/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL495/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM495/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["990383",9,90,3,38,19,0,0,0,{"v":0,"d":"0.0"},344.4,0,0,0,1.362,1.1,1.1,1.1,51,0,0,0,9,0,0,0,0.2825921202379186,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK496/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL496/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM496/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6000000000000001,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9100143",9,100,3,14,4,0,0,0,{"v":0,"d":"0.0"},147,0,0,0,1.362,1.1,1.1,1.1,22,0,0,0,{"$f":"ROUND(S497*3600/(4186*ABS($M$1-$M$2)),0)","v":4},{"$f":"ROUND(T497*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U497*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V497*3600/(4186*ABS($M$1-$M$2)),0)","v":0},0.012692746488264683,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK497/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL497/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM497/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.16666666666666669,"d":"0.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
[{"$f":"CONCATENATE(B498,C498,E498,D498)","v":"9100183"},9,100,3,18,9,0,0,0,{"v":0,"d":"0.0"},191.1,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K498*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O498),0)","v":29},{"$f":"ROUND(L498*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P498),0)","v":0},0,0,{"$f":"ROUND(S498*3600/(4186*ABS($M$1-$M$2)),0)","v":5},0,0,0,0.0251325599308642,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK498/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL498/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM498/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.33333333333333337,"d":"0.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9100233",9,100,3,23,9,0,0,0,{"v":0,"d":"0.0"},231.7,0,0,0,1.362,1.1,1.1,1.1,35,0,0,0,6,0,0,0,0.034987986312321834,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK499/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL499/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM499/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.33333333333333337,"d":"0.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9100303",9,100,3,30,14,0,0,0,{"v":0,"d":"0.0"},305.2,0,0,0,1.362,1.1,1.1,1.1,46,0,0,0,8,0,0,0,0.1443073062485503,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK500/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL500/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM500/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9100383",9,100,3,38,19,0,0,0,{"v":0,"d":"0.0"},401.79999999999995,0,0,0,1.362,1.1,1.1,1.1,60,0,0,0,10,0,0,0,0.37806768715965605,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK501/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL501/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM501/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6666666666666667,"d":"0.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9110143",9,110,3,14,4,0,0,0,{"v":0,"d":"0.0"},168,0,0,0,1.362,1.1,1.1,1.1,25,0,0,0,4,0,0,0,0.014169445844370371,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK502/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL502/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM502/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.18333333333333335,"d":"0.18"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9110183",9,110,3,18,9,0,0,0,{"v":0,"d":"0.0"},218.4,0,0,0,1.362,1.1,1.1,1.1,33,0,0,0,6,0,0,0,0.03905896637940668,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE503*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH503),0)","v":0},{"$f":"ROUND(AF503*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI503),0)","v":0},0,0,0,0,{"$f":"(AK503/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL503/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM503/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3666666666666667,"d":"0.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9110233",9,110,3,23,9,0,0,0,{"v":0,"d":"0.0"},264.8,0,0,0,1.362,1.1,1.1,1.1,40,0,0,0,7,0,0,0,0.051665258153112514,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE504*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH504),0)","v":0},0,0,0,0,0,{"$f":"(AK504/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL504/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM504/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3666666666666667,"d":"0.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9110303",9,110,3,30,14,0,0,0,{"v":0,"d":"0.0"},348.8,0,0,0,1.362,1.1,1.1,1.1,52,0,0,0,9,0,0,0,0.19215679122977283,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK505/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL505/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM505/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.55,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9110383",9,110,3,38,19,0,0,0,{"v":0,"d":"0.0"},459.20000000000005,0,0,0,1.362,1.1,1.1,1.1,69,0,0,0,12,0,0,0,{"$f":"0.0098*(($BM506*(W506^$BO506)*($C506-14.4)*$BP506)+($BN506*W506*W506))","v":0.5638255305739398},0,{"$f":"0.0098*(($BM506*(Y506^$BO506)*($C506-14.4)*$BP506)+($BN506*Y506*Y506))","v":0},{"$f":"0.0098*(($BM506*(Z506^$BO506)*($C506-14.4)*$BP506)+($BN506*Z506*Z506))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK506/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL506/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM506/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7333333333333334,"d":"0.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9120143",9,120,3,14,4,0,0,0,{"v":0,"d":"0.0"},189,0,0,0,1.362,1.1,1.1,1.1,28,0,0,0,5,0,0,0,0.022987530345093,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK507/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL507/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM507/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.2,"d":"0.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9120183",9,120,3,18,9,0,0,0,{"v":0,"d":"0.0"},245.70000000000002,0,0,0,1.362,1.1,1.1,1.1,37,0,0,0,6,0,0,0,0.04312994644649151,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK508/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL508/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM508/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9120233",9,120,3,23,9,0,0,0,{"v":0,"d":"0.0"},297.90000000000003,0,0,0,1.362,1.1,1.1,1.1,44,0,0,0,8,0,0,0,0.07269066515235312,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK509/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL509/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM509/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9120303",9,120,3,30,14,0,0,0,{"v":0,"d":"0.0"},392.40000000000003,0,0,0,1.362,1.1,1.1,1.1,59,0,0,0,10,0,0,0,0.248422273464841,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK510/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL510/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM510/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9120383",9,120,3,38,19,0,0,0,{"v":0,"d":"0.0"},516.6,0,0,0,1.362,1.1,1.1,1.1,77,0,0,0,13,0,0,0,0.7069688951569888,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK511/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL511/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM511/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9130143",9,130,3,14,4,0,0,0,{"v":0,"d":"0.0"},210,0,0,0,1.362,1.1,1.1,1.1,31,0,0,0,5,0,0,0,0.02515665608799953,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,{"$f":"ROUND(AK512*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},0,0,{"$f":"(AK512/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL512/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM512/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.21666666666666667,"d":"0.22"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9130183",9,130,3,18,9,0,0,0,{"v":0,"d":"0.0"},273,0,0,0,1.362,1.1,1.1,1.1,41,0,0,0,7,0,0,0,0.06243391135828655,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK513/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL513/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM513/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.43333333333333335,"d":"0.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9130233",9,130,3,23,9,0,0,0,{"v":0,"d":"0.0"},331,0,0,0,1.362,1.1,1.1,1.1,49,0,0,0,8,0,0,0,0.0795506150193772,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE514*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH514),0)","v":0},0,0,0,0,0,{"$f":"(AK514/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL514/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM514/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.43333333333333335,"d":"0.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9130303",9,130,3,30,14,0,0,0,{"v":0,"d":"0.0"},436,0,0,0,1.362,1.1,1.1,1.1,65,0,0,0,11,0,0,0,0.3135426761390496,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK515/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL515/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM515/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.65,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9130383",9,130,3,38,19,0,0,0,{"v":0,"d":"0.0"},574,0,0,0,1.362,1.1,1.1,1.1,86,0,0,0,15,0,0,0,0.971106542736653,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK516/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL516/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM516/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8666666666666667,"d":"0.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9150143",9,150,3,14,4,0,0,0,{"v":0,"d":"0.0"},252,0,0,0,1.362,1.1,1.1,1.1,38,0,0,0,7,0,0,0,0.05268270126173568,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK517/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL517/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM517/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9150183",9,150,3,18,9,0,0,0,{"v":0,"d":"0.0"},327.59999999999997,0,0,0,1.362,1.1,1.1,1.1,49,0,0,0,8,0,0,0,0.09327051475342535,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK518/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL518/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM518/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9150233",9,150,3,23,9,0,0,0,{"v":0,"d":"0.0"},397.2,0,0,0,1.362,1.1,1.1,1.1,59,0,0,0,10,0,0,0,0.13982193617002808,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK519/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL519/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM519/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9150303",9,150,3,30,14,0,0,0,{"v":0,"d":"0.0"},523.1999999999999,0,0,0,1.362,1.1,1.1,1.1,78,0,0,0,13,0,0,0,0.472000450598339,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK520/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL520/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM520/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9150383",9,150,3,38,19,0,0,0,{"v":0,"d":"0.0"},688.8,0,0,0,1.362,1.1,1.1,1.1,103,0,0,0,18,0,0,0,1.5208706253837831,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK521/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL521/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM521/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F521=$BR$70,$C521*$BS$70,IF($F521=$BR$71,$C521*$BS$71,IF($F521=$BR$72,$C521*$BS$72,IF($F521=$BR$73,$C521*$BS$73,IF($F521=$BR$74,$C521*$BS$74,IF($F521=$BR$75,$C521*$BS$75,IF($F521=$BR$76,$C521*$BS$76,IF($F521=$BR$77,$C521*$BS$77,IF($F521=$BR$78,$C521*$BS$78,IF($F521=$BR$79,$C521*$BS$79,IF($F521=$BR$80,$C521*$BS$80,)))))))))))","v":{"v":1,"d":"1.00"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9170143",9,170,3,14,4,0,0,0,{"v":0,"d":"0.0"},294,0,0,0,1.362,1.1,1.1,1.1,44,0,0,0,8,0,0,0,0.07607148445486532,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK522/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL522/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM522/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM522*(AN522^$BO522)*($C522-14.4)*$BP522)+($BN522*AN522*AN522))","v":0},0,0,{"v":0.2833333333333333,"d":"0.28"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F522=$BR$70,$BT$70,IF($F522=$BR$71,$BT$71,IF($F522=$BR$72,$BT$72,IF($F522=$BR$73,$BT$73,IF($F522=$BR$74,$BT$74,IF($F522=$BR$75,$BT$75,IF($F522=$BR$76,$BT$76,IF($F522=$BR$77,$BT$77,IF($F522=$BR$78,$BT$78,IF($F522=$BR$79,$BT$79,IF($F522=$BR$80,$BT$80,)))))))))))","v":1.3823338826853E-3},{"$f":"IF($F522=$BR$70,$BU$70,IF($F522=$BR$71,$BU$71,IF($F522=$BR$72,$BU$72,IF($F522=$BR$73,$BU$73,IF($F522=$BR$74,$BU$74,IF($F522=$BR$75,$BU$75,IF($F522=$BR$76,$BU$76,IF($F522=$BR$77,$BU$77,IF($F522=$BR$78,$BU$78,IF($F522=$BR$79,$BU$79,IF($F522=$BR$80,$BU$80,)))))))))))","v":0.00033290816326531},{"$f":"IF($F522=$BR$70,$BV$70,IF($F522=$BR$71,$BV$71,IF($F522=$BR$72,$BV$72,IF($F522=$BR$73,$BV$73,IF($F522=$BR$74,$BV$74,IF($F522=$BR$75,$BV$75,IF($F522=$BR$76,$BV$76,IF($F522=$BR$77,$BV$77,IF($F522=$BR$78,$BV$78,IF($F522=$BR$79,$BV$79,IF($F522=$BR$80,$BV$80,)))))))))))","v":1.723172227894},{"$f":"IF($F522=$BR$70,$BW$70,IF($F522=$BR$71,$BW$71,IF($F522=$BR$72,$BW$72,IF($F522=$BR$73,$BW$73,IF($F522=$BR$74,$BW$74,IF($F522=$BR$75,$BW$75,IF($F522=$BR$76,$BW$76,IF($F522=$BR$77,$BW$77,IF($F522=$BR$78,$BW$78,IF($F522=$BR$79,$BW$79,IF($F522=$BR$80,$BW$80,)))))))))))","v":1}]
["9170183",9,170,3,18,9,0,0,0,{"v":0,"d":"0.0"},382.2,0,0,0,1.362,1.1,1.1,1.1,57,0,0,0,10,0,0,0,0.16038711975046666,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK523/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL523/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM523/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5666666666666667,"d":"0.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9170233",9,170,3,23,9,0,0,0,{"v":0,"d":"0.0"},463.4,0,0,0,1.362,1.1,1.1,1.1,69,0,0,0,12,0,0,0,0.22326981247242142,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK524/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL524/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM524/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5666666666666667,"d":"0.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9170303",9,170,3,30,14,0,0,0,{"v":0,"d":"0.0"},610.4,0,0,0,1.362,1.1,1.1,1.1,91,0,0,0,16,0,0,0,0.7386072270235654,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK525/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL525/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM525/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.85,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9170383",9,170,3,38,19,0,0,0,{"v":0,"d":"0.0"},803.5999999999999,0,0,0,1.362,1.1,1.1,1.1,120,0,0,0,21,0,0,0,2.228309036409947,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK526/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL526/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM526/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1333333333333333,"d":"1.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9190143",9,190,3,14,4,0,0,0,{"v":0,"d":"0.0"},336,0,0,0,1.362,1.1,1.1,1.1,50,0,0,0,9,0,0,0,0.10514306777227453,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK527/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL527/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM527/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3166666666666667,"d":"0.32"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9190183",9,190,3,18,9,0,0,0,{"v":0,"d":"0.0"},436.8,0,0,0,1.362,1.1,1.1,1.1,65,0,0,0,11,0,0,0,0.21511049502262594,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK528/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL528/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM528/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6333333333333334,"d":"0.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9190233",9,190,3,23,9,0,0,0,{"v":0,"d":"0.0"},529.6,0,0,0,1.362,1.1,1.1,1.1,79,0,0,0,14,0,0,0,0.33318166555581685,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK529/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL529/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM529/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6333333333333334,"d":"0.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9190303",9,190,3,30,14,0,0,0,{"v":0,"d":"0.0"},697.6,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K530*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O530),0)","v":104},0,0,0,18,0,0,0,0.9938368379351072,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK530/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL530/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM530/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9500000000000001,"d":"0.95"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9190383",9,190,3,38,19,0,0,0,{"v":0,"d":"0.0"},918.4000000000001,0,0,0,1.362,1.1,1.1,1.1,137,0,0,0,24,0,0,0,3.1076422699087214,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK531/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL531/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM531/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2666666666666668,"d":"1.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9210143",9,210,3,14,4,0,0,0,{"v":0,"d":"0.0"},378,0,0,0,1.362,1.1,1.1,1.1,56,0,0,0,10,0,0,0,0.14040753186853402,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK532/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL532/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM532/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.35000000000000003,"d":"0.35"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9210183",9,210,3,18,9,0,0,0,{"v":0,"d":"0.0"},491.40000000000003,0,0,0,1.362,1.1,1.1,1.1,73,0,0,0,13,0,0,0,0.3243639843854712,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK533/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL533/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM533/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9210233",9,210,3,23,9,0,0,0,{"v":0,"d":"0.0"},595.8000000000001,0,0,0,1.362,1.1,1.1,1.1,89,0,0,0,15,0,0,0,0.4205177597708368,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK534/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL534/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM534/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9210303",9,210,3,30,14,0,0,0,{"v":0,"d":"0.0"},784.8000000000001,0,0,0,1.362,1.1,1.1,1.1,117,0,0,0,20,0,0,0,1.295663723585732,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK535/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL535/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM535/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.05,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9210383",9,210,3,38,19,0,0,0,{"v":0,"d":"0.0"},1033.2,0,0,0,1.362,1.1,1.1,1.1,154,0,0,0,26,0,0,0,3.929582658734965,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK536/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL536/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM536/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4000000000000001,"d":"1.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9230143",9,230,3,14,4,0,0,0,{"v":0,"d":"0.0"},420,0,0,0,1.362,1.1,1.1,1.1,63,0,0,0,11,0,0,0,0.18235929199879208,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK537/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL537/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM537/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.38333333333333336,"d":"0.38"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9230183",9,230,3,18,9,0,0,0,{"v":0,"d":"0.0"},546,0,0,0,1.362,1.1,1.1,1.1,81,0,0,0,14,0,0,0,0.40890314214494994,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK538/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL538/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM538/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7666666666666667,"d":"0.77"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9230233",9,230,3,23,9,0,0,0,{"v":0,"d":"0.0"},662,0,0,0,1.362,1.1,1.1,1.1,99,0,0,0,17,0,0,0,0.581563313598903,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK539/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL539/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM539/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7666666666666667,"d":"0.77"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9230303",9,230,3,30,14,0,0,0,{"v":0,"d":"0.0"},872,0,0,0,1.362,1.1,1.1,1.1,130,0,0,0,22,0,0,0,1.6466028203409315,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK540/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL540/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM540/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1500000000000001,"d":"1.15"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9230383",9,230,3,38,19,0,0,0,{"v":0,"d":"0.0"},1148,0,0,0,1.362,1.1,1.1,1.1,171,0,0,0,29,0,0,0,5.150204288927729,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK541/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL541/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM541/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5333333333333334,"d":"1.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9250143",9,250,3,14,4,0,0,0,{"v":0,"d":"0.0"},462.00000000000006,0,0,0,1.362,1.1,1.1,1.1,69,0,0,0,12,0,0,0,0.23147910158223278,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK542/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL542/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM542/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4166666666666667,"d":"0.42"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9250183",9,250,3,18,9,0,0,0,{"v":0,"d":"0.0"},600.6,0,0,0,1.362,1.1,1.1,1.1,90,0,0,0,15,0,0,0,0.5063337677274552,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK543/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL543/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM543/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8333333333333334,"d":"0.83"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9250233",9,250,3,23,9,0,0,0,{"v":0,"d":"0.0"},728.2,0,0,0,1.362,1.1,1.1,1.1,109,0,0,0,19,0,0,0,0.7774748434438475,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK544/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL544/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM544/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8333333333333334,"d":"0.83"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9250303",9,250,3,30,14,0,0,0,{"v":0,"d":"0.0"},959.2,0,0,0,1.362,1.1,1.1,1.1,143,0,0,0,25,0,0,0,2.1779947192326357,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK545/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL545/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM545/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9250383",9,250,3,38,19,0,0,0,{"v":0,"d":"0.0"},1262.8000000000002,0,0,0,1.362,1.1,1.1,1.1,188,0,0,0,32,0,0,0,6.5787231866111275,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK546/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL546/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM546/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6666666666666667,"d":"1.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9270143",9,270,3,14,{"$f":"IF($E547=14,4,IF($E547=18,9,IF($E547=23,9,IF($E547=30,14,IF($E547=38,19,)))))","v":4},0,0,0,{"v":0,"d":"0.0"},504,0,0,0,1.362,1.1,1.1,1.1,75,0,0,0,13,0,0,0,0.28823563937024926,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK547/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL547/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM547/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9270183",9,270,3,18,9,0,0,0,{"v":0,"d":"0.0"},655.1999999999999,0,0,0,1.362,1.1,1.1,1.1,98,0,0,0,17,0,0,0,0.689250927361306,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK548/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL548/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM548/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9270233",9,270,3,23,9,0,0,0,{"v":0,"d":"0.0"},794.4,0,0,0,1.362,1.1,1.1,1.1,119,0,0,0,20,0,0,0,0.9256007330810442,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK549/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL549/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM549/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9270303",9,270,3,30,14,0,0,0,{"v":0,"d":"0.0"},1046.3999999999999,0,0,0,1.362,1.1,1.1,1.1,156,0,0,0,27,0,0,0,2.6506847595833642,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK550/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL550/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM550/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.35,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9270383",9,270,3,38,19,0,0,0,{"v":0,"d":"0.0"},1377.6,0,0,0,1.362,1.1,1.1,1.1,206,0,0,0,35,0,0,0,8.22696997791874,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK551/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL551/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM551/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.8,"d":"1.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9290143",9,290,3,14,4,0,0,0,{"v":0,"d":"0.0"},546,0,0,0,1.362,1.1,1.1,1.1,81,0,0,0,14,0,0,0,0.3530867945926205,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK552/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL552/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM552/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.48333333333333334,"d":"0.48"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9290183",9,290,3,18,9,0,0,0,{"v":0,"d":"0.0"},709.8000000000001,0,0,0,1.362,1.1,1.1,1.1,106,0,0,0,18,0,0,0,0.8242858637881794,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK553/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL553/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM553/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9666666666666667,"d":"0.97"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9290233",9,290,3,23,9,0,0,0,{"v":0,"d":"0.0"},860.6,0,0,0,1.362,1.1,1.1,1.1,128,0,0,0,22,0,0,0,1.1862652727747638,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK554/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL554/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM554/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9666666666666667,"d":"0.97"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9290303",9,290,3,30,14,0,0,0,{"v":0,"d":"0.0"},1133.6000000000001,0,0,0,1.362,1.1,1.1,1.1,169,0,0,0,29,0,0,0,3.1799833551297083,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK555/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL555/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM555/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9290383",9,290,3,38,19,0,0,0,{"v":0,"d":"0.0"},1492.4,0,0,0,1.362,1.1,1.1,1.1,223,0,0,0,38,0,0,0,10.106342508164412,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK556/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL556/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM556/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.9333333333333333,"d":"1.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9310143",9,310,3,14,4,0,0,0,{"v":0,"d":"0.0"},588,0,0,0,1.362,1.1,1.1,1.1,88,0,0,0,15,0,0,0,0.42648072655446717,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK557/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL557/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM557/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5166666666666667,"d":"0.52"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9310183",9,310,3,18,9,0,0,0,{"v":0,"d":"0.0"},764.4,0,0,0,1.362,1.1,1.1,1.1,114,0,0,0,20,0,0,0,1.070208051876416,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK558/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL558/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM558/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0333333333333334,"d":"1.03"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9310233",9,310,3,23,9,0,0,0,{"v":0,"d":"0.0"},926.8,0,0,0,1.362,1.1,1.1,1.1,138,0,0,0,24,0,0,0,1.4897525372473128,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK559/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL559/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM559/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0333333333333334,"d":"1.03"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9310303",9,310,3,30,14,0,0,0,{"v":0,"d":"0.0"},1220.8,0,0,0,1.362,1.1,1.1,1.1,182,0,0,0,31,0,0,0,3.767968204581134,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,{"$f":"ROUND(AK560*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},0,0,{"$f":"(AK560/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL560/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM560/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.55,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9310383",9,310,3,38,19,0,0,0,{"v":0,"d":"0.0"},1607.1999999999998,0,0,0,1.362,1.1,1.1,1.1,240,0,0,0,41,0,0,0,12.227855618298662,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK561/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL561/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM561/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.066666666666667,"d":"2.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
[{"$f":"CONCATENATE(B562,C562,E562,D562)","v":"9330143"},9,330,3,14,4,0,0,0,{"v":0,"d":"0.0"},630,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K562*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O562),0)","v":94},0,0,0,16,0,0,0,0.5088567516604612,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK562/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL562/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM562/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.55,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9330183",9,330,3,18,9,0,0,0,{"v":0,"d":"0.0"},819,0,0,0,1.362,1.1,1.1,1.1,122,0,0,0,21,0,0,0,1.2482471756812448,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK563/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL563/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM563/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9330233",9,330,3,23,9,0,0,0,{"v":0,"d":"0.0"},993,0,0,0,1.362,1.1,1.1,1.1,148,0,0,0,25,0,0,0,1.7126454332887506,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK564/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL564/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM564/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9330303",9,330,3,30,14,0,0,0,{"v":0,"d":"0.0"},1308,0,0,0,1.362,1.1,1.1,1.1,195,0,0,0,34,0,0,0,4.618220054037957,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK565/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL565/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM565/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6500000000000001,"d":"1.65"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9330383",9,330,3,38,19,0,0,0,{"v":0,"d":"0.0"},1722,0,0,0,1.362,1.1,1.1,1.1,257,0,0,0,44,0,0,0,14.602181877982916,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK566/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL566/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM566/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.2,"d":"2.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9350143",9,350,3,14,4,0,0,0,{"v":0,"d":"0.0"},672,0,0,0,1.362,1.1,1.1,1.1,100,0,0,0,17,0,0,0,0.6006460956680747,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK567/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL567/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM567/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5833333333333334,"d":"0.58"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9350183",9,350,3,18,9,0,0,0,{"v":0,"d":"0.0"},873.6,0,0,0,1.362,1.1,1.1,1.1,130,0,0,0,22,0,0,0,1.44411238030901,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK568/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL568/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM568/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1666666666666667,"d":"1.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9350233",9,350,3,23,9,0,0,0,{"v":0,"d":"0.0"},1059.2,0,0,0,1.362,1.1,1.1,1.1,158,0,0,0,27,0,0,0,2.093872050363853,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK569/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL569/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM569/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1666666666666667,"d":"1.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9350303",9,350,3,30,14,0,0,0,{"v":0,"d":"0.0"},1395.2,0,0,0,1.362,1.1,1.1,1.1,208,0,0,0,36,0,0,0,{"$f":"0.0098*(($BM570*(W570^$BO570)*($C570-14.4)*$BP570)+($BN570*W570*W570))","v":5.348520689638155},0,{"$f":"0.0098*(($BM570*(Y570^$BO570)*($C570-14.4)*$BP570)+($BN570*Y570*Y570))","v":0},{"$f":"0.0098*(($BM570*(Z570^$BO570)*($C570-14.4)*$BP570)+($BN570*Z570*Z570))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK570/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL570/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM570/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9350383",9,350,3,38,19,0,0,0,{"v":0,"d":"0.0"},1836.8000000000002,0,0,0,1.362,1.1,1.1,1.1,274,0,0,0,47,0,0,0,17.239685436784388,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK571/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL571/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM571/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.3333333333333335,"d":"2.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9370143",9,370,3,14,4,0,0,0,{"v":0,"d":"0.0"},714,0,0,0,1.362,1.1,1.1,1.1,107,0,0,0,18,0,0,0,0.7022725388293031,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK572/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL572/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM572/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6166666666666667,"d":"0.62"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9370183",9,370,3,18,9,0,0,0,{"v":0,"d":"0.0"},928.1999999999999,0,0,0,1.362,1.1,1.1,1.1,139,0,0,0,24,0,0,0,1.7916820743727735,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK573/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL573/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM573/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2333333333333334,"d":"1.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9370233",9,370,3,23,9,0,0,0,{"v":0,"d":"0.0"},1125.3999999999999,0,0,0,1.362,1.1,1.1,1.1,168,0,0,0,29,0,0,0,2.5255509078646936,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK574/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL574/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM574/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2333333333333334,"d":"1.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9370303",9,370,3,30,14,0,0,0,{"v":0,"d":"0.0"},1482.3999999999999,0,0,0,1.362,1.1,1.1,1.1,221,0,0,0,38,0,0,0,6.143887659158415,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK575/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL575/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM575/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.85,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9370383",9,370,3,38,19,0,0,0,{"v":0,"d":"0.0"},1951.6,0,0,0,1.362,1.1,1.1,1.1,291,{"$f":"ROUND(L576*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P576),0)","v":0},{"$f":"ROUND(M576*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q576),0)","v":0},{"$f":"ROUND(N576*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R576),0)","v":0},{"$f":"ROUND(S576*3600/(4186*ABS($M$1-$M$2)),0)","v":50},0,0,0,20.15045053068284,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK576/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL576/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM576/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.466666666666667,"d":"2.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9390143",9,390,3,14,4,0,0,0,{"v":0,"d":"0.0"},756,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K577*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O577),0)","v":113},0,0,0,19,0,0,0,0.814152974600655,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK577/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL577/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM577/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.65,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9390183",9,390,3,18,9,0,0,0,{"v":0,"d":"0.0"},982.8000000000001,0,0,0,1.362,1.1,1.1,1.1,147,0,0,0,25,0,0,0,2.0377800314726215,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE578*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH578),0)","v":0},0,0,0,0,0,{"$f":"(AK578/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL578/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM578/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9390233",9,390,3,23,9,0,0,0,{"v":0,"d":"0.0"},1191.6000000000001,0,0,0,1.362,1.1,1.1,1.1,178,0,0,0,31,0,0,0,3.0104597264911135,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK579/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL579/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM579/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9390303",9,390,3,30,14,0,0,0,{"v":0,"d":"0.0"},1569.6000000000001,0,0,0,1.362,1.1,1.1,1.1,234,0,0,0,40,0,0,0,7.006130377882931,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK580/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL580/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM580/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.95,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9390383",9,390,3,38,19,0,0,0,{"v":0,"d":"0.0"},2066.4,0,0,0,1.362,1.1,1.1,1.1,308,0,0,0,53,0,0,0,23.34430576435592,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK581/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL581/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM581/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.6,"d":"2.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9410143",9,410,3,14,4,0,0,0,{"v":0,"d":"0.0"},798,0,0,0,1.362,1.1,1.1,1.1,119,0,0,0,20,0,0,0,0.93669789767544,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK582/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL582/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM582/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6833333333333333,"d":"0.68"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9410183",9,410,3,18,9,0,0,0,{"v":0,"d":"0.0"},1037.3999999999999,0,0,0,1.362,1.1,1.1,1.1,155,0,0,0,27,0,0,0,2.467715139583368,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK583/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL583/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM583/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3666666666666667,"d":"1.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9410233",9,410,3,23,9,0,0,0,{"v":0,"d":"0.0"},1257.8,0,0,0,1.362,1.1,1.1,1.1,188,0,0,0,32,0,0,0,3.3585306152410803,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK584/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL584/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM584/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3666666666666667,"d":"1.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9410303",9,410,3,30,14,0,0,0,{"v":0,"d":"0.0"},1656.8,0,0,0,1.362,1.1,1.1,1.1,247,0,0,0,42,0,0,0,7.9370094792215165,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK585/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL585/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM585/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F585=$BR$70,$C585*$BS$70,IF($F585=$BR$71,$C585*$BS$71,IF($F585=$BR$72,$C585*$BS$72,IF($F585=$BR$73,$C585*$BS$73,IF($F585=$BR$74,$C585*$BS$74,IF($F585=$BR$75,$C585*$BS$75,IF($F585=$BR$76,$C585*$BS$76,IF($F585=$BR$77,$C585*$BS$77,IF($F585=$BR$78,$C585*$BS$78,IF($F585=$BR$79,$C585*$BS$79,IF($F585=$BR$80,$C585*$BS$80,)))))))))))","v":2.05},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9410383",9,410,3,38,19,0,0,0,{"v":0,"d":"0.0"},2181.2,0,0,0,1.362,1.1,1.1,1.1,326,0,0,0,56,0,0,0,26.830845003537494,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK586/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL586/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM586/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM586*(AN586^$BO586)*($C586-14.4)*$BP586)+($BN586*AN586*AN586))","v":0},0,0,{"v":2.7333333333333334,"d":"2.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F586=$BR$70,$BT$70,IF($F586=$BR$71,$BT$71,IF($F586=$BR$72,$BT$72,IF($F586=$BR$73,$BT$73,IF($F586=$BR$74,$BT$74,IF($F586=$BR$75,$BT$75,IF($F586=$BR$76,$BT$76,IF($F586=$BR$77,$BT$77,IF($F586=$BR$78,$BT$78,IF($F586=$BR$79,$BT$79,IF($F586=$BR$80,$BT$80,)))))))))))","v":0.011616292894075},{"$f":"IF($F586=$BR$70,$BU$70,IF($F586=$BR$71,$BU$71,IF($F586=$BR$72,$BU$72,IF($F586=$BR$73,$BU$73,IF($F586=$BR$74,$BU$74,IF($F586=$BR$75,$BU$75,IF($F586=$BR$76,$BU$76,IF($F586=$BR$77,$BU$77,IF($F586=$BR$78,$BU$78,IF($F586=$BR$79,$BU$79,IF($F586=$BR$80,$BU$80,)))))))))))","v":0.0016553227470232},{"$f":"IF($F586=$BR$70,$BV$70,IF($F586=$BR$71,$BV$71,IF($F586=$BR$72,$BV$72,IF($F586=$BR$73,$BV$73,IF($F586=$BR$74,$BV$74,IF($F586=$BR$75,$BV$75,IF($F586=$BR$76,$BV$76,IF($F586=$BR$77,$BV$77,IF($F586=$BR$78,$BV$78,IF($F586=$BR$79,$BV$79,IF($F586=$BR$80,$BV$80,)))))))))))","v":1.5869346821791},{"$f":"IF($F586=$BR$70,$BW$70,IF($F586=$BR$71,$BW$71,IF($F586=$BR$72,$BW$72,IF($F586=$BR$73,$BW$73,IF($F586=$BR$74,$BW$74,IF($F586=$BR$75,$BW$75,IF($F586=$BR$76,$BW$76,IF($F586=$BR$77,$BW$77,IF($F586=$BR$78,$BW$78,IF($F586=$BR$79,$BW$79,IF($F586=$BR$80,$BW$80,)))))))))))","v":1}]
["9430143",9,430,3,14,4,0,0,0,{"v":0,"d":"0.0"},840,0,0,0,1.362,1.1,1.1,1.1,125,0,0,0,22,0,0,0,1.159663018072622,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK587/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL587/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM587/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7166666666666667,"d":"0.72"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9430183",9,430,3,18,9,0,0,0,{"v":0,"d":"0.0"},1092,0,0,0,1.362,1.1,1.1,1.1,163,0,0,0,28,0,0,0,2.769122073604798,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK588/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL588/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM588/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4333333333333333,"d":"1.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9430233",9,430,3,23,9,0,0,0,{"v":0,"d":"0.0"},1324,0,0,0,1.362,1.1,1.1,1.1,198,0,0,0,34,0,0,0,3.938278524788483,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK589/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL589/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM589/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4333333333333333,"d":"1.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9430303",9,430,3,30,14,0,0,0,{"v":0,"d":"0.0"},1744,0,0,0,1.362,1.1,1.1,1.1,260,0,0,0,45,0,0,0,9.243614683776842,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK590/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL590/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM590/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.15,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9430383",9,430,3,38,19,0,0,0,{"v":0,"d":"0.0"},2296,0,0,0,1.362,1.1,1.1,1.1,343,0,0,0,59,0,0,0,30.619445510321473,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK591/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL591/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM591/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8666666666666667,"d":"2.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9450143",9,450,3,14,4,0,0,0,{"v":0,"d":"0.0"},882,0,0,0,1.362,1.1,1.1,1.1,132,0,0,0,23,0,0,0,1.3121699297272875,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK592/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL592/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM592/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9450183",9,450,3,18,9,0,0,0,{"v":0,"d":"0.0"},1146.6000000000001,0,0,0,1.362,1.1,1.1,1.1,171,0,0,0,29,0,0,0,3.0929909707206327,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,{"$f":"ROUND(AK593*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},0,0,{"$f":"(AK593/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL593/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM593/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9450233",9,450,3,23,9,0,0,0,{"v":0,"d":"0.0"},1390.2,0,0,0,1.362,1.1,1.1,1.1,208,0,0,0,36,0,0,0,4.5785464969271334,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK594/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL594/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM594/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9450303",9,450,3,30,14,0,0,0,{"v":0,"d":"0.0"},1831.2,0,0,0,1.362,1.1,1.1,1.1,273,0,0,0,47,0,0,0,10.3385855420632,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK595/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL595/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM595/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9450383",9,450,3,38,19,0,0,0,{"v":0,"d":"0.0"},2410.8,0,0,0,1.362,1.1,1.1,1.1,360,0,0,0,62,0,0,0,34.71928380941988,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK596/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL596/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM596/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3,"d":"3.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9470143",9,470,3,14,4,0,0,0,{"v":0,"d":"0.0"},924.0000000000001,0,0,0,1.362,1.1,1.1,1.1,138,0,0,0,24,0,0,0,1.4767854795696327,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK597/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL597/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM597/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7833333333333334,"d":"0.78"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9470183",9,470,3,18,9,0,0,0,{"v":0,"d":"0.0"},1201.2,0,0,0,1.362,1.1,1.1,1.1,179,0,0,0,31,0,0,0,3.6508669486907905,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK598/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL598/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM598/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5666666666666669,"d":"1.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9470233",9,470,3,23,9,0,0,0,{"v":0,"d":"0.0"},1456.4,0,0,0,1.362,1.1,1.1,1.1,217,0,0,0,37,0,0,0,5.0325529398758855,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK599/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL599/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM599/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5666666666666669,"d":"1.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9470303",9,470,3,30,14,0,0,0,{"v":0,"d":"0.0"},1918.4,0,0,0,1.362,1.1,1.1,1.1,286,0,0,0,49,0,0,0,11.507703581566133,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK600/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL600/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM600/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.35,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9470383",9,470,3,38,19,0,0,0,{"v":0,"d":"0.0"},2525.6000000000004,0,0,0,1.362,1.1,1.1,1.1,377,0,0,0,{"$f":"ROUND(S601*3600/(4186*ABS($M$1-$M$2)),0)","v":65},0,0,0,39.139349667189585,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK601/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL601/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM601/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1333333333333337,"d":"3.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["9490143",9,490,3,14,4,0,0,0,{"v":0,"d":"0.0"},965.9999999999999,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K602*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O602),0)","v":144},0,0,0,25,0,0,0,1.6538954007292748,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK602/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL602/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM602/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8166666666666668,"d":"0.82"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["9490183",9,490,3,18,9,0,0,0,{"v":0,"d":"0.0"},1255.8,0,0,0,1.362,1.1,1.1,1.1,187,0,0,0,32,0,0,0,4.036900100041043,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK603/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL603/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM603/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6333333333333335,"d":"1.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9490233",9,490,3,23,9,0,0,0,{"v":0,"d":"0.0"},1522.6,0,0,0,1.362,1.1,1.1,1.1,227,0,0,0,39,0,0,0,5.779651206670769,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK604/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL604/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM604/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6333333333333335,"d":"1.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["9490303",9,490,3,30,14,0,0,0,{"v":0,"d":"0.0"},2005.6,0,0,0,1.362,1.1,1.1,1.1,299,0,0,0,51,0,0,0,12.752556678953407,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK605/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL605/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM605/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["9490383",9,490,3,38,19,0,0,0,{"v":0,"d":"0.0"},2640.3999999999996,0,0,0,1.362,1.1,1.1,1.1,394,0,0,0,68,0,0,0,43.88845848606404,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK606/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL606/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM606/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.266666666666667,"d":"3.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
[{"$f":"CONCATENATE(B607,C607,E607,D607)","v":"1270143"},12,70,3,14,4,0,0,0,{"v":0,"d":"0.0"},91.2,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K607*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O607),0)","v":14},{"$f":"ROUND(L607*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P607),0)","v":0},{"$f":"ROUND(M607*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q607),0)","v":0},{"$f":"ROUND(N607*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R607),0)","v":0},{"$f":"ROUND(S607*3600/(4186*ABS($M$1-$M$2)),0)","v":2},{"$f":"ROUND(T607*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U607*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V607*3600/(4186*ABS($M$1-$M$2)),0)","v":0},2.4998470803170997E-3,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE607*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH607),0)","v":0},{"$f":"ROUND(AF607*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI607),0)","v":0},{"$f":"ROUND(AG607*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ607),0)","v":0},{"$f":"ROUND(AK607*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL607*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM607*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK607/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL607/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM607/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.11666666666666667,"d":"0.12"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["1270183",12,70,3,18,9,0,0,0,{"v":0,"d":"0.0"},135.20000000000002,0,0,0,1.362,1.1,1.1,1.1,20,0,0,0,3,0,0,0,6.4730267114827406E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK608/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL608/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM608/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.23333333333333334,"d":"0.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1270233",12,70,3,23,9,0,0,0,{"v":0,"d":"0.0"},158.8,0,0,0,1.362,1.1,1.1,1.1,24,0,0,0,4,0,0,0,0.010910857489775673,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK609/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL609/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM609/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.23333333333333334,"d":"0.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1270303",12,70,3,30,14,0,0,0,{"v":0,"d":"0.0"},220.8,0,0,0,1.362,1.1,1.1,1.1,33,0,0,0,6,0,0,0,0.06103056774869194,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK610/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL610/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM610/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.35000000000000003,"d":"0.35"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["1270383",12,70,3,38,{"$f":"IF($E611=14,4,IF($E611=18,9,IF($E611=23,9,IF($E611=30,14,IF($E611=38,19,)))))","v":19},0,0,0,{"v":0,"d":"0.0"},284.8,0,0,0,1.362,1.1,1.1,1.1,43,0,0,0,7,0,0,0,0.1396250416559609,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK611/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL611/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM611/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4666666666666667,"d":"0.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["1280143",12,80,3,14,4,0,0,0,{"v":0,"d":"0.0"},114,0,0,0,1.362,1.1,1.1,1.1,17,0,0,0,3,0,0,0,0.005930081911941236,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK612/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL612/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM612/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.13333333333333333,"d":"0.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["1280183",12,80,3,18,9,0,0,0,{"v":0,"d":"0.0"},169,0,0,0,1.362,1.1,1.1,1.1,25,0,0,0,4,0,0,0,0.012862019153558217,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK613/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL613/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM613/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.26666666666666666,"d":"0.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1280233",12,80,3,23,9,0,0,0,{"v":0,"d":"0.0"},198.5,0,0,0,1.362,1.1,1.1,1.1,30,0,0,0,5,0,0,0,0.019283246366097708,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK614/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL614/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM614/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.26666666666666666,"d":"0.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1280303",12,80,3,30,14,0,0,0,{"v":0,"d":"0.0"},276,0,0,0,1.362,1.1,1.1,1.1,41,0,0,0,7,0,0,0,0.09063486607384304,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK615/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL615/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM615/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["1280383",12,80,3,38,19,0,0,0,{"v":0,"d":"0.0"},356,0,0,0,1.362,1.1,1.1,1.1,53,0,0,0,9,0,0,0,0.24538601904197524,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK616/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL616/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM616/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5333333333333333,"d":"0.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["1290143",12,90,3,14,4,0,0,0,{"v":0,"d":"0.0"},136.79999999999998,0,0,0,1.362,1.1,1.1,1.1,20,0,0,0,3,0,0,0,0.006829581822298132,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK617/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL617/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM617/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.15000000000000002,"d":"0.15"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["1290183",12,90,3,18,9,0,0,0,{"v":0,"d":"0.0"},202.79999999999998,0,0,0,1.362,1.1,1.1,1.1,30,0,0,0,5,0,0,0,0.02220790314848095,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK618/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL618/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM618/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.30000000000000004,"d":"0.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1290233",12,90,3,23,9,0,0,0,{"v":0,"d":"0.0"},238.2,0,0,0,1.362,1.1,1.1,1.1,36,0,0,0,6,0,0,0,0.030917006245236994,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK619/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL619/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM619/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.30000000000000004,"d":"0.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1290303",12,90,3,30,14,0,0,0,{"v":0,"d":"0.0"},331.2,0,0,0,1.362,1.1,1.1,1.1,49,0,0,0,8,0,0,0,0.1274901263303854,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK620/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL620/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM620/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["1290383",12,90,3,38,19,0,0,0,{"v":0,"d":"0.0"},427.2,0,0,0,1.362,1.1,1.1,1.1,64,0,0,0,11,0,0,0,0.38871935810470565,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK621/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL621/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM621/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6000000000000001,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12100143",12,100,3,14,4,0,0,0,{"v":0,"d":"0.0"},159.6,0,0,0,1.362,1.1,1.1,1.1,24,0,0,0,4,0,0,0,0.012692746488264683,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK622/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL622/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM622/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.16666666666666669,"d":"0.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12100183",12,100,3,18,9,0,0,0,{"v":0,"d":"0.0"},236.6,0,0,0,1.362,1.1,1.1,1.1,35,0,0,0,6,0,0,0,0.034987986312321834,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK623/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL623/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM623/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.33333333333333337,"d":"0.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12100233",12,100,3,23,9,0,0,0,{"v":0,"d":"0.0"},277.9,0,0,0,1.362,1.1,1.1,1.1,41,0,0,0,7,0,0,0,0.046280931550525505,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK624/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL624/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM624/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.33333333333333337,"d":"0.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12100303",12,100,3,30,14,0,0,0,{"v":0,"d":"0.0"},386.4,0,0,0,1.362,1.1,1.1,1.1,58,0,0,0,10,0,0,0,0.20147683996920915,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK625/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL625/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM625/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12100383",12,100,3,38,19,0,0,0,{"v":0,"d":"0.0"},498.4,0,0,0,1.362,1.1,1.1,1.1,74,0,0,0,13,0,0,0,0.5735925031828658,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK626/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL626/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM626/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6666666666666667,"d":"0.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
[{"$f":"CONCATENATE(B627,C627,E627,D627)","v":"12110143"},12,110,3,14,4,0,0,0,{"v":0,"d":"0.0"},182.4,0,0,0,1.362,1.1,1.1,1.1,27,0,0,0,5,0,0,0,0.020818404602186466,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK627/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL627/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM627/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.18333333333333335,"d":"0.18"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12110183",12,110,3,18,9,0,0,0,{"v":0,"d":"0.0"},270.40000000000003,0,0,0,1.362,1.1,1.1,1.1,40,0,0,0,7,0,0,0,0.051665258153112514,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK628/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL628/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM628/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3666666666666667,"d":"0.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12110233",12,110,3,23,9,0,0,0,{"v":0,"d":"0.0"},317.6,0,0,0,1.362,1.1,1.1,1.1,47,0,0,0,8,0,0,0,0.06583071528532904,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK629/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL629/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM629/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3666666666666667,"d":"0.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12110303",12,110,3,30,14,0,0,0,{"v":0,"d":"0.0"},441.6,0,0,0,1.362,1.1,1.1,1.1,66,0,0,0,11,0,0,0,0.25941175732183763,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK630/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL630/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM630/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.55,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12110383",12,110,3,38,19,0,0,0,{"v":0,"d":"0.0"},569.6,0,0,0,1.362,1.1,1.1,1.1,85,0,0,0,15,0,0,0,0.8037265157332849,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK631/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL631/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM631/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7333333333333334,"d":"0.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12120143",12,120,3,14,4,0,0,0,{"v":0,"d":"0.0"},205.20000000000002,0,0,0,1.362,1.1,1.1,1.1,31,0,0,0,5,0,0,0,0.022987530345093,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK632/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL632/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM632/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.2,"d":"0.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12120183",12,120,3,18,9,0,0,0,{"v":0,"d":"0.0"},304.2,0,0,0,1.362,1.1,1.1,1.1,45,0,0,0,8,0,0,0,0.07269066515235312,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK633/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL633/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM633/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12120233",12,120,3,23,9,0,0,0,{"v":0,"d":"0.0"},357.3,0,0,0,1.362,1.1,1.1,1.1,53,0,0,0,9,0,0,0,{"$f":"0.0098*(($BM634*(W634^$BO634)*($C634-14.4)*$BP634)+($BN634*W634*W634))","v":0.09001097188873623},0,{"$f":"0.0098*(($BM634*(Y634^$BO634)*($C634-14.4)*$BP634)+($BN634*Y634*Y634))","v":0},{"$f":"0.0098*(($BM634*(Z634^$BO634)*($C634-14.4)*$BP634)+($BN634*Z634*Z634))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK634/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL634/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM634/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12120303",12,120,3,30,14,0,0,0,{"v":0,"d":"0.0"},496.8,0,0,0,1.362,1.1,1.1,1.1,74,0,0,0,13,0,0,0,0.3677813575428125,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,{"$f":"ROUND(AK635*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},0,0,{"$f":"(AK635/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL635/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM635/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12120383",12,120,3,38,19,0,0,0,{"v":0,"d":"0.0"},640.8000000000001,0,0,0,1.362,1.1,1.1,1.1,96,0,0,0,17,0,0,0,1.082640684299574,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK636/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL636/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM636/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12130143",12,130,3,14,4,0,0,0,{"v":0,"d":"0.0"},228,0,0,0,1.362,1.1,1.1,1.1,34,0,0,0,6,0,0,0,0.03444837355493069,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK637/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL637/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM637/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.21666666666666667,"d":"0.22"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12130183",12,130,3,18,9,0,0,0,{"v":0,"d":"0.0"},338,0,0,0,1.362,1.1,1.1,1.1,50,0,0,0,9,0,0,0,0.09850482404575009,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK638/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL638/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM638/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.43333333333333335,"d":"0.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12130233",12,130,3,23,9,0,0,0,{"v":0,"d":"0.0"},397,0,0,0,1.362,1.1,1.1,1.1,59,0,0,0,10,0,0,0,0.11925675258958948,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK639/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL639/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM639/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.43333333333333335,"d":"0.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12130303",12,130,3,30,14,0,0,0,{"v":0,"d":"0.0"},552,0,0,0,1.362,1.1,1.1,1.1,82,0,0,0,14,0,0,0,0.4496966860232294,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK640/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL640/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM640/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.65,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12130383",12,130,3,38,19,0,0,0,{"v":0,"d":"0.0"},712,0,0,0,1.362,1.1,1.1,1.1,106,0,0,0,18,0,0,0,1.2973286424048103,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK641/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL641/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM641/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8666666666666667,"d":"0.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12150143",12,150,3,14,4,0,0,0,{"v":0,"d":"0.0"},273.59999999999997,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K642*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O642),0)","v":41},0,0,0,7,0,0,0,0.05268270126173568,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK642/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL642/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM642/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12150183",12,150,3,18,9,0,0,0,{"v":0,"d":"0.0"},405.59999999999997,0,0,0,1.362,1.1,1.1,1.1,61,0,0,0,10,0,0,0,0.13982193617002808,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE643*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH643),0)","v":0},0,0,0,0,0,{"$f":"(AK643/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL643/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM643/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12150233",12,150,3,23,9,0,0,0,{"v":0,"d":"0.0"},476.4,0,0,0,1.362,1.1,1.1,1.1,71,0,0,0,12,0,0,0,0.1946440766472133,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK644/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL644/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM644/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12150303",12,150,3,30,14,0,0,0,{"v":0,"d":"0.0"},662.4,0,0,0,1.362,1.1,1.1,1.1,99,0,0,0,17,0,0,0,0.704949624403007,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK645/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL645/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM645/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12150383",12,150,3,38,19,0,0,0,{"v":0,"d":"0.0"},854.4,0,0,0,1.362,1.1,1.1,1.1,128,0,0,0,22,0,0,0,2.091816568306519,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK646/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL646/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM646/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12170143",12,170,3,14,4,0,0,0,{"v":0,"d":"0.0"},319.2,0,0,0,1.362,1.1,1.1,1.1,48,0,0,0,8,0,0,0,0.07607148445486532,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK647/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL647/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM647/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.2833333333333333,"d":"0.28"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12170183",12,170,3,18,9,0,0,0,{"v":0,"d":"0.0"},473.2,0,0,0,1.362,1.1,1.1,1.1,71,0,0,0,12,0,0,0,0.22326981247242142,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK648/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL648/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM648/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5666666666666667,"d":"0.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12170233",12,170,3,23,9,0,0,0,{"v":0,"d":"0.0"},555.8,0,0,0,1.362,1.1,1.1,1.1,83,0,0,0,14,0,0,0,0.2953209272612503,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK649/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL649/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM649/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F649=$BR$70,$C649*$BS$70,IF($F649=$BR$71,$C649*$BS$71,IF($F649=$BR$72,$C649*$BS$72,IF($F649=$BR$73,$C649*$BS$73,IF($F649=$BR$74,$C649*$BS$74,IF($F649=$BR$75,$C649*$BS$75,IF($F649=$BR$76,$C649*$BS$76,IF($F649=$BR$77,$C649*$BS$77,IF($F649=$BR$78,$C649*$BS$78,IF($F649=$BR$79,$C649*$BS$79,IF($F649=$BR$80,$C649*$BS$80,)))))))))))","v":{"v":0.5666666666666667,"d":"0.57"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12170303",12,170,3,30,14,0,0,0,{"v":0,"d":"0.0"},772.8,0,0,0,1.362,1.1,1.1,1.1,115,0,0,0,20,0,0,0,1.0311520292801872,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK650/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL650/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM650/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM650*(AN650^$BO650)*($C650-14.4)*$BP650)+($BN650*AN650*AN650))","v":0},0,0,0.85,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F650=$BR$70,$BT$70,IF($F650=$BR$71,$BT$71,IF($F650=$BR$72,$BT$72,IF($F650=$BR$73,$BT$73,IF($F650=$BR$74,$BT$74,IF($F650=$BR$75,$BT$75,IF($F650=$BR$76,$BT$76,IF($F650=$BR$77,$BT$77,IF($F650=$BR$78,$BT$78,IF($F650=$BR$79,$BT$79,IF($F650=$BR$80,$BT$80,)))))))))))","v":0.00255823982887},{"$f":"IF($F650=$BR$70,$BU$70,IF($F650=$BR$71,$BU$71,IF($F650=$BR$72,$BU$72,IF($F650=$BR$73,$BU$73,IF($F650=$BR$74,$BU$74,IF($F650=$BR$75,$BU$75,IF($F650=$BR$76,$BU$76,IF($F650=$BR$77,$BU$77,IF($F650=$BR$78,$BU$78,IF($F650=$BR$79,$BU$79,IF($F650=$BR$80,$BU$80,)))))))))))","v":0.00056161694684148},{"$f":"IF($F650=$BR$70,$BV$70,IF($F650=$BR$71,$BV$71,IF($F650=$BR$72,$BV$72,IF($F650=$BR$73,$BV$73,IF($F650=$BR$74,$BV$74,IF($F650=$BR$75,$BV$75,IF($F650=$BR$76,$BV$76,IF($F650=$BR$77,$BV$77,IF($F650=$BR$78,$BV$78,IF($F650=$BR$79,$BV$79,IF($F650=$BR$80,$BV$80,)))))))))))","v":1.4942747715062},{"$f":"IF($F650=$BR$70,$BW$70,IF($F650=$BR$71,$BW$71,IF($F650=$BR$72,$BW$72,IF($F650=$BR$73,$BW$73,IF($F650=$BR$74,$BW$74,IF($F650=$BR$75,$BW$75,IF($F650=$BR$76,$BW$76,IF($F650=$BR$77,$BW$77,IF($F650=$BR$78,$BW$78,IF($F650=$BR$79,$BW$79,IF($F650=$BR$80,$BW$80,)))))))))))","v":3}]
["12170383",12,170,3,38,19,0,0,0,{"v":0,"d":"0.0"},996.8,0,0,0,1.362,1.1,1.1,1.1,149,0,0,0,26,0,0,0,3.1282295960354793,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,{"$f":"ROUND(AK651*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},0,0,{"$f":"(AK651/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL651/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM651/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1333333333333333,"d":"1.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12190143",12,190,3,14,4,0,0,0,{"v":0,"d":"0.0"},364.8,0,0,0,1.362,1.1,1.1,1.1,54,0,0,0,9,0,0,0,0.10514306777227453,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK652/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL652/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM652/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3166666666666667,"d":"0.32"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12190183",12,190,3,18,9,0,0,0,{"v":0,"d":"0.0"},540.8000000000001,0,0,0,1.362,1.1,1.1,1.1,81,0,0,0,14,0,0,0,0.33318166555581685,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK653/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL653/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM653/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6333333333333334,"d":"0.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12190233",12,190,3,23,9,0,0,0,{"v":0,"d":"0.0"},635.2,0,0,0,1.362,1.1,1.1,1.1,95,0,0,0,16,0,0,0,0.42451761457968273,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK654/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL654/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM654/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6333333333333334,"d":"0.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12190303",12,190,3,30,14,0,0,0,{"v":0,"d":"0.0"},883.2,0,0,0,1.362,1.1,1.1,1.1,132,0,0,0,23,0,0,0,1.4338094438588642,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK655/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL655/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM655/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9500000000000001,"d":"0.95"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12190383",12,190,3,38,19,0,0,0,{"v":0,"d":"0.0"},1139.2,0,0,0,1.362,1.1,1.1,1.1,170,0,0,0,29,0,0,0,4.197224428090752,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK656/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL656/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM656/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2666666666666668,"d":"1.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12210143",12,210,3,14,4,0,0,0,{"v":0,"d":"0.0"},410.40000000000003,0,0,0,1.362,1.1,1.1,1.1,61,0,0,0,10,0,0,0,0.14040753186853402,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK657/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL657/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM657/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.35000000000000003,"d":"0.35"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12210183",12,210,3,18,9,0,0,0,{"v":0,"d":"0.0"},608.4,0,0,0,1.362,1.1,1.1,1.1,91,0,0,0,16,0,0,0,0.47275442965409814,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK658/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL658/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM658/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12210233",12,210,3,23,9,0,0,0,{"v":0,"d":"0.0"},714.6,0,0,0,1.362,1.1,1.1,1.1,107,0,0,0,18,0,0,0,0.5853824410463798,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK659/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL659/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM659/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12210303",12,210,3,30,14,0,0,0,{"v":0,"d":"0.0"},993.6,0,0,0,1.362,1.1,1.1,1.1,148,0,0,0,25,0,0,0,1.8088003532847183,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK660/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL660/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM660/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.05,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12210383",12,210,3,38,19,0,0,0,{"v":0,"d":"0.0"},1281.6000000000001,0,0,0,1.362,1.1,1.1,1.1,191,0,0,0,33,0,0,0,5.738309861702612,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK661/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL661/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM661/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4000000000000001,"d":"1.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12230143",12,230,3,14,4,0,0,0,{"v":0,"d":"0.0"},456,0,0,0,1.362,1.1,1.1,1.1,68,0,0,0,12,0,0,0,0.21186880433416547,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK662/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL662/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM662/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.38333333333333336,"d":"0.38"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12230183",12,230,3,18,9,0,0,0,{"v":0,"d":"0.0"},676,0,0,0,1.362,1.1,1.1,1.1,101,0,0,0,17,0,0,0,0.581563313598903,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK663/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL663/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM663/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7666666666666667,"d":"0.77"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12230233",12,230,3,23,9,0,0,0,{"v":0,"d":"0.0"},794,0,0,0,1.362,1.1,1.1,1.1,119,0,0,0,20,0,0,0,0.7809934142856723,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK664/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL664/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM664/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7666666666666667,"d":"0.77"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12230303",12,230,3,30,14,0,0,0,{"v":0,"d":"0.0"},1104,0,0,0,1.362,1.1,1.1,1.1,165,0,0,0,28,0,0,{"$f":"ROUND(V665*3600/(4186*ABS($M$1-$M$2)),0)","v":0},2.361475107440162,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK665/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL665/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM665/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1500000000000001,"d":"1.15"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12230383",12,230,3,38,19,0,0,0,{"v":0,"d":"0.0"},1424,0,0,0,1.362,1.1,1.1,1.1,213,0,0,0,{"$f":"ROUND(S666*3600/(4186*ABS($M$1-$M$2)),0)","v":37},0,0,0,7.583153344573588,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK666/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL666/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM666/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5333333333333334,"d":"1.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12250143",12,250,3,14,4,0,0,0,{"v":0,"d":"0.0"},501.6,0,0,0,1.362,1.1,1.1,1.1,75,0,0,0,13,0,0,0,0.26572513257289015,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK667/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL667/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM667/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4166666666666667,"d":"0.42"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12250183",12,250,3,18,9,0,0,0,{"v":0,"d":"0.0"},743.6,0,0,0,1.362,1.1,1.1,1.1,111,0,0,0,19,0,0,0,0.7774748434438475,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK668/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL668/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM668/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8333333333333334,"d":"0.83"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12250233",12,250,3,23,9,0,0,0,{"v":0,"d":"0.0"},873.4000000000001,0,0,0,1.362,1.1,1.1,1.1,130,0,0,0,22,0,0,0,1.0143672010852665,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK669/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL669/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM669/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8333333333333334,"d":"0.83"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12250303",12,250,3,30,14,0,0,0,{"v":0,"d":"0.0"},1214.4,0,0,0,1.362,1.1,1.1,1.1,181,0,0,0,31,0,0,0,3.0042309227477433,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK670/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL670/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM670/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12250383",12,250,3,38,19,0,0,0,{"v":0,"d":"0.0"},1566.4,0,0,0,1.362,1.1,1.1,1.1,234,0,0,0,40,0,0,0,9.376426270975275,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK671/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL671/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM671/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6666666666666667,"d":"1.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12270143",12,270,3,14,4,0,0,0,{"v":0,"d":"0.0"},547.1999999999999,0,0,0,1.362,1.1,1.1,1.1,82,0,0,0,14,0,0,0,0.3275100642157975,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK672/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL672/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM672/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12270183",12,270,3,18,9,0,0,0,{"v":0,"d":"0.0"},811.1999999999999,0,0,0,1.362,1.1,1.1,1.1,121,0,0,0,21,0,0,0,1.011264796747819,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK673/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL673/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM673/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12270233",12,270,3,23,9,0,0,0,{"v":0,"d":"0.0"},952.8,0,0,0,1.362,1.1,1.1,1.1,142,0,0,0,24,0,0,0,1.2884661791636722,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK674/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL674/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM674/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12270303",12,270,3,30,{"$f":"IF($E675=14,4,IF($E675=18,9,IF($E675=23,9,IF($E675=30,14,IF($E675=38,19,)))))","v":14},0,0,0,{"v":0,"d":"0.0"},1324.8,0,0,0,1.362,1.1,1.1,1.1,198,0,0,0,34,0,0,0,3.7414410411157935,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK675/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL675/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM675/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.35,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12270383",12,270,3,38,19,0,0,0,{"v":0,"d":"0.0"},1708.8,0,0,0,1.362,1.1,1.1,1.1,255,0,0,0,44,0,0,0,11.832072415897708,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK676/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL676/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM676/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.8,"d":"1.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12290143",12,290,3,14,4,0,0,0,{"v":0,"d":"0.0"},592.8000000000001,0,0,0,1.362,1.1,1.1,1.1,88,0,0,0,15,0,0,0,0.3976751335873178,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK677/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL677/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM677/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.48333333333333334,"d":"0.48"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12290183",12,290,3,18,9,0,0,0,{"v":0,"d":"0.0"},878.8000000000001,0,0,0,1.362,1.1,1.1,1.1,131,0,0,0,23,0,0,0,1.2858920108185188,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK678/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL678/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM678/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9666666666666667,"d":"0.97"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12290233",12,290,3,23,9,0,0,0,{"v":0,"d":"0.0"},1032.2,0,0,0,1.362,1.1,1.1,1.1,154,0,0,0,26,0,0,0,1.6062041244305802,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK679/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL679/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM679/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9666666666666667,"d":"0.97"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12290303",12,290,3,30,14,0,0,0,{"v":0,"d":"0.0"},1435.2,0,0,0,1.362,1.1,1.1,1.1,214,0,0,0,37,0,0,0,4.577280884244118,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK680/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL680/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM680/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12290383",12,290,3,38,19,0,0,0,{"v":0,"d":"0.0"},1851.2,0,0,0,1.362,1.1,1.1,1.1,276,0,0,0,47,0,0,0,14.163907603847747,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK681/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL681/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM681/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.9333333333333333,"d":"1.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12310143",12,310,3,14,4,0,0,0,{"v":0,"d":"0.0"},638.4,0,0,0,1.362,1.1,1.1,1.1,95,0,0,0,16,0,0,0,0.4766627369798236,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK682/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL682/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM682/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5166666666666667,"d":"0.52"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12310183",12,310,3,18,9,0,0,0,{"v":0,"d":"0.0"},946.4,0,0,0,1.362,1.1,1.1,1.1,141,0,0,0,24,0,0,0,1.4897525372473128,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK683/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL683/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM683/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0333333333333334,"d":"1.03"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12310233",12,310,3,23,9,0,0,0,{"v":0,"d":"0.0"},1111.6,0,0,0,1.362,1.1,1.1,1.1,166,0,0,0,29,0,0,0,2.099970860722739,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK684/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL684/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM684/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0333333333333334,"d":"1.03"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12310303",12,310,3,30,14,0,0,0,{"v":0,"d":"0.0"},1545.6,0,0,0,1.362,1.1,1.1,1.1,231,0,0,0,40,0,0,0,5.515752481363984,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK685/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL685/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM685/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.55,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12310383",12,310,3,38,19,0,0,0,{"v":0,"d":"0.0"},1993.6,0,0,0,1.362,1.1,1.1,1.1,298,0,0,0,51,0,0,0,17.29264246604115,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK686/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL686/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM686/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.066666666666667,"d":"2.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12330143",12,330,3,14,4,0,0,0,{"v":0,"d":"0.0"},684,0,0,0,1.362,1.1,1.1,1.1,102,0,0,0,18,0,0,0,0.6233956559463668,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK687/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL687/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM687/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.55,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12330183",12,330,3,18,9,0,0,0,{"v":0,"d":"0.0"},1014,0,0,0,1.362,1.1,1.1,1.1,151,0,0,0,26,0,0,0,1.8389425543183473,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK688/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL688/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM688/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12330233",12,330,3,23,9,0,0,0,{"v":0,"d":"0.0"},1191,0,0,0,1.362,1.1,1.1,1.1,178,0,0,0,31,0,0,0,2.5301543098413557,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK689/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL689/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM689/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12330303",12,330,3,30,14,0,0,0,{"v":0,"d":"0.0"},1656,0,0,0,1.362,1.1,1.1,1.1,247,0,0,0,42,0,0,0,6.333915304350317,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK690/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL690/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM690/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6500000000000001,"d":"1.65"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
[{"$f":"CONCATENATE(B691,C691,E691,D691)","v":"12330383"},12,330,3,38,19,0,0,0,{"v":0,"d":"0.0"},2136,0,0,0,1.362,1.1,1.1,1.1,319,0,0,0,55,0,0,0,20.81123214090481,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK691/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL691/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM691/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.2,"d":"2.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12350143",12,350,3,14,4,0,0,0,{"v":0,"d":"0.0"},729.6,0,0,0,1.362,1.1,1.1,1.1,109,0,0,0,19,0,0,0,0.7275741447709794,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK692/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL692/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM692/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5833333333333334,"d":"0.58"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12350183",12,350,3,18,9,0,0,0,{"v":0,"d":"0.0"},1081.6000000000001,0,0,0,1.362,1.1,1.1,1.1,161,0,0,0,28,0,0,0,2.2366746163792532,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK693/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL693/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM693/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1666666666666667,"d":"1.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12350233",12,350,3,23,9,0,0,0,{"v":0,"d":"0.0"},1270.4,0,0,0,1.362,1.1,1.1,1.1,190,0,0,0,33,0,0,0,3.0133613260217738,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK694/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL694/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM694/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1666666666666667,"d":"1.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12350303",12,350,3,30,14,0,0,0,{"v":0,"d":"0.0"},1766.4,0,0,0,1.362,1.1,1.1,1.1,264,0,0,0,45,0,0,0,7.466430969538772,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK695/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL695/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM695/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12350383",12,350,3,38,19,0,0,0,{"v":0,"d":"0.0"},2278.4,0,0,0,1.362,1.1,1.1,1.1,340,0,0,0,58,0,0,0,24.073886713582485,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK696/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL696/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM696/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.3333333333333335,"d":"2.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12370143",12,370,3,14,4,0,0,0,{"v":0,"d":"0.0"},775.1999999999999,0,0,0,1.362,1.1,1.1,1.1,116,0,0,0,20,0,0,0,0.8421182315808555,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK697/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL697/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM697/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6166666666666667,"d":"0.62"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12370183",12,370,3,18,9,0,0,0,{"v":0,"d":"0.0"},1149.2,0,0,0,1.362,1.1,1.1,1.1,172,0,0,0,30,0,0,0,{"$f":"0.0098*(($BM698*(W698^$BO698)*($C698-14.4)*$BP698)+($BN698*W698*W698))","v":2.685750673728019},0,{"$f":"0.0098*(($BM698*(Y698^$BO698)*($C698-14.4)*$BP698)+($BN698*Y698*Y698))","v":0},{"$f":"0.0098*(($BM698*(Z698^$BO698)*($C698-14.4)*$BP698)+($BN698*Z698*Z698))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK698/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL698/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM698/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2333333333333334,"d":"1.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12370233",12,370,3,23,9,0,0,0,{"v":0,"d":"0.0"},1349.8,0,0,0,1.362,1.1,1.1,1.1,201,0,0,0,35,0,0,0,3.552340878869367,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK699/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL699/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM699/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2333333333333334,"d":"1.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12370303",12,370,3,30,14,0,0,0,{"v":0,"d":"0.0"},1876.8,0,0,0,1.362,1.1,1.1,1.1,280,0,0,0,48,0,0,0,8.712028869081788,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK700/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL700/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM700/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.85,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12370383",12,370,3,38,19,0,0,0,{"v":0,"d":"0.0"},2420.7999999999997,0,0,0,1.362,1.1,1.1,1.1,361,0,0,0,62,0,0,0,28.35437548707787,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK701/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL701/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM701/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.466666666666667,"d":"2.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12390143",12,390,3,14,4,0,0,0,{"v":0,"d":"0.0"},820.8000000000001,0,0,0,1.362,1.1,1.1,1.1,123,0,0,0,21,0,0,0,0.9674366582706402,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK702/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL702/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM702/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.65,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12390183",12,390,3,18,9,0,0,0,{"v":0,"d":"0.0"},1216.8,0,0,0,1.362,1.1,1.1,1.1,182,0,0,0,31,0,0,0,3.0104597264911135,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK703/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL703/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM703/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12390233",12,390,3,23,9,0,0,0,{"v":0,"d":"0.0"},1429.2,0,0,0,1.362,1.1,1.1,1.1,213,0,0,0,37,0,0,0,4.149811244298349,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK704/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL704/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM704/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12390303",12,390,3,30,14,0,0,0,{"v":0,"d":"0.0"},1987.2,0,0,0,1.362,1.1,1.1,1.1,297,0,0,{"$f":"ROUND(N705*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R705),0)","v":0},51,0,0,0,10.074204875904245,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK705/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL705/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM705/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,1.95,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12390383",12,390,3,38,19,0,0,0,{"v":0,"d":"0.0"},2563.2000000000003,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K706*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O706),0)","v":383},{"$f":"ROUND(L706*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P706),0)","v":0},{"$f":"ROUND(M706*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q706),0)","v":0},0,66,0,0,0,33.070865125873794,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK706/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL706/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM706/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.6,"d":"2.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12410143",12,410,3,14,4,0,0,0,{"v":0,"d":"0.0"},866.4,0,0,0,1.362,1.1,1.1,1.1,129,0,0,0,22,0,0,0,1.103932317010417,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE707*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH707),0)","v":0},{"$f":"ROUND(AF707*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI707),0)","v":0},{"$f":"ROUND(AG707*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ707),0)","v":0},0,0,0,{"$f":"(AK707/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL707/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM707/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6833333333333333,"d":"0.68"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12410183",12,410,3,18,9,0,0,0,{"v":0,"d":"0.0"},1284.3999999999999,0,0,0,1.362,1.1,1.1,1.1,192,0,0,0,33,0,0,0,3.551343623753297,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK708/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL708/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM708/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3666666666666667,"d":"1.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12410233",12,410,3,23,9,0,0,0,{"v":0,"d":"0.0"},1508.6,0,0,0,1.362,1.1,1.1,1.1,225,0,0,0,39,0,0,0,4.808462066883204,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK709/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL709/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM709/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3666666666666667,"d":"1.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12410303",12,410,3,30,14,0,0,0,{"v":0,"d":"0.0"},2097.6,0,0,0,1.362,1.1,1.1,1.1,313,0,0,0,54,0,0,0,11.556350816222912,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK710/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL710/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM710/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.05,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12410383",12,410,3,38,19,0,0,0,{"v":0,"d":"0.0"},2705.6,0,0,0,1.362,1.1,1.1,1.1,404,0,0,0,69,0,0,0,37.3750417905566,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK711/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL711/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM711/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.7333333333333334,"d":"2.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12430143",12,430,3,14,4,0,0,0,{"v":0,"d":"0.0"},912,0,0,0,1.362,1.1,1.1,1.1,136,0,0,0,23,0,0,0,1.2520026171824166,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK712/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL712/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM712/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7166666666666667,"d":"0.72"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12430183",12,430,3,18,9,0,0,0,{"v":0,"d":"0.0"},1352,0,0,0,1.362,1.1,1.1,1.1,202,0,0,0,35,0,0,0,4.150917394571254,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK713/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL713/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM713/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F713=$BR$70,$C713*$BS$70,IF($F713=$BR$71,$C713*$BS$71,IF($F713=$BR$72,$C713*$BS$72,IF($F713=$BR$73,$C713*$BS$73,IF($F713=$BR$74,$C713*$BS$74,IF($F713=$BR$75,$C713*$BS$75,IF($F713=$BR$76,$C713*$BS$76,IF($F713=$BR$77,$C713*$BS$77,IF($F713=$BR$78,$C713*$BS$78,IF($F713=$BR$79,$C713*$BS$79,IF($F713=$BR$80,$C713*$BS$80,)))))))))))","v":{"v":1.4333333333333333,"d":"1.43"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12430233",12,430,3,23,9,0,0,0,{"v":0,"d":"0.0"},1588,0,0,0,1.362,1.1,1.1,1.1,237,0,0,0,41,0,0,0,5.5309561802889675,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK714/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL714/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM714/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM714*(AN714^$BO714)*($C714-14.4)*$BP714)+($BN714*AN714*AN714))","v":0},0,0,{"v":1.4333333333333333,"d":"1.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F714=$BR$70,$BT$70,IF($F714=$BR$71,$BT$71,IF($F714=$BR$72,$BT$72,IF($F714=$BR$73,$BT$73,IF($F714=$BR$74,$BT$74,IF($F714=$BR$75,$BT$75,IF($F714=$BR$76,$BT$76,IF($F714=$BR$77,$BT$77,IF($F714=$BR$78,$BT$78,IF($F714=$BR$79,$BT$79,IF($F714=$BR$80,$BT$80,)))))))))))","v":0.00080534470601597},{"$f":"IF($F714=$BR$70,$BU$70,IF($F714=$BR$71,$BU$71,IF($F714=$BR$72,$BU$72,IF($F714=$BR$73,$BU$73,IF($F714=$BR$74,$BU$74,IF($F714=$BR$75,$BU$75,IF($F714=$BR$76,$BU$76,IF($F714=$BR$77,$BU$77,IF($F714=$BR$78,$BU$78,IF($F714=$BR$79,$BU$79,IF($F714=$BR$80,$BU$80,)))))))))))","v":0.00039795050474944},{"$f":"IF($F714=$BR$70,$BV$70,IF($F714=$BR$71,$BV$71,IF($F714=$BR$72,$BV$72,IF($F714=$BR$73,$BV$73,IF($F714=$BR$74,$BV$74,IF($F714=$BR$75,$BV$75,IF($F714=$BR$76,$BV$76,IF($F714=$BR$77,$BV$77,IF($F714=$BR$78,$BV$78,IF($F714=$BR$79,$BV$79,IF($F714=$BR$80,$BV$80,)))))))))))","v":1.813864715518},{"$f":"IF($F714=$BR$70,$BW$70,IF($F714=$BR$71,$BW$71,IF($F714=$BR$72,$BW$72,IF($F714=$BR$73,$BW$73,IF($F714=$BR$74,$BW$74,IF($F714=$BR$75,$BW$75,IF($F714=$BR$76,$BW$76,IF($F714=$BR$77,$BW$77,IF($F714=$BR$78,$BW$78,IF($F714=$BR$79,$BW$79,IF($F714=$BR$80,$BW$80,)))))))))))","v":2}]
["12430303",12,430,3,30,14,0,0,0,{"v":0,"d":"0.0"},2208,0,0,0,1.362,1.1,1.1,1.1,330,0,0,0,57,0,0,0,13.16176316763117,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,{"$f":"ROUND(AK715*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL715*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM715*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK715/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL715/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM715/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.15,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12430383",12,430,3,38,19,0,0,0,{"v":0,"d":"0.0"},2848,0,0,0,1.362,1.1,1.1,1.1,425,0,0,0,73,0,0,0,42.93546253934386,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK716/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL716/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM716/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8666666666666667,"d":"2.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12450143",12,450,3,14,4,0,0,0,{"v":0,"d":"0.0"},957.6,0,0,0,1.362,1.1,1.1,1.1,143,0,0,0,25,0,0,0,1.5149671973458203,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK717/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL717/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM717/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,0.75,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12450183",12,450,3,18,9,0,0,0,{"v":0,"d":"0.0"},1419.6000000000001,0,0,0,1.362,1.1,1.1,1.1,212,0,0,0,36,0,0,0,4.5785464969271334,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK718/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL718/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM718/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12450233",12,450,3,23,9,0,0,0,{"v":0,"d":"0.0"},1667.4,0,0,0,1.362,1.1,1.1,1.1,249,0,0,0,43,0,0,0,6.319931225064794,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK719/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL719/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM719/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12450303",12,450,3,30,14,0,0,0,{"v":0,"d":"0.0"},2318.4,0,0,0,1.362,1.1,1.1,1.1,346,0,0,0,60,0,0,0,14.893650612089068,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK720/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL720/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM720/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.25,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12450383",12,450,3,38,19,0,0,0,{"v":0,"d":"0.0"},2990.4,0,0,0,1.362,1.1,1.1,1.1,446,0,0,0,77,0,0,0,48.9748151717216,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK721/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL721/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM721/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3,"d":"3.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12470143",12,470,3,14,4,0,0,0,{"v":0,"d":"0.0"},1003.2,0,0,0,1.362,1.1,1.1,1.1,150,0,0,0,26,0,0,0,1.6952388299500143,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK722/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL722/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM722/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7833333333333334,"d":"0.78"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12470183",12,470,3,18,9,0,0,0,{"v":0,"d":"0.0"},1487.2,0,0,0,1.362,1.1,1.1,1.1,222,0,0,0,38,0,0,0,5.282002407729772,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK723/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL723/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM723/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5666666666666669,"d":"1.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12470233",12,470,3,23,9,0,0,0,{"v":0,"d":"0.0"},1746.8000000000002,0,0,0,1.362,1.1,1.1,1.1,261,0,0,0,45,0,0,0,7.17800109510436,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK724/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL724/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM724/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5666666666666669,"d":"1.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12470303",12,470,3,30,14,0,0,0,{"v":0,"d":"0.0"},2428.8,0,0,0,1.362,1.1,1.1,1.1,363,0,0,0,62,0,0,0,16.35912264421196,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK725/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL725/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM725/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.35,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12470383",12,470,3,38,19,0,0,0,{"v":0,"d":"0.0"},3132.8,0,0,0,1.362,1.1,1.1,1.1,468,0,0,0,80,0,0,0,54.42345753631059,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK726/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL726/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM726/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1333333333333337,"d":"3.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
["12490143",12,490,3,14,4,0,0,0,{"v":0,"d":"0.0"},1048.8,0,0,0,1.362,1.1,1.1,1.1,157,0,0,0,27,0,0,0,1.888488986227691,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK727/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL727/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM727/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8166666666666668,"d":"0.82"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.3823338826853E-3,0.00033290816326531,1.723172227894,1]
["12490183",12,490,3,18,9,0,0,0,{"v":0,"d":"0.0"},1554.8,0,0,0,1.362,1.1,1.1,1.1,232,0,0,0,40,0,0,0,6.051288729788074,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK728/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL728/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM728/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6333333333333335,"d":"1.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12490233",12,490,3,23,9,0,0,0,{"v":0,"d":"0.0"},1826.1999999999998,0,0,0,1.362,1.1,1.1,1.1,273,0,0,0,47,0,0,0,8.107757238013036,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK729/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL729/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM729/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6333333333333335,"d":"1.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["12490303",12,490,3,30,14,0,0,0,{"v":0,"d":"0.0"},2539.2,0,0,0,1.362,1.1,1.1,1.1,379,0,0,0,{"$f":"ROUND(S730*3600/(4186*ABS($M$1-$M$2)),0)","v":65},{"$f":"ROUND(T730*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U730*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V730*3600/(4186*ABS($M$1-$M$2)),0)","v":0},18.32620505319294,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK730/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL730/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM730/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,2.45,0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00255823982887,0.00056161694684148,1.4942747715062,3]
["12490383",12,490,3,38,19,0,0,0,{"v":0,"d":"0.0"},3275.2,0,0,0,1.362,1.1,1.1,1.1,489,0,0,0,84,0,0,0,61.38349471032493,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK731/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL731/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM731/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.266666666666667,"d":"3.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.011616292894075,0.0016553227470232,1.5869346821791,1]
[{"$f":"CONCATENATE(B732,C732,E732,D732)","v":"1570143"},15,70,3,14,{"$f":"IF($E732=14,5,IF($E732=18,10,IF($E732=23,10,IF($E732=30,15,IF($E732=38,20,)))))","v":5},0,0,0,{"v":0,"d":"0.0"},100.80000000000001,0,0,0,1.362,1.1,1.1,1.1,15,0,0,0,3,0,0,0,6.4730267114827406E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK732/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL732/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM732/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.23333333333333334,"d":"0.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1570183",15,70,3,18,{"$f":"IF($E733=14,5,IF($E733=18,10,IF($E733=23,10,IF($E733=30,15,IF($E733=38,20,)))))","v":10},0,0,0,{"v":0,"d":"0.0"},165.20000000000002,0,0,0,1.362,1.1,1.1,1.1,25,0,0,0,4,0,0,0,0.012474492861344375,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK733/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL733/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM733/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4666666666666667,"d":"0.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1570233",15,70,3,23,10,0,0,0,{"v":0,"d":"0.0"},246,0,0,0,1.362,1.1,1.1,1.1,37,0,0,0,6,0,0,0,0.022820690230756533,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK734/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL734/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM734/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4666666666666667,"d":"0.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1570303",15,70,3,30,15,0,0,0,{"v":0,"d":"0.0"},309.6,0,0,0,1.362,1.1,1.1,1.1,46,0,0,0,8,0,0,0,0.008675886122333415,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK735/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL735/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM735/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["1570383",15,70,3,38,20,0,0,0,{"v":0,"d":"0.0"},383.20000000000005,0,0,0,1.362,1.1,1.1,1.1,57,0,0,0,10,0,0,0,0.04298363768350606,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK736/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL736/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM736/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9333333333333333,"d":"0.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["1580143",15,80,3,14,5,0,0,0,{"v":0,"d":"0.0"},126,0,0,0,1.362,1.1,1.1,1.1,19,0,0,{"$f":"ROUND(N737*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R737),0)","v":0},3,0,0,0,7.630927336835948E-3,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK737/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL737/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM737/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.26666666666666666,"d":"0.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1580183",15,80,3,18,10,0,0,0,{"v":0,"d":"0.0"},206.5,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K738*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O738),0)","v":31},{"$f":"ROUND(L738*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P738),0)","v":0},{"$f":"ROUND(M738*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q738),0)","v":0},0,5,0,0,0,0.020504259301806473,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK738/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL738/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM738/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5333333333333333,"d":"0.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1580233",15,80,3,23,10,0,0,0,{"v":0,"d":"0.0"},307.5,0,0,0,1.362,1.1,1.1,1.1,46,0,0,0,8,0,0,0,0.04129365705804856,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE739*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH739),0)","v":0},{"$f":"ROUND(AF739*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI739),0)","v":0},{"$f":"ROUND(AG739*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ739),0)","v":0},0,0,0,{"$f":"(AK739/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL739/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM739/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5333333333333333,"d":"0.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1580303",15,80,3,30,15,0,0,0,{"v":0,"d":"0.0"},387,0,0,0,1.362,1.1,1.1,1.1,58,0,0,0,10,0,0,0,0.015129499819799296,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK740/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL740/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM740/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["1580383",15,80,3,38,20,0,0,0,{"v":0,"d":"0.0"},479,0,0,0,1.362,1.1,1.1,1.1,71,0,0,0,12,0,0,0,0.0650706691640389,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK741/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL741/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM741/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0666666666666667,"d":"1.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["1590143",15,90,3,14,5,0,0,0,{"v":0,"d":"0.0"},151.2,0,0,0,1.362,1.1,1.1,1.1,23,0,0,0,4,0,0,0,0.014813180817340765,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK742/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL742/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM742/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.30000000000000004,"d":"0.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["1590183",15,90,3,18,10,0,0,0,{"v":0,"d":"0.0"},247.79999999999998,0,0,0,1.362,1.1,1.1,1.1,37,0,0,0,6,0,0,0,0.030981560817359595,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK743/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL743/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM743/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6000000000000001,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1590233",15,90,3,23,10,0,0,0,{"v":0,"d":"0.0"},369,0,0,0,1.362,1.1,1.1,1.1,55,0,0,0,9,0,0,0,0.05667144609694029,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK744/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL744/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM744/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6000000000000001,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["1590303",15,90,3,30,15,0,0,0,{"v":0,"d":"0.0"},464.4,0,0,0,1.362,1.1,1.1,1.1,69,0,0,0,12,0,0,0,0.02399509402200527,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK745/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL745/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM745/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["1590383",15,90,3,38,20,0,0,0,{"v":0,"d":"0.0"},574.8,0,0,0,1.362,1.1,1.1,1.1,86,0,0,0,15,0,0,0,0.10178573234014354,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK746/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL746/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM746/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2000000000000002,"d":"1.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15100143",15,100,3,14,5,0,0,0,{"v":0,"d":"0.0"},176.39999999999998,0,0,0,1.362,1.1,1.1,1.1,26,0,0,0,4,0,0,0,0.016764342481123313,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,{"$f":"ROUND(AK747*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL747*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM747*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK747/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL747/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM747/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.33333333333333337,"d":"0.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15100183",15,100,3,18,10,0,0,0,{"v":0,"d":"0.0"},289.09999999999997,0,0,0,1.362,1.1,1.1,1.1,43,0,0,0,7,0,0,0,0.0441077873235914,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK748/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL748/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM748/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6666666666666667,"d":"0.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15100233",15,100,3,23,10,0,0,0,{"v":0,"d":"0.0"},430.5,0,0,0,1.362,1.1,1.1,1.1,64,0,0,0,11,0,0,0,0.08646705339839474,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK749/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL749/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM749/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.6666666666666667,"d":"0.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15100303",15,100,3,30,15,0,0,0,{"v":0,"d":"0.0"},541.8,0,0,0,1.362,1.1,1.1,1.1,81,0,0,0,14,0,0,0,0.03559326252514379,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK750/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL750/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM750/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15100383",15,100,3,38,20,0,0,0,{"v":0,"d":"0.0"},670.5999999999999,0,0,0,1.362,1.1,1.1,1.1,100,0,0,0,17,0,0,0,0.1367499201402335,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK751/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL751/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM751/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3333333333333335,"d":"1.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15110143",15,110,3,14,5,0,0,0,{"v":0,"d":"0.0"},201.60000000000002,0,0,0,1.362,1.1,1.1,1.1,30,0,0,0,5,0,0,0,0.028057216713247447,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK752/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL752/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM752/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.3666666666666667,"d":"0.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15110183",15,110,3,18,10,0,0,0,{"v":0,"d":"0.0"},330.40000000000003,0,0,0,1.362,1.1,1.1,1.1,49,0,0,0,8,0,0,0,0.06006943924922931,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK753/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL753/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM753/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7333333333333334,"d":"0.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15110233",15,110,3,23,10,0,0,0,{"v":0,"d":"0.0"},492,0,0,0,1.362,1.1,1.1,1.1,73,0,0,0,13,0,0,0,0.12378117280594328,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK754/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL754/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM754/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7333333333333334,"d":"0.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15110303",15,110,3,30,15,0,0,0,{"v":0,"d":"0.0"},619.2,0,0,0,1.362,1.1,1.1,1.1,92,0,0,0,16,0,0,0,0.05023342091388339,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK755/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL755/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM755/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15110383",15,110,3,38,20,0,0,0,{"v":0,"d":"0.0"},766.4000000000001,0,0,0,1.362,1.1,1.1,1.1,114,0,0,0,20,0,0,0,0.19077691320730933,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK756/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL756/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM756/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4666666666666668,"d":"1.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15120143",15,120,3,14,5,0,0,0,{"v":0,"d":"0.0"},226.8,0,0,0,1.362,1.1,1.1,1.1,34,0,0,0,6,0,0,0,0.04312994644649151,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK757/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL757/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM757/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.4,"d":"0.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15120183",15,120,3,18,10,0,0,0,{"v":0,"d":"0.0"},371.7,0,0,0,1.362,1.1,1.1,1.1,55,0,0,0,9,0,0,0,0.07904094554017056,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK758/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL758/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM758/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15120233",15,120,3,23,10,0,0,0,{"v":0,"d":"0.0"},553.5,0,0,0,1.362,1.1,1.1,1.1,83,0,0,0,14,0,0,0,0.15261059094536503,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK759/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL759/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM759/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15120303",15,120,3,30,15,0,0,0,{"v":0,"d":"0.0"},696.6,0,0,0,1.362,1.1,1.1,1.1,104,0,0,0,18,0,0,0,0.06821559178775338,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK760/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL760/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM760/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2,"d":"1.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15120383",15,120,3,38,20,0,0,0,{"v":0,"d":"0.0"},862.2,0,0,0,1.362,1.1,1.1,1.1,129,0,0,0,22,0,0,0,0.2400448528256133,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK761/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL761/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM761/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6,"d":"1.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15130143",15,130,3,14,5,0,0,0,{"v":0,"d":"0.0"},252,0,0,0,1.362,1.1,1.1,1.1,38,0,0,0,{"$f":"ROUND(S762*3600/(4186*ABS($M$1-$M$2)),0)","v":7},{"$f":"ROUND(T762*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U762*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V762*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"0.0098*(($BM762*(W762^$BO762)*($C762-14.4)*$BP762)+($BN762*W762*W762))","v":0.06243391135828655},0,{"$f":"0.0098*(($BM762*(Y762^$BO762)*($C762-14.4)*$BP762)+($BN762*Y762*Y762))","v":0},{"$f":"0.0098*(($BM762*(Z762^$BO762)*($C762-14.4)*$BP762)+($BN762*Z762*Z762))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK762/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL762/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM762/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.43333333333333335,"d":"0.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15130183",15,130,3,18,10,0,0,0,{"v":0,"d":"0.0"},413,0,0,0,1.362,1.1,1.1,1.1,62,0,0,0,11,0,0,0,0.11661370499829944,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK763/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL763/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM763/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8666666666666667,"d":"0.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15130233",15,130,3,23,10,0,0,0,{"v":0,"d":"0.0"},615,0,0,0,1.362,1.1,1.1,1.1,92,0,0,0,16,0,0,0,0.20373299726951039,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK764/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL764/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM764/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8666666666666667,"d":"0.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15130303",15,130,3,30,15,0,0,0,{"v":0,"d":"0.0"},774,0,0,0,1.362,1.1,1.1,1.1,116,0,0,0,20,0,0,0,0.08983173479030017,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK765/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL765/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM765/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15130383",15,130,3,38,20,0,0,0,{"v":0,"d":"0.0"},958,0,0,0,1.362,1.1,1.1,1.1,143,0,0,0,25,0,0,0,0.31301979317857853,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK766/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL766/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM766/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.7333333333333334,"d":"1.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15150143",15,150,3,14,5,0,0,0,{"v":0,"d":"0.0"},302.4,0,0,0,1.362,1.1,1.1,1.1,45,0,0,0,8,0,0,0,0.09327051475342535,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK767/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL767/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM767/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5,"d":"0.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15150183",15,150,3,18,10,0,0,0,{"v":0,"d":"0.0"},495.59999999999997,0,0,0,1.362,1.1,1.1,1.1,74,0,0,0,13,0,0,0,0.17531029636491535,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK768/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL768/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM768/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15150233",15,150,3,23,10,0,0,0,{"v":0,"d":"0.0"},738,0,0,0,1.362,1.1,1.1,1.1,110,0,0,{"$f":"ROUND(N769*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R769),0)","v":0},19,0,0,0,0.30845786834959366,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK769/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL769/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM769/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15150303",15,150,3,30,15,0,0,0,{"v":0,"d":"0.0"},928.8,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K770*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O770),0)","v":139},{"$f":"ROUND(L770*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P770),0)","v":0},{"$f":"ROUND(M770*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q770),0)","v":0},0,24,0,0,0,0.14509939713157038,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK770/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL770/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM770/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15150383",15,150,3,38,20,0,0,0,{"v":0,"d":"0.0"},1149.6,0,0,0,1.362,1.1,1.1,1.1,172,0,0,0,30,0,0,0,0.4711562583001336,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE771*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH771),0)","v":0},{"$f":"ROUND(AF771*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI771),0)","v":0},{"$f":"ROUND(AG771*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ771),0)","v":0},0,0,0,{"$f":"(AK771/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL771/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM771/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2,"d":"2.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15170143",15,170,3,14,5,0,0,0,{"v":0,"d":"0.0"},352.79999999999995,0,0,0,1.362,1.1,1.1,1.1,53,0,0,0,9,0,0,0,0.13248023267380543,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK772/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL772/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM772/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.5666666666666667,"d":"0.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15170183",15,170,3,18,10,0,0,0,{"v":0,"d":"0.0"},578.1999999999999,0,0,0,1.362,1.1,1.1,1.1,86,0,0,0,15,0,0,0,0.24881011485076113,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK773/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL773/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM773/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1333333333333333,"d":"1.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15170233",15,170,3,23,10,0,0,0,{"v":0,"d":"0.0"},861,0,0,0,1.362,1.1,1.1,1.1,129,0,0,0,22,0,0,0,0.4400487689070514,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK774/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL774/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM774/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1333333333333333,"d":"1.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15170303",15,170,3,30,15,0,0,0,{"v":0,"d":"0.0"},1083.6,0,0,0,1.362,1.1,1.1,1.1,162,0,0,0,28,0,0,0,0.21824488717886567,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK775/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL775/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM775/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.7,"d":"1.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15170383",15,170,3,38,20,0,0,0,{"v":0,"d":"0.0"},1341.1999999999998,0,0,0,1.362,1.1,1.1,1.1,200,0,0,0,34,0,0,0,0.6414868653975905,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK776/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL776/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM776/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.2666666666666666,"d":"2.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15190143",15,190,3,14,5,0,0,0,{"v":0,"d":"0.0"},403.20000000000005,0,0,0,1.362,1.1,1.1,1.1,60,0,0,0,10,0,0,0,0.18095230333090526,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK777/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL777/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM777/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F777=$BR$70,$C777*$BS$70,IF($F777=$BR$71,$C777*$BS$71,IF($F777=$BR$72,$C777*$BS$72,IF($F777=$BR$73,$C777*$BS$73,IF($F777=$BR$74,$C777*$BS$74,IF($F777=$BR$75,$C777*$BS$75,IF($F777=$BR$76,$C777*$BS$76,IF($F777=$BR$77,$C777*$BS$77,IF($F777=$BR$78,$C777*$BS$78,IF($F777=$BR$79,$C777*$BS$79,IF($F777=$BR$80,$C777*$BS$80,)))))))))))","v":{"v":0.6333333333333334,"d":"0.63"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15190183",15,190,3,18,10,0,0,0,{"v":0,"d":"0.0"},660.8000000000001,0,0,0,1.362,1.1,1.1,1.1,99,0,0,0,17,0,0,0,0.33816340345190316,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK778/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL778/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM778/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM778*(AN778^$BO778)*($C778-14.4)*$BP778)+($BN778*AN778*AN778))","v":0},0,0,{"v":1.2666666666666668,"d":"1.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F778=$BR$70,$BT$70,IF($F778=$BR$71,$BT$71,IF($F778=$BR$72,$BT$72,IF($F778=$BR$73,$BT$73,IF($F778=$BR$74,$BT$74,IF($F778=$BR$75,$BT$75,IF($F778=$BR$76,$BT$76,IF($F778=$BR$77,$BT$77,IF($F778=$BR$78,$BT$78,IF($F778=$BR$79,$BT$79,IF($F778=$BR$80,$BT$80,)))))))))))","v":0.0014501879713726},{"$f":"IF($F778=$BR$70,$BU$70,IF($F778=$BR$71,$BU$71,IF($F778=$BR$72,$BU$72,IF($F778=$BR$73,$BU$73,IF($F778=$BR$74,$BU$74,IF($F778=$BR$75,$BU$75,IF($F778=$BR$76,$BU$76,IF($F778=$BR$77,$BU$77,IF($F778=$BR$78,$BU$78,IF($F778=$BR$79,$BU$79,IF($F778=$BR$80,$BU$80,)))))))))))","v":0.00037831632653061},{"$f":"IF($F778=$BR$70,$BV$70,IF($F778=$BR$71,$BV$71,IF($F778=$BR$72,$BV$72,IF($F778=$BR$73,$BV$73,IF($F778=$BR$74,$BV$74,IF($F778=$BR$75,$BV$75,IF($F778=$BR$76,$BV$76,IF($F778=$BR$77,$BV$77,IF($F778=$BR$78,$BV$78,IF($F778=$BR$79,$BV$79,IF($F778=$BR$80,$BV$80,)))))))))))","v":1.4868910444209},{"$f":"IF($F778=$BR$70,$BW$70,IF($F778=$BR$71,$BW$71,IF($F778=$BR$72,$BW$72,IF($F778=$BR$73,$BW$73,IF($F778=$BR$74,$BW$74,IF($F778=$BR$75,$BW$75,IF($F778=$BR$76,$BW$76,IF($F778=$BR$77,$BW$77,IF($F778=$BR$78,$BW$78,IF($F778=$BR$79,$BW$79,IF($F778=$BR$80,$BW$80,)))))))))))","v":2}]
["15190233",15,190,3,23,10,0,0,0,{"v":0,"d":"0.0"},984,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K779*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O779),0)","v":147},{"$f":"ROUND(L779*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P779),0)","v":0},{"$f":"ROUND(M779*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q779),0)","v":0},0,25,0,0,0,0.6004386147949138,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,{"$f":"ROUND(AK779*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL779*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM779*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK779/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL779/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM779/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2666666666666668,"d":"1.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15190303",15,190,3,30,15,0,0,0,{"v":0,"d":"0.0"},1238.4,0,0,0,1.362,1.1,1.1,1.1,185,0,0,0,32,0,0,0,0.311395514024296,0,0,0,0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE780*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH780),0)","v":0},{"$f":"ROUND(AF780*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI780),0)","v":0},{"$f":"ROUND(AG780*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ780),0)","v":0},0,0,0,{"$f":"(AK780/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL780/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM780/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.9000000000000001,"d":"1.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15190383",15,190,3,38,20,0,0,0,{"v":0,"d":"0.0"},1532.8000000000002,0,0,0,1.362,1.1,1.1,1.1,229,0,0,0,{"$f":"ROUND(S781*3600/(4186*ABS($M$1-$M$2)),0)","v":39},{"$f":"ROUND(T781*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U781*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V781*3600/(4186*ABS($M$1-$M$2)),0)","v":0},0.8733751135070073,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK781/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL781/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM781/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.5333333333333337,"d":"2.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15210143",15,210,3,14,5,0,0,0,{"v":0,"d":"0.0"},453.6,0,0,0,1.362,1.1,1.1,1.1,68,0,0,0,{"$f":"ROUND(S782*3600/(4186*ABS($M$1-$M$2)),0)","v":12},{"$f":"ROUND(T782*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U782*3600/(4186*ABS($M$1-$M$2)),0)","v":0},0,0.2805212841228376,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK782/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL782/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM782/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15210183",15,210,3,18,10,0,0,0,{"v":0,"d":"0.0"},743.4,0,0,0,1.362,1.1,1.1,1.1,111,0,0,0,19,0,0,0,0.44435143509720143,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK783/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL783/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM783/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4000000000000001,"d":"1.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15210233",15,210,3,23,10,0,0,0,{"v":0,"d":"0.0"},1107,0,0,0,1.362,1.1,1.1,1.1,165,0,0,0,28,0,0,0,0.7914318069544937,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK784/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL784/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM784/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4000000000000001,"d":"1.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15210303",15,210,3,30,15,0,0,0,{"v":0,"d":"0.0"},1393.2,0,0,0,1.362,1.1,1.1,1.1,208,0,0,0,36,0,0,0,0.42661108599487074,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK785/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL785/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM785/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.1,"d":"2.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15210383",15,210,3,38,20,0,0,0,{"v":0,"d":"0.0"},1724.4,0,0,0,1.362,1.1,1.1,1.1,257,0,0,0,44,0,0,0,1.1473540704526308,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK786/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL786/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM786/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8000000000000003,"d":"2.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15230143",15,230,3,14,5,0,0,0,{"v":0,"d":"0.0"},504,0,0,0,1.362,1.1,1.1,1.1,75,0,0,0,13,0,0,0,0.3574626447903286,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK787/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL787/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM787/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7666666666666667,"d":"0.77"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15230183",15,230,3,18,10,0,0,0,{"v":0,"d":"0.0"},826,0,0,0,1.362,1.1,1.1,1.1,123,0,0,0,21,0,0,0,0.5682983963281394,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK788/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL788/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM788/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5333333333333334,"d":"1.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15230233",15,230,3,23,10,0,0,0,{"v":0,"d":"0.0"},1230,0,0,0,1.362,1.1,1.1,1.1,184,0,0,0,32,0,0,0,1.0638386676140126,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK789/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL789/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM789/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5333333333333334,"d":"1.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15230303",15,230,3,30,15,0,0,0,{"v":0,"d":"0.0"},1548,0,0,0,1.362,1.1,1.1,1.1,231,0,0,0,40,0,0,0,0.5658939017026267,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK790/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL790/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM790/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.3000000000000003,"d":"2.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15230383",15,230,3,38,20,0,0,0,{"v":0,"d":"0.0"},1916,0,0,0,1.362,1.1,1.1,1.1,286,0,0,0,49,0,0,0,1.4652400940970833,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK791/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL791/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM791/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.066666666666667,"d":"3.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15250143",15,250,3,14,5,0,0,0,{"v":0,"d":"0.0"},554.4000000000001,0,0,0,1.362,1.1,1.1,1.1,83,0,0,0,14,0,0,0,0.4467638804395164,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK792/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL792/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM792/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8333333333333334,"d":"0.83"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15250183",15,250,3,18,10,0,0,0,{"v":0,"d":"0.0"},908.6,0,0,0,1.362,1.1,1.1,1.1,136,0,0,0,23,0,0,0,0.710880208943805,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK793/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL793/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM793/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6666666666666667,"d":"1.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15250233",15,250,3,23,10,0,0,0,{"v":0,"d":"0.0"},1353,0,0,0,1.362,1.1,1.1,1.1,202,0,0,0,35,0,0,0,1.3280193116086283,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,{"$f":"ROUND(AK794*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL794*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM794*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK794/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL794/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM794/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6666666666666667,"d":"1.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15250303",15,250,3,30,15,0,0,0,{"v":0,"d":"0.0"},1702.8000000000002,0,0,0,1.362,1.1,1.1,1.1,254,0,0,0,44,0,0,0,0.7311963445324051,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK795/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL795/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM795/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.5,"d":"2.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15250383",15,250,3,38,20,0,0,0,{"v":0,"d":"0.0"},2107.6000000000004,0,0,0,1.362,1.1,1.1,1.1,315,0,0,0,54,0,0,0,1.8287291099928271,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK796/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL796/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM796/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.3333333333333335,"d":"3.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15270143",15,270,3,14,{"$f":"IF($E797=14,5,IF($E797=18,10,IF($E797=23,10,IF($E797=30,15,IF($E797=38,20,)))))","v":5},0,0,0,{"v":0,"d":"0.0"},604.8,0,0,0,1.362,1.1,1.1,1.1,90,0,0,0,15,0,0,0,0.5492417717057644,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK797/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL797/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM797/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15270183",15,270,3,18,10,0,0,0,{"v":0,"d":"0.0"},991.1999999999999,0,0,0,1.362,1.1,1.1,1.1,148,0,0,0,25,0,0,0,0.8729312923780179,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK798/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL798/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM798/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.8,"d":"1.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15270233",15,270,3,23,10,0,0,0,{"v":0,"d":"0.0"},1476,0,0,0,1.362,1.1,1.1,1.1,220,0,0,0,38,0,0,0,1.6279380489986648,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK799/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL799/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM799/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.8,"d":"1.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15270303",15,270,3,30,15,0,0,0,{"v":0,"d":"0.0"},1857.6,0,0,0,1.362,1.1,1.1,1.1,277,0,0,0,48,0,0,0,0.9244268335276367,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK800/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL800/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM800/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.7,"d":"2.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15270383",15,270,3,38,20,0,0,0,{"v":0,"d":"0.0"},2299.2,0,0,0,1.362,1.1,1.1,1.1,343,0,0,{"$f":"ROUND(N801*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R801),0)","v":0},59,0,0,0,2.239415301174394,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK801/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL801/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM801/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.6,"d":"3.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15290143",15,290,3,14,5,0,0,0,{"v":0,"d":"0.0"},655.2,0,0,0,1.362,1.1,1.1,1.1,98,0,0,0,17,0,0,0,0.7430947342425075,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK802/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL802/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM802/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9666666666666667,"d":"0.97"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15290183",15,290,3,18,10,0,0,0,{"v":0,"d":"0.0"},1073.8,0,0,0,1.362,1.1,1.1,1.1,160,0,0,0,28,0,0,0,1.1139369713530598,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK803/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL803/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM803/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.9333333333333333,"d":"1.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15290233",15,290,3,23,10,0,0,0,{"v":0,"d":"0.0"},1599,0,0,0,1.362,1.1,1.1,1.1,239,0,0,0,41,0,0,0,1.9650474663589599,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK804/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL804/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM804/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.9333333333333333,"d":"1.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15290303",15,290,3,30,15,0,0,0,{"v":0,"d":"0.0"},2012.4,0,0,0,1.362,1.1,1.1,1.1,300,0,0,0,52,0,0,0,1.147454600908598,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK805/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL805/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM805/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.9,"d":"2.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15290383",15,290,3,38,20,0,0,0,{"v":0,"d":"0.0"},2490.8,0,0,0,1.362,1.1,1.1,1.1,372,0,0,0,64,0,0,0,2.698805524408733,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK806/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL806/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM806/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.8666666666666667,"d":"3.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15310143",15,310,3,14,5,0,0,0,{"v":0,"d":"0.0"},705.5999999999999,0,0,0,1.362,1.1,1.1,1.1,105,0,0,0,18,0,0,0,0.8840117194736292,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK807/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL807/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM807/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0333333333333334,"d":"1.03"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15310183",15,310,3,18,10,0,0,0,{"v":0,"d":"0.0"},1156.3999999999999,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K808*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O808),0)","v":173},0,0,0,30,0,0,0,1.3237296025760112,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK808/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL808/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM808/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.066666666666667,"d":"2.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15310233",15,310,3,23,10,0,0,0,{"v":0,"d":"0.0"},1722,0,0,0,1.362,1.1,1.1,1.1,257,0,0,0,44,0,0,0,2.3407425256061978,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK809/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL809/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM809/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.066666666666667,"d":"2.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15310303",15,310,3,30,15,0,0,0,{"v":0,"d":"0.0"},2167.2,0,0,0,1.362,1.1,1.1,1.1,323,0,0,0,56,0,0,0,1.4021136044224956,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK810/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL810/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM810/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1,"d":"3.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15310383",15,310,3,38,20,0,0,0,{"v":0,"d":"0.0"},2682.3999999999996,0,0,0,1.362,1.1,1.1,1.1,400,0,0,0,69,0,0,0,3.208330693761257,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK811/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL811/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM811/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.133333333333334,"d":"4.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15330143",15,330,3,14,5,0,0,0,{"v":0,"d":"0.0"},756,0,0,0,1.362,1.1,1.1,1.1,113,0,0,0,19,0,0,0,1.040995038400773,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK812/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL812/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM812/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15330183",15,330,3,18,10,0,0,0,{"v":0,"d":"0.0"},1239,0,0,0,1.362,1.1,1.1,1.1,185,0,0,0,32,0,0,0,1.5555094410898995,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK813/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL813/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM813/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.2,"d":"2.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15330233",15,330,3,23,10,0,0,0,{"v":0,"d":"0.0"},1845,0,0,0,1.362,1.1,1.1,1.1,275,0,0,0,{"$f":"ROUND(S814*3600/(4186*ABS($M$1-$M$2)),0)","v":47},0,0,0,2.756366830726476,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK814/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL814/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM814/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.2,"d":"2.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15330303",15,330,3,30,15,0,0,0,{"v":0,"d":"0.0"},2322,0,0,0,1.362,1.1,1.1,1.1,347,0,0,0,60,0,0,0,1.6902057845869796,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK815/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL815/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM815/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.3000000000000003,"d":"3.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15330383",15,330,3,38,20,0,0,0,{"v":0,"d":"0.0"},2874,0,0,0,1.362,1.1,1.1,1.1,429,0,0,0,74,0,0,0,3.7693549468675456,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK816/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL816/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM816/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.4,"d":"4.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15350143",15,350,3,14,5,0,0,0,{"v":0,"d":"0.0"},806.4000000000001,0,0,0,1.362,1.1,1.1,1.1,120,0,0,0,21,0,0,0,1.3272413019923863,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK817/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL817/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM817/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1666666666666667,"d":"1.17"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15350183",15,350,3,18,10,0,0,0,{"v":0,"d":"0.0"},1321.6000000000001,0,0,0,1.362,1.1,1.1,1.1,197,0,0,0,34,0,0,0,1.8099817557833695,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK818/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL818/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM818/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.3333333333333335,"d":"2.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15350233",15,350,3,23,10,0,0,0,{"v":0,"d":"0.0"},1968,0,0,0,1.362,1.1,1.1,1.1,294,0,0,0,51,0,0,0,3.3093330860106605,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK819/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL819/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM819/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.3333333333333335,"d":"2.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15350303",15,350,3,30,15,0,0,0,{"v":0,"d":"0.0"},2476.8,0,0,0,1.362,1.1,1.1,1.1,370,0,0,0,64,0,0,0,2.0135038147139803,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK820/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL820/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM820/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.5,"d":"3.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15350383",15,350,3,38,20,0,0,0,{"v":0,"d":"0.0"},3065.6000000000004,0,0,0,1.362,1.1,1.1,1.1,458,0,0,0,79,0,0,0,4.383183148962008,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK821/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL821/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM821/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.666666666666667,"d":"4.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15370143",15,370,3,14,5,0,0,0,{"v":0,"d":"0.0"},856.8,0,0,0,1.362,1.1,1.1,1.1,128,0,0,0,22,0,0,0,1.5300614161537585,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK822/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL822/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM822/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2333333333333334,"d":"1.23"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15370183",15,370,3,18,10,0,0,0,{"v":0,"d":"0.0"},1404.2,0,0,0,1.362,1.1,1.1,1.1,210,0,0,0,36,0,0,0,2.087829395802291,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK823/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL823/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM823/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.466666666666667,"d":"2.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15370233",15,370,3,23,10,0,0,0,{"v":0,"d":"0.0"},2091,0,0,0,1.362,1.1,1.1,1.1,312,0,0,0,54,0,0,0,3.8172852573811857,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK824/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL824/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM824/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.466666666666667,"d":"2.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15370303",15,370,3,30,15,0,0,0,{"v":0,"d":"0.0"},2631.6,0,0,0,1.362,1.1,1.1,1.1,393,0,0,0,68,0,0,0,2.373753450707282,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK825/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL825/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM825/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.7,"d":"3.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15370383",15,370,3,38,20,0,0,0,{"v":0,"d":"0.0"},3257.2,0,0,0,1.362,1.1,1.1,1.1,486,0,0,0,84,0,0,0,{"$f":"0.0098*(($BM826*(W826^$BO826)*($C826-14.4)*$BP826)+($BN826*W826*W826))","v":5.051067123920566},0,{"$f":"0.0098*(($BM826*(Y826^$BO826)*($C826-14.4)*$BP826)+($BN826*Y826*Y826))","v":0},{"$f":"0.0098*(($BM826*(Z826^$BO826)*($C826-14.4)*$BP826)+($BN826*Z826*Z826))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK826/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL826/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM826/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.933333333333334,"d":"4.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15390143",15,390,3,14,5,0,0,0,{"v":0,"d":"0.0"},907.2,0,0,0,1.362,1.1,1.1,1.1,135,0,0,0,23,0,0,0,1.751722546309011,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK827/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL827/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM827/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15390183",15,390,3,18,10,0,0,0,{"v":0,"d":"0.0"},1486.8,0,0,0,1.362,1.1,1.1,1.1,222,0,0,0,38,0,0,0,2.3897147715332494,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK828/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL828/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM828/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.6,"d":"2.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15390233",15,390,3,23,10,0,0,0,{"v":0,"d":"0.0"},2214,0,0,0,1.362,1.1,1.1,1.1,330,0,0,0,57,0,0,0,4.369176005656667,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK829/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL829/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM829/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.6,"d":"2.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15390303",15,390,3,30,15,0,0,0,{"v":0,"d":"0.0"},2786.4,0,0,0,1.362,1.1,1.1,1.1,416,0,0,0,72,0,0,0,2.77267555986573,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK830/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL830/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM830/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.9,"d":"3.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15390383",15,390,3,38,20,0,0,0,{"v":0,"d":"0.0"},3448.8,0,0,0,1.362,1.1,1.1,1.1,515,0,0,0,89,0,0,0,5.774210892347711,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK831/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL831/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM831/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":5.2,"d":"5.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15410143",15,410,3,14,5,0,0,0,{"v":0,"d":"0.0"},957.5999999999999,0,0,0,1.362,1.1,1.1,1.1,143,0,0,0,25,0,0,0,2.146158230867245,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK832/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL832/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM832/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3666666666666667,"d":"1.37"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
[{"$f":"CONCATENATE(B833,C833,E833,D833)","v":"15410183"},15,410,3,18,10,0,0,0,{"v":0,"d":"0.0"},1569.3999999999999,0,0,0,1.362,1.1,1.1,1.1,234,{"$f":"ROUND(L833*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P833),0)","v":0},0,{"$f":"ROUND(N833*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R833),0)","v":0},40,{"$f":"ROUND(T833*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U833*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V833*3600/(4186*ABS($M$1-$M$2)),0)","v":0},2.7162815606716206,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK833/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL833/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM833/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.7333333333333334,"d":"2.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15410233",15,410,3,23,10,0,0,0,{"v":0,"d":"0.0"},2337,0,0,0,1.362,1.1,1.1,1.1,349,0,0,0,60,0,0,0,4.966181573632571,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK834/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL834/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM834/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.7333333333333334,"d":"2.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15410303",15,410,3,30,15,0,0,0,{"v":0,"d":"0.0"},2941.2,0,0,0,1.362,1.1,1.1,1.1,439,0,0,0,76,0,0,0,3.2119678885587186,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK835/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL835/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM835/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.1,"d":"4.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15410383",15,410,3,38,20,0,0,0,{"v":0,"d":"0.0"},3640.3999999999996,0,0,0,1.362,1.1,1.1,1.1,543,0,0,0,93,0,0,0,6.458313519372723,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK836/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL836/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM836/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":5.466666666666667,"d":"5.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15430143",15,430,3,14,5,0,0,0,{"v":0,"d":"0.0"},1008,0,0,0,1.362,1.1,1.1,1.1,150,0,0,0,26,0,0,0,2.4207886290377654,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK837/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL837/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM837/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4333333333333333,"d":"1.43"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15430183",15,430,3,18,10,0,0,0,{"v":0,"d":"0.0"},1652,0,0,0,1.362,1.1,1.1,1.1,247,0,0,0,42,0,0,0,3.0681561899556726,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK838/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL838/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM838/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8666666666666667,"d":"2.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15430233",15,430,3,23,10,0,0,0,{"v":0,"d":"0.0"},2460,0,0,0,1.362,1.1,1.1,1.1,367,0,0,0,63,0,0,0,5.609446680075872,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK839/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL839/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM839/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8666666666666667,"d":"2.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15430303",15,430,3,30,15,0,0,0,{"v":0,"d":"0.0"},3096,0,0,0,1.362,1.1,1.1,1.1,462,0,0,0,79,0,0,0,3.6120662551223797,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK840/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL840/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM840/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.3,"d":"4.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15430383",15,430,3,38,20,0,0,0,{"v":0,"d":"0.0"},3832,0,0,0,1.362,1.1,1.1,1.1,572,0,0,0,98,0,0,0,7.288656273128006,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK841/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL841/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM841/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F841=$BR$70,$C841*$BS$70,IF($F841=$BR$71,$C841*$BS$71,IF($F841=$BR$72,$C841*$BS$72,IF($F841=$BR$73,$C841*$BS$73,IF($F841=$BR$74,$C841*$BS$74,IF($F841=$BR$75,$C841*$BS$75,IF($F841=$BR$76,$C841*$BS$76,IF($F841=$BR$77,$C841*$BS$77,IF($F841=$BR$78,$C841*$BS$78,IF($F841=$BR$79,$C841*$BS$79,IF($F841=$BR$80,$C841*$BS$80,)))))))))))","v":{"v":5.733333333333333,"d":"5.73"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15450143",15,450,3,14,5,0,0,0,{"v":0,"d":"0.0"},1058.4,0,0,0,1.362,1.1,1.1,1.1,158,0,0,0,27,0,0,0,2.7169438657297116,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK842/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL842/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM842/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM842*(AN842^$BO842)*($C842-14.4)*$BP842)+($BN842*AN842*AN842))","v":0},0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F842=$BR$70,$BT$70,IF($F842=$BR$71,$BT$71,IF($F842=$BR$72,$BT$72,IF($F842=$BR$73,$BT$73,IF($F842=$BR$74,$BT$74,IF($F842=$BR$75,$BT$75,IF($F842=$BR$76,$BT$76,IF($F842=$BR$77,$BT$77,IF($F842=$BR$78,$BT$78,IF($F842=$BR$79,$BT$79,IF($F842=$BR$80,$BT$80,)))))))))))","v":0.00080534470601597},{"$f":"IF($F842=$BR$70,$BU$70,IF($F842=$BR$71,$BU$71,IF($F842=$BR$72,$BU$72,IF($F842=$BR$73,$BU$73,IF($F842=$BR$74,$BU$74,IF($F842=$BR$75,$BU$75,IF($F842=$BR$76,$BU$76,IF($F842=$BR$77,$BU$77,IF($F842=$BR$78,$BU$78,IF($F842=$BR$79,$BU$79,IF($F842=$BR$80,$BU$80,)))))))))))","v":0.00039795050474944},{"$f":"IF($F842=$BR$70,$BV$70,IF($F842=$BR$71,$BV$71,IF($F842=$BR$72,$BV$72,IF($F842=$BR$73,$BV$73,IF($F842=$BR$74,$BV$74,IF($F842=$BR$75,$BV$75,IF($F842=$BR$76,$BV$76,IF($F842=$BR$77,$BV$77,IF($F842=$BR$78,$BV$78,IF($F842=$BR$79,$BV$79,IF($F842=$BR$80,$BV$80,)))))))))))","v":1.813864715518},{"$f":"IF($F842=$BR$70,$BW$70,IF($F842=$BR$71,$BW$71,IF($F842=$BR$72,$BW$72,IF($F842=$BR$73,$BW$73,IF($F842=$BR$74,$BW$74,IF($F842=$BR$75,$BW$75,IF($F842=$BR$76,$BW$76,IF($F842=$BR$77,$BW$77,IF($F842=$BR$78,$BW$78,IF($F842=$BR$79,$BW$79,IF($F842=$BR$80,$BW$80,)))))))))))","v":2}]
["15450183",15,450,3,18,10,0,0,0,{"v":0,"d":"0.0"},1734.6000000000001,0,0,0,1.362,1.1,1.1,1.1,259,0,0,0,45,0,0,0,3.563125901384955,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK843/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL843/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM843/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3,"d":"3.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15450233",15,450,3,23,10,0,0,0,{"v":0,"d":"0.0"},2583,0,0,0,1.362,1.1,1.1,1.1,386,0,0,0,66,0,0,0,6.300086889127907,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK844/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL844/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM844/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3,"d":"3.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15450303",15,450,3,30,15,0,0,0,{"v":0,"d":"0.0"},3250.8,0,0,0,1.362,1.1,1.1,1.1,485,0,0,0,83,0,0,0,4.129959460083961,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK845/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL845/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM845/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.5,"d":"4.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15450383",15,450,3,38,20,0,0,0,{"v":0,"d":"0.0"},4023.6000000000004,0,0,0,1.362,1.1,1.1,1.1,601,0,0,0,{"$f":"ROUND(S846*3600/(4186*ABS($M$1-$M$2)),0)","v":103},0,0,0,8.177503233010215,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK846/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL846/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM846/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6,"d":"6.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15470143",15,470,3,14,5,0,0,0,{"v":0,"d":"0.0"},1108.8000000000002,0,0,0,1.362,1.1,1.1,1.1,166,0,0,0,29,0,0,0,3.2348509864346173,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK847/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL847/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM847/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5666666666666669,"d":"1.57"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15470183",15,470,3,18,10,0,0,0,{"v":0,"d":"0.0"},1817.2,0,0,0,1.362,1.1,1.1,1.1,271,0,0,0,47,0,0,0,3.975456738368132,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK848/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL848/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM848/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1333333333333337,"d":"3.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15470233",15,470,3,23,10,0,0,0,{"v":0,"d":"0.0"},2706,0,0,0,1.362,1.1,1.1,1.1,404,0,0,0,69,0,0,0,7.039190697740161,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK849/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL849/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM849/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1333333333333337,"d":"3.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15470303",15,470,3,30,15,0,0,0,{"v":0,"d":"0.0"},3405.6000000000004,0,0,0,1.362,1.1,1.1,1.1,508,0,0,0,87,0,0,0,4.692932507588133,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK850/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL850/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM850/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.7,"d":"4.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15470383",15,470,3,38,20,0,0,0,{"v":0,"d":"0.0"},4215.200000000001,0,0,0,1.362,1.1,1.1,1.1,629,0,0,0,108,0,0,0,9.12590956794999,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK851/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL851/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM851/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6.2666666666666675,"d":"6.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["15490143",15,490,3,14,5,0,0,0,{"v":0,"d":"0.0"},1159.1999999999998,0,0,0,1.362,1.1,1.1,1.1,173,0,0,0,30,0,0,0,3.590893784057421,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK852/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL852/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM852/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6333333333333335,"d":"1.63"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00080534470601597,0.00039795050474944,1.813864715518,2]
["15490183",15,490,3,18,10,0,0,0,{"v":0,"d":"0.0"},1899.8,0,0,0,1.362,1.1,1.1,1.1,284,0,0,0,49,0,0,0,4.415055285381012,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK853/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL853/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM853/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.266666666666667,"d":"3.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15490233",15,490,3,23,10,0,0,0,{"v":0,"d":"0.0"},2829,0,0,0,1.362,1.1,1.1,1.1,422,0,0,0,73,0,0,0,7.990160426129281,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK854/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL854/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM854/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.266666666666667,"d":"3.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["15490303",15,490,3,30,15,0,0,0,{"v":0,"d":"0.0"},3560.3999999999996,0,0,0,1.362,1.1,1.1,1.1,531,0,0,0,91,0,0,0,5.302607285836738,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK855/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL855/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM855/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.9,"d":"4.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["15490383",15,490,3,38,20,0,0,0,{"v":0,"d":"0.0"},4406.799999999999,0,0,0,1.362,1.1,1.1,1.1,658,0,0,0,113,0,0,0,10.134899360813293,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK856/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL856/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM856/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6.533333333333334,"d":"6.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["2070143",20,70,3,14,{"$f":"IF($E857=23,10,IF($E857=30,15,IF($E857=38,20,)))","v":0},0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",{"$f":"ROUND(L857*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P857),0)","v":0},{"$f":"ROUND(M857*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q857),0)","v":0},0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE857*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH857),0)","v":0},{"$f":"ROUND(AF857*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI857),0)","v":0},{"$f":"ROUND(AG857*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ857),0)","v":0},{"$f":"ROUND(AK857*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL857*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM857*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK857/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL857/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM857/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
[{"$f":"CONCATENATE(B858,C858,E858,D858)","v":"2070183"},20,70,3,18,{"$f":"IF($E858=23,10,IF($E858=30,15,IF($E858=38,20,)))","v":0},0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",{"$f":"ROUND(L858*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P858),0)","v":0},{"$f":"ROUND(M858*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q858),0)","v":0},{"$f":"ROUND(N858*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R858),0)","v":0},"-",{"$f":"ROUND(T858*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U858*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V858*3600/(4186*ABS($M$1-$M$2)),0)","v":0},"-","-","-","-",0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE858*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH858),0)","v":0},{"$f":"ROUND(AF858*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI858),0)","v":0},{"$f":"ROUND(AG858*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ858),0)","v":0},{"$f":"ROUND(AK858*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL858*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM858*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK858/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL858/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM858/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["2070233",20,70,3,23,10,0,0,0,{"v":0,"d":"0.0"},264.40000000000003,0,0,0,1.362,1.1,1.1,1.1,39,0,0,0,{"$f":"ROUND(S859*3600/(4186*ABS($M$1-$M$2)),0)","v":7},0,0,0,{"$f":"0.0098*(($BM859*(W859^$BO859)*($C859-14.4)*$BP859)+($BN859*W859*W859))","v":0.02871311916111778},0,{"$f":"0.0098*(($BM859*(Y859^$BO859)*($C859-14.4)*$BP859)+($BN859*Y859*Y859))","v":0},{"$f":"0.0098*(($BM859*(Z859^$BO859)*($C859-14.4)*$BP859)+($BN859*Z859*Z859))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK859/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL859/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM859/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM859*(AN859^$BO859)*($C859-14.4)*$BP859)+($BN859*AN859*AN859))","v":0},0,0,{"v":0.4666666666666667,"d":"0.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["2070303",20,70,3,30,15,0,0,0,{"v":0,"d":"0.0"},351.20000000000005,0,0,0,1.362,1.1,1.1,1.1,52,0,0,0,9,0,0,0,0.010692124129083854,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK860/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL860/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM860/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.7000000000000001,"d":"0.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["2070383",20,70,3,38,20,0,0,0,{"v":0,"d":"0.0"},491.6,0,0,0,1.362,1.1,1.1,1.1,73,0,0,0,13,0,0,0,0.061645085901544945,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK861/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL861/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM861/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9333333333333333,"d":"0.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["2080143",20,80,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK862/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL862/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM862/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["2080183",20,80,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK863/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL863/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM863/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["2080233",20,80,3,23,10,0,0,0,{"v":0,"d":"0.0"},330.5,0,0,0,1.362,1.1,1.1,1.1,49,0,0,0,8,0,0,0,{"$f":"0.0098*(($BM864*(W864^$BO864)*($C864-14.4)*$BP864)+($BN864*W864*W864))","v":0.04129365705804856},0,{"$f":"0.0098*(($BM864*(Y864^$BO864)*($C864-14.4)*$BP864)+($BN864*Y864*Y864))","v":0},{"$f":"0.0098*(($BM864*(Z864^$BO864)*($C864-14.4)*$BP864)+($BN864*Z864*Z864))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK864/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL864/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM864/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM864*(AN864^$BO864)*($C864-14.4)*$BP864)+($BN864*AN864*AN864))","v":0},0,0,{"v":0.5333333333333333,"d":"0.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["2080303",20,80,3,30,15,0,0,0,{"v":0,"d":"0.0"},439,0,0,0,1.362,1.1,1.1,1.1,66,0,0,0,11,0,0,0,0.017915381643047696,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK865/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL865/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM865/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["2080383",20,80,3,38,20,0,0,0,{"v":0,"d":"0.0"},614.5,0,0,0,1.362,1.1,1.1,1.1,92,0,0,0,16,0,0,0,0.09661965107481238,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK866/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL866/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM866/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.0666666666666667,"d":"1.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["2090143",20,90,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK867/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL867/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM867/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["2090183",20,90,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK868/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL868/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM868/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["2090233",20,90,3,23,10,0,0,0,{"v":0,"d":"0.0"},396.59999999999997,0,0,0,1.362,1.1,1.1,1.1,59,0,0,0,10,0,0,0,{"$f":"0.0098*(($BM869*(W869^$BO869)*($C869-14.4)*$BP869)+($BN869*W869*W869))","v":0.06630228846578327},0,{"$f":"0.0098*(($BM869*(Y869^$BO869)*($C869-14.4)*$BP869)+($BN869*Y869*Y869))","v":0},{"$f":"0.0098*(($BM869*(Z869^$BO869)*($C869-14.4)*$BP869)+($BN869*Z869*Z869))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK869/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL869/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM869/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM869*(AN869^$BO869)*($C869-14.4)*$BP869)+($BN869*AN869*AN869))","v":0},0,0,{"v":0.6000000000000001,"d":"0.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["2090303",20,90,3,30,15,0,0,0,{"v":0,"d":"0.0"},526.8,0,0,0,1.362,1.1,1.1,1.1,79,0,0,0,14,0,0,0,0.031535493547618004,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK870/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL870/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM870/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":0.9,"d":"0.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["2090383",20,90,3,38,20,0,0,0,{"v":0,"d":"0.0"},737.4,0,0,0,1.362,1.1,1.1,1.1,110,0,0,0,19,0,0,0,0.1408471068466651,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK871/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL871/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM871/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2000000000000002,"d":"1.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20100143",20,100,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK872/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL872/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM872/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20100183",20,100,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK873/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL873/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM873/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20100233",20,100,3,23,10,0,0,0,{"v":0,"d":"0.0"},462.7,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K874*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O874),0)","v":69},0,0,0,12,0,0,0,{"$f":"0.0098*(($BM874*(W874^$BO874)*($C874-14.4)*$BP874)+($BN874*W874*W874))","v":0.09843306235408848},0,{"$f":"0.0098*(($BM874*(Y874^$BO874)*($C874-14.4)*$BP874)+($BN874*Y874*Y874))","v":0},{"$f":"0.0098*(($BM874*(Z874^$BO874)*($C874-14.4)*$BP874)+($BN874*Z874*Z874))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK874/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL874/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM874/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM874*(AN874^$BO874)*($C874-14.4)*$BP874)+($BN874*AN874*AN874))","v":0},0,0,{"v":0.6666666666666667,"d":"0.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20100303",20,100,3,30,15,0,0,0,{"v":0,"d":"0.0"},614.5999999999999,0,0,0,1.362,1.1,1.1,1.1,92,0,0,0,16,0,0,0,0.04509620594543746,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK875/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL875/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM875/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20100383",20,100,3,38,20,0,0,0,{"v":0,"d":"0.0"},860.3,0,0,0,1.362,1.1,1.1,1.1,128,0,0,0,22,0,0,0,0.1948776294078419,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK876/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL876/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM876/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3333333333333335,"d":"1.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20110143",20,110,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK877/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL877/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM877/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20110183",20,110,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK878/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL878/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM878/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20110233",20,110,3,23,10,0,0,0,{"v":0,"d":"0.0"},528.8000000000001,0,0,0,1.362,1.1,1.1,1.1,79,0,0,0,14,0,0,0,{"$f":"0.0098*(($BM879*(W879^$BO879)*($C879-14.4)*$BP879)+($BN879*W879*W879))","v":0.13822764388614486},0,{"$f":"0.0098*(($BM879*(Y879^$BO879)*($C879-14.4)*$BP879)+($BN879*Y879*Y879))","v":0},{"$f":"0.0098*(($BM879*(Z879^$BO879)*($C879-14.4)*$BP879)+($BN879*Z879*Z879))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK879/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL879/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM879/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM879*(AN879^$BO879)*($C879-14.4)*$BP879)+($BN879*AN879*AN879))","v":0},0,0,{"v":0.7333333333333334,"d":"0.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20110303",20,110,3,30,15,0,0,0,{"v":0,"d":"0.0"},702.4000000000001,0,0,0,1.362,1.1,1.1,1.1,105,0,0,0,18,0,0,0,0.06189021216630829,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK880/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL880/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM880/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.1,"d":"1.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20110383",20,110,3,38,20,0,0,0,{"v":0,"d":"0.0"},983.2,0,0,0,1.362,1.1,1.1,1.1,147,0,0,0,25,0,0,0,0.25921307002340205,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK881/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL881/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM881/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.4666666666666668,"d":"1.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20120143",20,120,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK882/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL882/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM882/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20120183",20,120,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK883/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL883/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM883/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20120233",20,120,3,23,10,0,0,0,{"v":0,"d":"0.0"},594.9,0,0,0,1.362,1.1,1.1,1.1,89,0,0,0,15,0,0,0,{"$f":"0.0098*(($BM884*(W884^$BO884)*($C884-14.4)*$BP884)+($BN884*W884*W884))","v":0.16912633356838286},0,{"$f":"0.0098*(($BM884*(Y884^$BO884)*($C884-14.4)*$BP884)+($BN884*Y884*Y884))","v":0},{"$f":"0.0098*(($BM884*(Z884^$BO884)*($C884-14.4)*$BP884)+($BN884*Z884*Z884))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK884/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL884/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM884/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM884*(AN884^$BO884)*($C884-14.4)*$BP884)+($BN884*AN884*AN884))","v":0},0,0,{"v":0.8,"d":"0.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20120303",20,120,3,30,15,0,0,0,{"v":0,"d":"0.0"},790.2,0,0,0,1.362,1.1,1.1,1.1,118,0,0,0,20,0,0,0,0.08221243001490929,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK885/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL885/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM885/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.2,"d":"1.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20120383",20,120,3,38,20,0,0,0,{"v":0,"d":"0.0"},1106.1000000000001,0,0,0,1.362,1.1,1.1,1.1,165,0,0,0,28,0,0,0,0.33431656458767134,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK886/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL886/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM886/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.6,"d":"1.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20130143",20,130,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK887/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL887/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM887/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20130183",20,130,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK888/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL888/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM888/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20130233",20,130,3,23,10,0,0,0,{"v":0,"d":"0.0"},661,0,0,0,1.362,1.1,1.1,1.1,99,0,0,0,17,0,0,0,{"$f":"0.0098*(($BM889*(W889^$BO889)*($C889-14.4)*$BP889)+($BN889*W889*W889))","v":0.22298392647517085},0,{"$f":"0.0098*(($BM889*(Y889^$BO889)*($C889-14.4)*$BP889)+($BN889*Y889*Y889))","v":0},{"$f":"0.0098*(($BM889*(Z889^$BO889)*($C889-14.4)*$BP889)+($BN889*Z889*Z889))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK889/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL889/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM889/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM889*(AN889^$BO889)*($C889-14.4)*$BP889)+($BN889*AN889*AN889))","v":0},0,0,{"v":0.8666666666666667,"d":"0.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20130303",20,130,3,30,15,0,0,0,{"v":0,"d":"0.0"},878,0,0,0,1.362,1.1,1.1,1.1,131,0,0,0,23,0,0,0,0.11506177947269977,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK890/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL890/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM890/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.3,"d":"1.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20130383",20,130,3,38,20,0,0,0,{"v":0,"d":"0.0"},1229,0,0,0,1.362,1.1,1.1,1.1,183,0,0,0,31,0,0,0,0.4206194033522489,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK891/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL891/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM891/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.7333333333333334,"d":"1.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20150143",20,150,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK892/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL892/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM892/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20150183",20,150,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK893/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL893/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM893/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20150233",20,150,3,23,10,0,0,0,{"v":0,"d":"0.0"},793.1999999999999,0,0,0,1.362,1.1,1.1,1.1,118,0,0,0,20,0,0,0,{"$f":"0.0098*(($BM894*(W894^$BO894)*($C894-14.4)*$BP894)+($BN894*W894*W894))","v":0.33294207077150206},0,{"$f":"0.0098*(($BM894*(Y894^$BO894)*($C894-14.4)*$BP894)+($BN894*Y894*Y894))","v":0},{"$f":"0.0098*(($BM894*(Z894^$BO894)*($C894-14.4)*$BP894)+($BN894*Z894*Z894))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK894/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL894/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM894/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM894*(AN894^$BO894)*($C894-14.4)*$BP894)+($BN894*AN894*AN894))","v":0},0,0,{"v":1,"d":"1.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20150303",20,150,3,30,15,0,0,0,{"v":0,"d":"0.0"},1053.6,0,0,0,1.362,1.1,1.1,1.1,157,0,0,0,27,0,0,0,0.1787454830950581,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK895/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL895/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM895/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.5,"d":"1.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20150383",20,150,3,38,20,0,0,0,{"v":0,"d":"0.0"},1474.8,0,0,0,1.362,1.1,1.1,1.1,220,0,0,0,38,0,0,0,0.6518660650687568,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK896/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL896/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM896/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2,"d":"2.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20170143",20,170,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK897/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL897/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM897/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20170183",20,170,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK898/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL898/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM898/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20170233",20,170,3,23,10,0,0,0,{"v":0,"d":"0.0"},925.4,0,0,0,1.362,1.1,1.1,1.1,138,0,0,0,24,0,0,0,{"$f":"0.0098*(($BM899*(W899^$BO899)*($C899-14.4)*$BP899)+($BN899*W899*W899))","v":0.5009208792799289},0,{"$f":"0.0098*(($BM899*(Y899^$BO899)*($C899-14.4)*$BP899)+($BN899*Y899*Y899))","v":0},{"$f":"0.0098*(($BM899*(Z899^$BO899)*($C899-14.4)*$BP899)+($BN899*Z899*Z899))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK899/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL899/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM899/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM899*(AN899^$BO899)*($C899-14.4)*$BP899)+($BN899*AN899*AN899))","v":0},0,0,{"v":1.1333333333333333,"d":"1.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20170303",20,170,3,30,15,0,0,0,{"v":0,"d":"0.0"},1229.1999999999998,0,0,0,1.362,1.1,1.1,1.1,183,0,0,0,31,0,0,0,0.26133191650600074,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK900/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL900/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM900/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":1.7,"d":"1.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20170383",20,170,3,38,20,0,0,0,{"v":0,"d":"0.0"},1720.6,0,0,0,1.362,1.1,1.1,1.1,257,0,0,0,44,0,0,0,0.9139989748016064,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK901/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL901/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM901/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.2666666666666666,"d":"2.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20190143",20,190,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK902/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL902/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM902/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20190183",20,190,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK903/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL903/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM903/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20190233",20,190,3,23,10,0,0,0,{"v":0,"d":"0.0"},1057.6000000000001,0,0,0,1.362,1.1,1.1,1.1,158,0,0,0,27,0,0,0,{"$f":"0.0098*(($BM904*(W904^$BO904)*($C904-14.4)*$BP904)+($BN904*W904*W904))","v":0.6733387379849093},0,{"$f":"0.0098*(($BM904*(Y904^$BO904)*($C904-14.4)*$BP904)+($BN904*Y904*Y904))","v":0},{"$f":"0.0098*(($BM904*(Z904^$BO904)*($C904-14.4)*$BP904)+($BN904*Z904*Z904))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK904/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL904/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM904/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM904*(AN904^$BO904)*($C904-14.4)*$BP904)+($BN904*AN904*AN904))","v":0},0,0,{"v":1.2666666666666668,"d":"1.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20190303",20,190,3,30,15,0,0,0,{"v":0,"d":"0.0"},1404.8000000000002,0,0,0,1.362,1.1,1.1,1.1,210,0,0,0,36,0,0,0,0.38357092709367463,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK905/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL905/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM905/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"$f":"IF($F905=$BR$70,$C905*$BS$70,IF($F905=$BR$71,$C905*$BS$71,IF($F905=$BR$72,$C905*$BS$72,IF($F905=$BR$73,$C905*$BS$73,IF($F905=$BR$74,$C905*$BS$74,IF($F905=$BR$75,$C905*$BS$75,IF($F905=$BR$76,$C905*$BS$76,IF($F905=$BR$77,$C905*$BS$77,IF($F905=$BR$78,$C905*$BS$78,IF($F905=$BR$79,$C905*$BS$79,IF($F905=$BR$80,$C905*$BS$80,)))))))))))","v":{"v":1.9000000000000001,"d":"1.90"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20190383",20,190,3,38,20,0,0,0,{"v":0,"d":"0.0"},1966.4,0,0,0,1.362,1.1,1.1,1.1,294,0,0,0,51,0,0,0,1.2623145450208735,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK906/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL906/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM906/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.5333333333333337,"d":"2.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F906=$BR$70,$BT$70,IF($F906=$BR$71,$BT$71,IF($F906=$BR$72,$BT$72,IF($F906=$BR$73,$BT$73,IF($F906=$BR$74,$BT$74,IF($F906=$BR$75,$BT$75,IF($F906=$BR$76,$BT$76,IF($F906=$BR$77,$BT$77,IF($F906=$BR$78,$BT$78,IF($F906=$BR$79,$BT$79,IF($F906=$BR$80,$BT$80,)))))))))))","v":1.6730950035507E-3},{"$f":"IF($F906=$BR$70,$BU$70,IF($F906=$BR$71,$BU$71,IF($F906=$BR$72,$BU$72,IF($F906=$BR$73,$BU$73,IF($F906=$BR$74,$BU$74,IF($F906=$BR$75,$BU$75,IF($F906=$BR$76,$BU$76,IF($F906=$BR$77,$BU$77,IF($F906=$BR$78,$BU$78,IF($F906=$BR$79,$BU$79,IF($F906=$BR$80,$BU$80,)))))))))))","v":0.00032929523945446},{"$f":"IF($F906=$BR$70,$BV$70,IF($F906=$BR$71,$BV$71,IF($F906=$BR$72,$BV$72,IF($F906=$BR$73,$BV$73,IF($F906=$BR$74,$BV$74,IF($F906=$BR$75,$BV$75,IF($F906=$BR$76,$BV$76,IF($F906=$BR$77,$BV$77,IF($F906=$BR$78,$BV$78,IF($F906=$BR$79,$BV$79,IF($F906=$BR$80,$BV$80,)))))))))))","v":1.3691788367472},{"$f":"IF($F906=$BR$70,$BW$70,IF($F906=$BR$71,$BW$71,IF($F906=$BR$72,$BW$72,IF($F906=$BR$73,$BW$73,IF($F906=$BR$74,$BW$74,IF($F906=$BR$75,$BW$75,IF($F906=$BR$76,$BW$76,IF($F906=$BR$77,$BW$77,IF($F906=$BR$78,$BW$78,IF($F906=$BR$79,$BW$79,IF($F906=$BR$80,$BW$80,)))))))))))","v":2}]
["20210143",20,210,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK907/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL907/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM907/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20210183",20,210,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK908/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL908/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM908/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20210233",20,210,3,23,10,0,0,0,{"v":0,"d":"0.0"},1189.8,0,0,0,1.362,1.1,1.1,1.1,178,0,0,0,31,0,0,0,{"$f":"0.0098*(($BM909*(W909^$BO909)*($C909-14.4)*$BP909)+($BN909*W909*W909))","v":0.9209266407865357},0,{"$f":"0.0098*(($BM909*(Y909^$BO909)*($C909-14.4)*$BP909)+($BN909*Y909*Y909))","v":0},{"$f":"0.0098*(($BM909*(Z909^$BO909)*($C909-14.4)*$BP909)+($BN909*Z909*Z909))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK909/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL909/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM909/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM909*(AN909^$BO909)*($C909-14.4)*$BP909)+($BN909*AN909*AN909))","v":0},0,0,{"v":1.4000000000000001,"d":"1.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20210303",20,210,3,30,15,0,0,0,{"v":0,"d":"0.0"},1580.4,0,0,0,1.362,1.1,1.1,1.1,236,0,0,0,41,0,0,0,0.5370100211636012,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK910/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL910/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM910/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.1,"d":"2.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20210383",20,210,3,38,20,0,0,0,{"v":0,"d":"0.0"},2212.2000000000003,0,0,0,1.362,1.1,1.1,1.1,330,0,0,0,57,0,0,0,1.6369778933082488,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK911/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL911/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM911/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.8000000000000003,"d":"2.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20230143",20,230,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK912/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL912/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM912/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20230183",20,230,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK913/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL913/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM913/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20230233",20,230,3,23,10,0,0,0,{"v":0,"d":"0.0"},1322,0,0,0,1.362,1.1,1.1,1.1,197,0,0,0,34,0,0,0,{"$f":"0.0098*(($BM914*(W914^$BO914)*($C914-14.4)*$BP914)+($BN914*W914*W914))","v":1.1643217251099356},0,{"$f":"0.0098*(($BM914*(Y914^$BO914)*($C914-14.4)*$BP914)+($BN914*Y914*Y914))","v":0},{"$f":"0.0098*(($BM914*(Z914^$BO914)*($C914-14.4)*$BP914)+($BN914*Z914*Z914))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK914/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL914/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM914/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM914*(AN914^$BO914)*($C914-14.4)*$BP914)+($BN914*AN914*AN914))","v":0},0,0,{"v":1.5333333333333334,"d":"1.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20230303",20,230,3,30,15,0,0,0,{"v":0,"d":"0.0"},1756,0,0,0,1.362,1.1,1.1,1.1,262,0,0,0,45,0,0,0,0.6970178290823396,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK915/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL915/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM915/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.3000000000000003,"d":"2.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20230383",20,230,3,38,20,0,0,0,{"v":0,"d":"0.0"},2458,0,0,0,1.362,1.1,1.1,1.1,367,0,0,0,63,0,0,0,2.068909268333964,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK916/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL916/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM916/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.066666666666667,"d":"3.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20250143",20,250,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK917/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL917/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM917/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20250183",20,250,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK918/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL918/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM918/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20250233",20,250,3,23,10,0,0,0,{"v":0,"d":"0.0"},1454.2,0,0,0,1.362,1.1,1.1,1.1,217,0,0,0,37,0,0,0,{"$f":"0.0098*(($BM919*(W919^$BO919)*($C919-14.4)*$BP919)+($BN919*W919*W919))","v":1.4425520735799477},0,{"$f":"0.0098*(($BM919*(Y919^$BO919)*($C919-14.4)*$BP919)+($BN919*Y919*Y919))","v":0},{"$f":"0.0098*(($BM919*(Z919^$BO919)*($C919-14.4)*$BP919)+($BN919*Z919*Z919))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK919/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL919/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM919/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM919*(AN919^$BO919)*($C919-14.4)*$BP919)+($BN919*AN919*AN919))","v":0},0,0,{"v":1.6666666666666667,"d":"1.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20250303",20,250,3,30,15,0,0,0,{"v":0,"d":"0.0"},1931.6000000000001,0,0,0,1.362,1.1,1.1,1.1,288,0,0,0,50,0,0,0,0.9167602414940689,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK920/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL920/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM920/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.5,"d":"2.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20250383",20,250,3,38,20,0,0,0,{"v":0,"d":"0.0"},2703.8,0,0,0,1.362,1.1,1.1,1.1,404,0,0,0,69,0,0,0,2.5602319449782045,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK921/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL921/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM921/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.3333333333333335,"d":"3.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20270143",20,270,3,14,{"$f":"IF($E922=23,10,IF($E922=30,15,IF($E922=38,20,)))","v":0},0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK922/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL922/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM922/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20270183",20,270,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK923/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL923/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM923/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20270233",20,270,3,23,10,0,0,0,{"v":0,"d":"0.0"},1586.3999999999999,0,0,0,1.362,1.1,1.1,1.1,237,0,0,0,41,0,0,0,{"$f":"0.0098*(($BM924*(W924^$BO924)*($C924-14.4)*$BP924)+($BN924*W924*W924))","v":1.8228983256580191},0,{"$f":"0.0098*(($BM924*(Y924^$BO924)*($C924-14.4)*$BP924)+($BN924*Y924*Y924))","v":0},{"$f":"0.0098*(($BM924*(Z924^$BO924)*($C924-14.4)*$BP924)+($BN924*Z924*Z924))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK924/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL924/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM924/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM924*(AN924^$BO924)*($C924-14.4)*$BP924)+($BN924*AN924*AN924))","v":0},0,0,{"v":1.8,"d":"1.80"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20270303",20,270,3,30,15,0,0,0,{"v":0,"d":"0.0"},2107.2,0,0,0,1.362,1.1,1.1,1.1,315,0,0,0,54,0,0,0,1.138580241751938,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK925/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL925/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM925/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.7,"d":"2.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20270383",20,270,3,38,20,0,0,0,{"v":0,"d":"0.0"},2949.6,0,0,0,1.362,1.1,1.1,1.1,440,0,0,0,76,0,0,0,3.170069869373425,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK926/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL926/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM926/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.6,"d":"3.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20290143",20,290,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK927/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL927/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM927/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20290183",20,290,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK928/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL928/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM928/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20290233",20,290,3,23,10,0,0,0,{"v":0,"d":"0.0"},1718.6000000000001,0,0,0,1.362,1.1,1.1,1.1,257,0,0,0,44,0,0,0,{"$f":"0.0098*(($BM929*(W929^$BO929)*($C929-14.4)*$BP929)+($BN929*W929*W929))","v":2.1828558675814214},0,{"$f":"0.0098*(($BM929*(Y929^$BO929)*($C929-14.4)*$BP929)+($BN929*Y929*Y929))","v":0},{"$f":"0.0098*(($BM929*(Z929^$BO929)*($C929-14.4)*$BP929)+($BN929*Z929*Z929))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK929/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL929/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM929/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM929*(AN929^$BO929)*($C929-14.4)*$BP929)+($BN929*AN929*AN929))","v":0},0,0,{"v":1.9333333333333333,"d":"1.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20290303",20,290,3,30,15,0,0,0,{"v":0,"d":"0.0"},2282.8,0,0,0,1.362,1.1,1.1,1.1,341,0,0,0,59,0,0,0,1.4346886535326542,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK930/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL930/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM930/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":2.9,"d":"2.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20290383",20,290,3,38,20,0,0,0,{"v":0,"d":"0.0"},3195.4,0,0,0,1.362,1.1,1.1,1.1,477,0,0,0,82,0,0,0,3.792288972262474,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK931/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL931/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM931/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.8666666666666667,"d":"3.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20310143",20,310,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK932/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL932/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM932/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20310183",20,310,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK933/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL933/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM933/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20310233",20,310,3,23,10,0,0,0,{"v":0,"d":"0.0"},1850.8,0,0,0,1.362,1.1,1.1,1.1,276,0,0,0,47,0,0,0,{"$f":"0.0098*(($BM934*(W934^$BO934)*($C934-14.4)*$BP934)+($BN934*W934*W934))","v":2.582211129634811},0,{"$f":"0.0098*(($BM934*(Y934^$BO934)*($C934-14.4)*$BP934)+($BN934*Y934*Y934))","v":0},{"$f":"0.0098*(($BM934*(Z934^$BO934)*($C934-14.4)*$BP934)+($BN934*Z934*Z934))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK934/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL934/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM934/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM934*(AN934^$BO934)*($C934-14.4)*$BP934)+($BN934*AN934*AN934))","v":0},0,0,{"v":2.066666666666667,"d":"2.07"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20310303",20,310,3,30,15,0,0,0,{"v":0,"d":"0.0"},2458.3999999999996,0,0,0,1.362,1.1,1.1,1.1,367,0,0,0,63,0,0,0,1.7268743375976907,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK935/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL935/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM935/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.1,"d":"3.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20310383",20,310,3,38,20,0,0,0,{"v":0,"d":"0.0"},3441.2,0,0,0,1.362,1.1,1.1,1.1,{"$f":"ROUND(K936*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),O936),0)","v":514},0,0,0,88,0,0,0,4.4797641000701285,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK936/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL936/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM936/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.133333333333334,"d":"4.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20330143",20,330,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK937/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL937/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM937/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20330183",20,330,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK938/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL938/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM938/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20330233",20,330,3,23,10,0,0,0,{"v":0,"d":"0.0"},1983,0,0,0,1.362,1.1,1.1,1.1,296,0,0,0,51,0,0,0,{"$f":"0.0098*(($BM939*(W939^$BO939)*($C939-14.4)*$BP939)+($BN939*W939*W939))","v":3.1126888739420875},0,{"$f":"0.0098*(($BM939*(Y939^$BO939)*($C939-14.4)*$BP939)+($BN939*Y939*Y939))","v":0},{"$f":"0.0098*(($BM939*(Z939^$BO939)*($C939-14.4)*$BP939)+($BN939*Z939*Z939))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK939/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL939/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM939/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM939*(AN939^$BO939)*($C939-14.4)*$BP939)+($BN939*AN939*AN939))","v":0},0,0,{"v":2.2,"d":"2.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20330303",20,330,3,30,15,0,0,0,{"v":0,"d":"0.0"},2634,0,0,0,1.362,1.1,1.1,1.1,393,0,0,0,68,0,0,0,2.1090184987203204,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK940/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL940/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM940/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.3000000000000003,"d":"3.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20330383",20,330,3,38,20,0,0,0,{"v":0,"d":"0.0"},3687,0,0,0,1.362,1.1,1.1,1.1,550,0,0,0,95,0,0,0,5.310790997336448,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK941/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL941/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM941/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.4,"d":"4.40"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20350143",20,350,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK942/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL942/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM942/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20350183",20,350,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK943/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL943/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM943/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20350233",20,350,3,23,10,0,0,0,{"v":0,"d":"0.0"},2115.2000000000003,0,0,0,1.362,1.1,1.1,1.1,316,0,0,0,54,0,0,0,{"$f":"0.0098*(($BM944*(W944^$BO944)*($C944-14.4)*$BP944)+($BN944*W944*W944))","v":3.603197845267508},0,{"$f":"0.0098*(($BM944*(Y944^$BO944)*($C944-14.4)*$BP944)+($BN944*Y944*Y944))","v":0},{"$f":"0.0098*(($BM944*(Z944^$BO944)*($C944-14.4)*$BP944)+($BN944*Z944*Z944))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK944/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL944/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM944/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM944*(AN944^$BO944)*($C944-14.4)*$BP944)+($BN944*AN944*AN944))","v":0},0,0,{"v":2.3333333333333335,"d":"2.33"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20350303",20,350,3,30,15,0,0,0,{"v":0,"d":"0.0"},2809.6000000000004,0,0,0,1.362,1.1,1.1,1.1,419,0,0,0,72,0,0,0,2.479814832272436,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK945/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL945/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM945/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.5,"d":"3.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20350383",20,350,3,38,20,0,0,0,{"v":0,"d":"0.0"},3932.8,0,0,0,1.362,1.1,1.1,1.1,587,0,0,0,101,0,0,0,6.140553983251267,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK946/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL946/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM946/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.666666666666667,"d":"4.67"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20370143",20,370,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK947/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL947/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM947/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20370183",20,370,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK948/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL948/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM948/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20370233",20,370,3,23,10,0,0,0,{"v":0,"d":"0.0"},2247.4,0,0,0,1.362,1.1,1.1,1.1,335,0,0,0,58,0,0,0,{"$f":"0.0098*(($BM949*(W949^$BO949)*($C949-14.4)*$BP949)+($BN949*W949*W949))","v":4.245658635741807},0,{"$f":"0.0098*(($BM949*(Y949^$BO949)*($C949-14.4)*$BP949)+($BN949*Y949*Y949))","v":0},{"$f":"0.0098*(($BM949*(Z949^$BO949)*($C949-14.4)*$BP949)+($BN949*Z949*Z949))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK949/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL949/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM949/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM949*(AN949^$BO949)*($C949-14.4)*$BP949)+($BN949*AN949*AN949))","v":0},0,0,{"v":2.466666666666667,"d":"2.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20370303",20,370,3,30,15,0,0,0,{"v":0,"d":"0.0"},2985.2,0,0,0,1.362,1.1,1.1,1.1,446,0,0,0,77,0,0,0,2.9573413316583808,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK950/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL950/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM950/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.7,"d":"3.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20370383",20,370,3,38,20,0,0,0,{"v":0,"d":"0.0"},4178.599999999999,0,0,0,1.362,1.1,1.1,1.1,624,0,0,0,107,0,0,0,7.040650393387221,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK951/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL951/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM951/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.933333333333334,"d":"4.93"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20390143",20,390,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK952/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL952/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM952/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20390183",20,390,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK953/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL953/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM953/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20390233",20,390,3,23,10,0,0,0,{"v":0,"d":"0.0"},2379.6,0,0,0,1.362,1.1,1.1,1.1,355,0,0,0,61,0,0,0,{"$f":"0.0098*(($BM954*(W954^$BO954)*($C954-14.4)*$BP954)+($BN954*W954*W954))","v":4.83323914356915},0,{"$f":"0.0098*(($BM954*(Y954^$BO954)*($C954-14.4)*$BP954)+($BN954*Y954*Y954))","v":0},{"$f":"0.0098*(($BM954*(Z954^$BO954)*($C954-14.4)*$BP954)+($BN954*Z954*Z954))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK954/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL954/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM954/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM954*(AN954^$BO954)*($C954-14.4)*$BP954)+($BN954*AN954*AN954))","v":0},0,0,{"v":2.6,"d":"2.60"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20390303",20,390,3,30,15,0,0,0,{"v":0,"d":"0.0"},3160.8,0,0,0,1.362,1.1,1.1,1.1,472,0,0,0,81,0,0,0,3.414735884206643,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK955/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL955/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM955/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":3.9,"d":"3.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20390383",20,390,3,38,20,0,0,0,{"v":0,"d":"0.0"},4424.400000000001,0,0,0,1.362,1.1,1.1,1.1,660,0,0,0,114,0,0,0,8.110068591235784,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK956/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL956/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM956/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":5.2,"d":"5.20"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20410143",20,410,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK957/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL957/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM957/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20410183",20,410,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",{"$f":"ROUND(L958*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P958),0)","v":0},{"$f":"ROUND(M958*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q958),0)","v":0},{"$f":"ROUND(N958*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R958),0)","v":0},"-",{"$f":"ROUND(T958*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U958*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V958*3600/(4186*ABS($M$1-$M$2)),0)","v":0},"-","-","-","-",0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE958*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH958),0)","v":0},{"$f":"ROUND(AF958*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI958),0)","v":0},{"$f":"ROUND(AG958*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ958),0)","v":0},{"$f":"ROUND(AK958*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL958*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM958*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK958/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL958/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM958/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20410233",20,410,3,23,10,0,0,0,{"v":0,"d":"0.0"},2511.7999999999997,0,0,0,1.362,1.1,1.1,1.1,375,{"$f":"ROUND(L959*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P959),0)","v":0},{"$f":"ROUND(M959*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),Q959),0)","v":0},{"$f":"ROUND(N959*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),R959),0)","v":0},{"$f":"ROUND(S959*3600/(4186*ABS($M$1-$M$2)),0)","v":65},{"$f":"ROUND(T959*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(U959*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"ROUND(V959*3600/(4186*ABS($M$1-$M$2)),0)","v":0},{"$f":"0.0098*(($BM959*(W959^$BO959)*($C959-14.4)*$BP959)+($BN959*W959*W959))","v":5.594470544717497},0,{"$f":"0.0098*(($BM959*(Y959^$BO959)*($C959-14.4)*$BP959)+($BN959*Y959*Y959))","v":0},{"$f":"0.0098*(($BM959*(Z959^$BO959)*($C959-14.4)*$BP959)+($BN959*Z959*Z959))","v":0},0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE959*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH959),0)","v":0},{"$f":"ROUND(AF959*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AI959),0)","v":0},{"$f":"ROUND(AG959*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AJ959),0)","v":0},{"$f":"ROUND(AK959*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AL959*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"ROUND(AM959*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},{"$f":"(AK959/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL959/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM959/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM959*(AN959^$BO959)*($C959-14.4)*$BP959)+($BN959*AN959*AN959))","v":0},0,0,{"v":2.7333333333333334,"d":"2.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20410303",20,410,3,30,15,0,0,0,{"v":0,"d":"0.0"},3336.3999999999996,0,0,0,1.362,1.1,1.1,1.1,498,0,0,0,86,0,0,0,3.996718237859822,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK960/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL960/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM960/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.1,"d":"4.10"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20410383",20,410,3,38,20,0,0,0,{"v":0,"d":"0.0"},4670.2,0,0,0,1.362,1.1,1.1,1.1,697,0,0,0,120,0,0,0,9.162461745544531,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK961/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL961/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM961/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":5.466666666666667,"d":"5.47"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20430143",20,430,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK962/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL962/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM962/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20430183",20,430,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK963/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL963/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM963/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20430233",20,430,3,23,10,0,0,0,{"v":0,"d":"0.0"},2644,0,0,0,1.362,1.1,1.1,1.1,395,0,0,0,68,0,0,0,{"$f":"0.0098*(($BM964*(W964^$BO964)*($C964-14.4)*$BP964)+($BN964*W964*W964))","v":6.2846818284316095},0,{"$f":"0.0098*(($BM964*(Y964^$BO964)*($C964-14.4)*$BP964)+($BN964*Y964*Y964))","v":0},{"$f":"0.0098*(($BM964*(Z964^$BO964)*($C964-14.4)*$BP964)+($BN964*Z964*Z964))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK964/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL964/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM964/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM964*(AN964^$BO964)*($C964-14.4)*$BP964)+($BN964*AN964*AN964))","v":0},0,0,{"v":2.8666666666666667,"d":"2.87"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20430303",20,430,3,30,15,0,0,0,{"v":0,"d":"0.0"},3512,0,0,0,1.362,1.1,1.1,1.1,524,0,0,0,90,0,0,0,4.54847874286282,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK965/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL965/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM965/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.3,"d":"4.30"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20430383",20,430,3,38,20,0,0,0,{"v":0,"d":"0.0"},4916,0,0,0,1.362,1.1,1.1,1.1,734,0,0,0,126,0,0,0,10.289704515366871,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK966/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL966/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM966/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":5.733333333333333,"d":"5.73"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20450143",20,450,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK967/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL967/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM967/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20450183",20,450,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK968/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL968/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM968/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20450233",20,450,3,23,10,0,0,0,{"v":0,"d":"0.0"},2776.2000000000003,0,0,0,1.362,1.1,1.1,1.1,414,0,0,0,71,0,0,0,{"$f":"0.0098*(($BM969*(W969^$BO969)*($C969-14.4)*$BP969)+($BN969*W969*W969))","v":7.02335984179961},0,{"$f":"0.0098*(($BM969*(Y969^$BO969)*($C969-14.4)*$BP969)+($BN969*Y969*Y969))","v":0},{"$f":"0.0098*(($BM969*(Z969^$BO969)*($C969-14.4)*$BP969)+($BN969*Z969*Z969))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK969/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL969/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM969/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM969*(AN969^$BO969)*($C969-14.4)*$BP969)+($BN969*AN969*AN969))","v":0},0,0,{"$f":"IF($F969=$BR$70,$C969*$BS$70,IF($F969=$BR$71,$C969*$BS$71,IF($F969=$BR$72,$C969*$BS$72,IF($F969=$BR$73,$C969*$BS$73,IF($F969=$BR$74,$C969*$BS$74,IF($F969=$BR$75,$C969*$BS$75,IF($F969=$BR$76,$C969*$BS$76,IF($F969=$BR$77,$C969*$BS$77,IF($F969=$BR$78,$C969*$BS$78,IF($F969=$BR$79,$C969*$BS$79,IF($F969=$BR$80,$C969*$BS$80,)))))))))))","v":{"v":3,"d":"3.00"}},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20450303",20,450,3,30,15,0,0,0,{"v":0,"d":"0.0"},3687.6000000000004,0,0,0,1.362,1.1,1.1,1.1,550,0,0,0,95,0,0,0,5.243754957635606,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK970/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL970/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM970/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.5,"d":"4.50"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,{"$f":"IF($F970=$BR$70,$BT$70,IF($F970=$BR$71,$BT$71,IF($F970=$BR$72,$BT$72,IF($F970=$BR$73,$BT$73,IF($F970=$BR$74,$BT$74,IF($F970=$BR$75,$BT$75,IF($F970=$BR$76,$BT$76,IF($F970=$BR$77,$BT$77,IF($F970=$BR$78,$BT$78,IF($F970=$BR$79,$BT$79,IF($F970=$BR$80,$BT$80,)))))))))))","v":0.00019563320356262},{"$f":"IF($F970=$BR$70,$BU$70,IF($F970=$BR$71,$BU$71,IF($F970=$BR$72,$BU$72,IF($F970=$BR$73,$BU$73,IF($F970=$BR$74,$BU$74,IF($F970=$BR$75,$BU$75,IF($F970=$BR$76,$BU$76,IF($F970=$BR$77,$BU$77,IF($F970=$BR$78,$BU$78,IF($F970=$BR$79,$BU$79,IF($F970=$BR$80,$BU$80,)))))))))))","v":4.4708458846471E-4},{"$f":"IF($F970=$BR$70,$BV$70,IF($F970=$BR$71,$BV$71,IF($F970=$BR$72,$BV$72,IF($F970=$BR$73,$BV$73,IF($F970=$BR$74,$BV$74,IF($F970=$BR$75,$BV$75,IF($F970=$BR$76,$BV$76,IF($F970=$BR$77,$BV$77,IF($F970=$BR$78,$BV$78,IF($F970=$BR$79,$BV$79,IF($F970=$BR$80,$BV$80,)))))))))))","v":1.766459432507},{"$f":"IF($F970=$BR$70,$BW$70,IF($F970=$BR$71,$BW$71,IF($F970=$BR$72,$BW$72,IF($F970=$BR$73,$BW$73,IF($F970=$BR$74,$BW$74,IF($F970=$BR$75,$BW$75,IF($F970=$BR$76,$BW$76,IF($F970=$BR$77,$BW$77,IF($F970=$BR$78,$BW$78,IF($F970=$BR$79,$BW$79,IF($F970=$BR$80,$BW$80,)))))))))))","v":2}]
["20450383",20,450,3,38,20,0,0,0,{"v":0,"d":"0.0"},5161.8,0,0,0,1.362,1.1,1.1,1.1,770,0,0,0,132,0,0,0,11.493159665968475,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK971/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL971/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM971/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6,"d":"6.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20470143",20,470,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK972/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL972/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM972/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20470183",20,470,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK973/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL973/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM973/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
[{"$f":"CONCATENATE(B974,C974,E974,D974)","v":"20470233"},20,470,3,23,10,0,0,0,{"v":0,"d":"0.0"},2908.4,0,0,0,1.362,1.1,1.1,1.1,434,0,0,0,75,0,0,0,{"$f":"0.0098*(($BM974*(W974^$BO974)*($C974-14.4)*$BP974)+($BN974*W974*W974))","v":7.969184608089089},0,{"$f":"0.0098*(($BM974*(Y974^$BO974)*($C974-14.4)*$BP974)+($BN974*Y974*Y974))","v":0},{"$f":"0.0098*(($BM974*(Z974^$BO974)*($C974-14.4)*$BP974)+($BN974*Z974*Z974))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK974/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL974/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM974/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM974*(AN974^$BO974)*($C974-14.4)*$BP974)+($BN974*AN974*AN974))","v":0},0,0,{"v":3.1333333333333337,"d":"3.13"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20470303",20,470,3,30,15,0,0,0,{"v":0,"d":"0.0"},3863.2000000000003,0,0,0,1.362,1.1,1.1,1.1,577,0,0,0,99,0,0,0,5.897457975194254,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK975/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL975/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM975/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.7,"d":"4.70"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20470383",20,470,3,38,20,0,0,0,{"v":0,"d":"0.0"},5407.6,0,0,0,1.362,1.1,1.1,1.1,807,0,0,0,139,0,0,0,12.901341846235352,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK976/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL976/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM976/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6.2666666666666675,"d":"6.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]
["20490143",20,490,3,14,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",{"$f":"ROUND(L977*POWER((($M$1-$M$2)/LN(($M$1-$M$3)/($M$2-$M$3)))/((75-65)/LN((75-20)/(65-20))),P977),0)","v":0},0,0,"-",{"$f":"ROUND(T977*3600/(4186*ABS($M$1-$M$2)),0)","v":0},0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,{"$f":"ROUND(AE977*POWER((($AG$1-$AG$2)/LN(($AG$1-$AG$3)/($AG$2-$AG$3)))/((16-18)/LN((16-27)/(18-27))),AH977),0)","v":0},0,0,{"$f":"ROUND(AK977*3600/(4186*ABS($AG$1-$AG$2)),0)","v":0},0,0,{"$f":"(AK977/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL977/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM977/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20490183",20,490,3,18,0,0,0,0,{"v":0,"d":"0.0"},"Niet bestaand",0,0,0,1.362,1.1,1.1,1.1,"-",0,0,0,"-",0,0,0,"-","-","-","-",0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK978/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL978/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM978/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},"-","-","-",{"v":0,"d":"0.00"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0,0,0,0]
["20490233",20,490,3,23,10,0,0,0,{"v":0,"d":"0.0"},3040.6,0,0,0,1.362,1.1,1.1,1.1,454,0,0,0,{"$f":"ROUND(S979*3600/(4186*ABS($M$1-$M$2)),0)","v":78},0,0,0,{"$f":"0.0098*(($BM979*(W979^$BO979)*($C979-14.4)*$BP979)+($BN979*W979*W979))","v":8.81806053790544},0,{"$f":"0.0098*(($BM979*(Y979^$BO979)*($C979-14.4)*$BP979)+($BN979*Y979*Y979))","v":0},{"$f":"0.0098*(($BM979*(Z979^$BO979)*($C979-14.4)*$BP979)+($BN979*Z979*Z979))","v":0},0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK979/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL979/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM979/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"0.0098*(($BM979*(AN979^$BO979)*($C979-14.4)*$BP979)+($BN979*AN979*AN979))","v":0},0,0,{"v":3.266666666666667,"d":"3.27"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.0014501879713726,0.00037831632653061,1.4868910444209,2]
["20490303",20,490,3,30,15,0,0,0,{"v":0,"d":"0.0"},4038.7999999999997,0,0,0,1.362,1.1,1.1,1.1,603,0,0,0,{"$f":"ROUND(S980*3600/(4186*ABS($M$1-$M$2)),0)","v":104},0,0,0,6.714659675140365,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK980/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL980/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM980/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":4.9,"d":"4.90"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,0.00019563320356262,4.4708458846471E-4,1.766459432507,2]
["20490383",20,490,3,38,20,0,0,0,{"v":0,"d":"0.0"},5653.4,0,0,0,1.362,1.1,1.1,1.1,844,0,0,0,{"$f":"ROUND(S981*3600/(4186*ABS($M$1-$M$2)),0)","v":145},0,0,0,14.26881429717107,0,0,0,0,0,0,0.98,0.98,0.98,0,0,0,0,0,0,{"$f":"(AK981/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AL981/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},{"$f":"(AM981/(IF((237.3*LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))/(17.27-LN(('Mini Canal'!$J$13*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))<((data!$AG$1+data!$AG$2)/2),1,IF(1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))>1,1,1/(1+((2258*((0.622/((101325/(1*611*EXP(17.27*(((data!$AG$1+data!$AG$2)/2)/(((data!$AG$1+data!$AG$2)/2)+237.3))))))-1)*1000-(0.622/((101325/('Mini Canal'!$J$13*611*EXP(17.27*(data!$AG$3/(data!$AG$3+237.3))))))-1)*1000))/(1005*(((data!$AG$1+data!$AG$2)/2)-data!$AG$3))))))))","v":0},0,0,0,{"v":6.533333333333334,"d":"6.53"},0,0,0,null,0,0,0,0,null,0,0,0,0,null,null,1.6730950035507E-3,0.00032929523945446,1.3691788367472,2]

{"sheet":"NL","index":2,"n_rows":22,"n_cols":17,"rows_kept":22,"hidden":true,"merged":[[7,0,7,2],[7,5,7,8],[8,0,8,2],[8,5,8,8],[9,0,9,2],[9,5,9,8],[14,0,14,12]]}
[]
["Invulformulier"]
[{"$nulls":6},"Toestel"]
["Randvoorwaarden",{"$nulls":5},"Uitvoering"]
[]
["Temperaturen",{"$nulls":8},"Hoogte","Breedte","Lengte","Type"]
["Verwarmen:",{"$nulls":4},"Koelen:",{"$nulls":10},"Kopieer alle data"]
["Aanvoertemp.",null,null,{"$f":"'Mini Canal'!E10","v":35},null,{"$f":"A8","v":"Aanvoertemp."},{"$nulls":3},{"$f":"'Mini Canal'!J10","v":16},null,"Eenheidsstelsel",{"$nulls":4},"SI-eenheden"]
["Retourtemp.",null,null,{"$f":"'Mini Canal'!E11","v":30},null,{"$f":"A9","v":"Retourtemp."},{"$nulls":3},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":6},"Imperiale-eenheden"]
["Ruimtetemp.",null,null,{"$f":"'Mini Canal'!E12","v":20},null,{"$f":"A10","v":"Ruimtetemp."},{"$nulls":3},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}}]
[{"$nulls":5},"rel. vocht. [%]",{"$nulls":3},{"$f":"'Mini Canal'!J13","v":{"v":0.5,"d":"50%"}}]
[]
[]
["Snelheidsniveau:","Stuurspanning: [V]",{"$f":"CONCATENATE(\"Warmteafgifte * \",ROUND(D8,0),\"/\",ROUND(D9,0),\"/\",ROUND(D10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Warmteafgifte * 35/30/20 [W]"},{"$f":"\"Waterdebiet, verwarming [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Waterdebiet, verwarming [l/h]"},{"$f":"\"Waterzijdig drukverlies [\"&IF(data!$P$1=1,\"kPa\",IF(data!$P$1=2,\"ftH2O\"))&\"]\"","v":"Waterzijdig drukverlies [kPa]"},{"$f":"CONCATENATE(\" Koelcapaciteit * \",ROUND(J8,0),\"/\",,ROUND(J9,0),\"/\",,ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":" Koelcapaciteit * 16/18/27 [W]"},{"$f":"CONCATENATE(\"Tot. koelcapaciteit \",,ROUND(J8,0),\"/\",,ROUND(J9,0),\"/\",,ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Tot. koelcapaciteit 16/18/27 [W]"},{"$f":"\"Waterdebiet, koeling [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Waterdebiet, koeling [l/h]"},{"$f":"E14","v":"Waterzijdig drukverlies [kPa]"},"Geluidsdruk *** [dB(A)]","Geluidsvermogen ** [dB(A)]","Elektrisch verbruik [W]","Watervolume [l]"]
[{"$f":"\"Mini Canal, \"&L6&\" \"&ROUND(data!C5,1)&\"cm, \"&J6&\" \"&ROUND(data!B5,1)&\"cm, \"&K6&\" \"&ROUND(data!E5,1)&\"cm\"","v":"Mini Canal, Lengte 290cm, Hoogte 14cm, Breedte 34cm"}]
[]
[]
[]
[]
["Waardes gemeten volgens EN 16430",{"$nulls":11},{"$f":"'Mini Canal'!M22","v":"v2023-06-16"}]
["Geluidsvermogen gemeten volgens ISO 3741:2010"]
["Geluidsdruk bij een aangenomen ruimtedemping van 8 dB(A)"]

{"sheet":"EN","index":3,"n_rows":22,"n_cols":17,"rows_kept":22,"hidden":true,"merged":[[7,0,7,2],[7,5,7,8],[8,0,8,2],[8,5,8,8],[9,0,9,2],[9,5,9,8],[14,0,14,12]]}
[]
["Formulary"]
[{"$nulls":6},"Device"]
["Conditions",{"$nulls":5},"Version"]
[]
["Temperatures",{"$nulls":8},"Heigth","Width","Length","Type"]
["Heating:",{"$nulls":4},"Cooling:",{"$nulls":10},"Copy all data"]
["Inlet temp.",null,null,{"$f":"'Mini Canal'!E10","v":35},null,{"$f":"A8","v":"Inlet temp."},{"$nulls":3},{"$f":"'Mini Canal'!J10","v":16},null,"Unit conversion",{"$nulls":4},"SI-units"]
["Return temp.",null,null,{"$f":"'Mini Canal'!E11","v":30},null,{"$f":"A9","v":"Return temp."},{"$nulls":3},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":6},"Imperial-units"]
["Room temp.",null,null,{"$f":"'Mini Canal'!E12","v":20},null,{"$f":"A10","v":"Room temp."},{"$nulls":3},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}}]
[{"$nulls":5},"rel. humid. [%]",{"$nulls":3},{"$f":"'Mini Canal'!J13","v":{"v":0.5,"d":"50%"}}]
[]
[]
["Speed level:","Control voltage [V]",{"$f":"CONCATENATE(\"Heat output * \",ROUND(D8,0),\"/\",ROUND(D9,0),\"/\",ROUND(D10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Heat output * 35/30/20 [W]"},{"$f":"\"Water flowrate, heating [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Water flowrate, heating [l/h]"},{"$f":"\"Watersided pressure loss [\"&IF(data!$P$1=1,\"kPa\",IF(data!$P$1=2,\"ftH2O\"))&\"]\"","v":"Watersided pressure loss [kPa]"},{"$f":"CONCATENATE(\"Cooling capacity * \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Cooling capacity * 16/18/27 [W]"},{"$f":"CONCATENATE(\"Tot. cooling capacity \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Tot. cooling capacity 16/18/27 [W]"},{"$f":"\"Water flowrate, cooling [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Water flowrate, cooling [l/h]"},{"$f":"E14","v":"Watersided pressure loss [kPa]"},"Sound pressure *** [dB(A)]","Sound power ** [dB(A)]","Electrical power [W]","Water volume [l]"]
[{"$f":"\"Mini Canal, \"&L6&\" \"&ROUND(data!C5,1)&\"cm, \"&J6&\" \"&ROUND(data!B5,1)&\"cm, \"&K6&\" \"&ROUND(data!E5,1)&\"cm\"","v":"Mini Canal, Length 290cm, Heigth 14cm, Width 34cm"}]
[]
[]
[]
[]
["Values according to EN 16430",{"$nulls":11},{"$f":"'Mini Canal'!M22","v":"v2023-06-16"}]
["Sound power according to ISO 3741:2010"]
["Sound pressure with an assumed room damping of 8dB(A)"]

{"sheet":"DE","index":4,"n_rows":22,"n_cols":17,"rows_kept":22,"hidden":true,"merged":[[7,0,7,2],[7,5,7,8],[8,0,8,2],[8,5,8,8],[9,0,9,2],[9,5,9,8],[14,0,14,12]]}
[]
["Eingabefelder"]
[{"$nulls":6},"Gerät"]
["Auslegungsrandbedingungen",{"$nulls":5},"Ausführung"]
[]
["Temperaturen",{"$nulls":8},"Höhe","Tiefe","Länge","Typ"]
["Heizen:",{"$nulls":4},"Kühlen:",{"$nulls":10},"Kopieren Sie alle daten"]
["Vorlauftemp.",null,null,{"$f":"'Mini Canal'!E10","v":35},null,{"$f":"A8","v":"Vorlauftemp."},{"$nulls":3},{"$f":"'Mini Canal'!J10","v":16},null,"Einheiten",{"$nulls":4},"SI-einheiten"]
["Rücklauftemp.",null,null,{"$f":"'Mini Canal'!E11","v":30},null,{"$f":"A9","v":"Rücklauftemp."},{"$nulls":3},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":6},"Imperiale-einheiten"]
["Raumtemp.",null,null,{"$f":"'Mini Canal'!E12","v":20},null,{"$f":"A10","v":"Raumtemp."},{"$nulls":3},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}}]
[{"$nulls":5},"rel. Luftf. [%]",{"$nulls":3},{"$f":"'Mini Canal'!J13","v":{"v":0.5,"d":"50%"}}]
[]
[]
["Drehzahlstufe:","Regelspannung: [V]",{"$f":"CONCATENATE(\"Heizleistung * \",ROUND(D8,0),\"/\",ROUND(D9,0),\"/\",ROUND(D10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Heizleistung * 35/30/20 [W]"},{"$f":"\"Heizmittelstrom [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Heizmittelstrom [l/h]"},{"$f":"\"zug. wassers. Druckverlust [\"&IF(data!$P$1=1,\"kPa\",IF(data!$P$1=2,\"ftH2O\"))&\"]\"","v":"zug. wassers. Druckverlust [kPa]"},{"$f":"CONCATENATE(\"Kühlleistung * \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Kühlleistung * 16/18/27 [W]"},{"$f":"CONCATENATE(\"Tot. Kühlleistung \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Tot. Kühlleistung 16/18/27 [W]"},{"$f":"\"Kühlmittelstrom [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Kühlmittelstrom [l/h]"},{"$f":"E14","v":"zug. wassers. Druckverlust [kPa]"},"Schalldruckpegel *** [dB(A)]","Schallleistungspegel ** [dB(A)]","Elektr. Leistung [W]","Wasservolumen [l]"]
[{"$f":"\"Mini Canal, \"&L6&\" \"&ROUND(data!C5,1)&\"cm, \"&J6&\" \"&ROUND(data!B5,1)&\"cm, \"&K6&\" \"&ROUND(data!E5,1)&\"cm\"","v":"Mini Canal, Länge 290cm, Höhe 14cm, Tiefe 34cm"}]
[]
[]
[]
[]
["Leistungsangaben nach EN 16430",{"$nulls":11},{"$f":"'Mini Canal'!M22","v":"v2023-06-16"}]
["Schallleistungspegel nach ISO 3741:2010"]
["Schalldruckpegel bei angenommener Raumdämpfung von 8dB(A)"]

{"sheet":"FR","index":5,"n_rows":22,"n_cols":17,"rows_kept":22,"hidden":true,"merged":[[7,0,7,2],[7,5,7,8],[8,0,8,2],[8,5,8,8],[9,0,9,2],[9,5,9,8],[14,0,14,12]]}
[]
["Formulaire"]
[{"$nulls":6},"Appareil"]
["Conditions",{"$nulls":5},"Version"]
[]
["Températures",{"$nulls":8},"Hauteur","Profondeur","Longeur","Type"]
["Chauffer:",{"$nulls":4},"Refroidir:",{"$nulls":10},"Copier toutes des données"]
["Temp. entrée",null,null,{"$f":"'Mini Canal'!E10","v":35},null,{"$f":"A8","v":"Temp. entrée"},{"$nulls":3},{"$f":"'Mini Canal'!J10","v":16},null,"Système unitaire",{"$nulls":4},"Unités-SI"]
["Temp. retour",null,null,{"$f":"'Mini Canal'!E11","v":30},null,{"$f":"A9","v":"Temp. retour"},{"$nulls":3},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":6},"Unités-Impériales"]
["Temp. ambiante",null,null,{"$f":"'Mini Canal'!E12","v":20},null,{"$f":"A10","v":"Temp. ambiante"},{"$nulls":3},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}}]
[{"$nulls":5},"hum. rel. [%]",{"$nulls":3},{"$f":"'Mini Canal'!J13","v":{"v":0.5,"d":"50%"}}]
[]
[]
["Niveau de vitesse","Voltage [V]",{"$f":"CONCATENATE(\"Puissance de cha. * \",ROUND(D8,0),\"/\",ROUND(D9,0),\"/\",ROUND(D10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Puissance de cha. * 35/30/20 [W]"},{"$f":"\"Débit d'eau, chauffer [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Débit d'eau, chauffer [l/h]"},{"$f":"\"Perte de charge [\"&IF(data!$P$1=1,\"kPa\",IF(data!$P$1=2,\"ftH2O\"))&\"]\"","v":"Perte de charge [kPa]"},{"$f":"CONCATENATE(\"Puissance de refr. * \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Puissance de refr. * 16/18/27 [W]"},{"$f":"CONCATENATE(\"Puissance tot. de refr. \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Puissance tot. de refr. 16/18/27 [W]"},{"$f":"\"Débit d'eau, refroidir [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Débit d'eau, refroidir [l/h]"},{"$f":"E14","v":"Perte de charge [kPa]"},"Pression sonore *** [dB(A)]","Puissance sonore ** [dB(A)]","Puissance absorbée elec. [W]","Volume d'eau [l]"]
[{"$f":"\"Mini Canal, \"&L6&\" \"&ROUND(data!C5,1)&\"cm, \"&J6&\" \"&ROUND(data!B5,1)&\"cm, \"&K6&\" \"&ROUND(data!E5,1)&\"cm\"","v":"Mini Canal, Longeur 290cm, Hauteur 14cm, Profondeur 34cm"}]
[]
[]
[]
[]
["Testé selon EN 16430",{"$nulls":11},{"$f":"'Mini Canal'!M22","v":"v2023-06-16"}]
["Puissance sonore testé selon ISO 3741:2010"]
["Pression sonore avec une atténuation ambiante du 8dB(A)"]

{"sheet":"NR","index":6,"n_rows":22,"n_cols":17,"rows_kept":22,"hidden":true,"merged":[[7,0,7,2],[7,5,7,8],[8,0,8,2],[8,5,8,8],[9,0,9,2],[9,5,9,8],[14,0,14,12]]}
[]
["Formulaire"]
[{"$nulls":6},"Modell"]
["Conditions",{"$nulls":5},"Versjon"]
[]
["Temperaturer",{"$nulls":8},"Høyde","Bredde","Lengde","Type"]
["Varme:",{"$nulls":4},"Kjøling:",{"$nulls":10},"Kopier alle data"]
["Tur temp.",null,null,{"$f":"'Mini Canal'!E10","v":35},null,{"$f":"A8","v":"Tur temp."},{"$nulls":3},{"$f":"'Mini Canal'!J10","v":16},null,"Enhetssystem",{"$nulls":4},"SI-enheter"]
["Retur temp.",null,null,{"$f":"'Mini Canal'!E11","v":30},null,{"$f":"A9","v":"Retur temp."},{"$nulls":3},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":6},"Imperiale-enheter"]
["Rom temp.",null,null,{"$f":"'Mini Canal'!E12","v":20},null,{"$f":"A10","v":"Rom temp."},{"$nulls":3},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}}]
[{"$nulls":5},"rel. fuktighet [%]",{"$nulls":3},{"$f":"'Mini Canal'!J13","v":{"v":0.5,"d":"50%"}}]
[]
[]
["Styresignal","Viftespenning [V]",{"$f":"CONCATENATE(\"Varme effekt \",ROUND(D8,0),\"/\",ROUND(D9,0),\"/\",ROUND(D10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Varme effekt 35/30/20 [W]"},{"$f":"\"Vannmengde [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Vannmengde [l/h]"},{"$f":"\"trykktap på vannsiden [\"&IF(data!$P$1=1,\"kPa\",IF(data!$P$1=2,\"ftH2O\"))&\"]\"","v":"trykktap på vannsiden [kPa]"},{"$f":"CONCATENATE(\"Kjøle effekt * \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Kjøle effekt * 16/18/27 [W]"},{"$f":"CONCATENATE(\"Tot. Kjøle effekt \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Tot. Kjøle effekt 16/18/27 [W]"},{"$f":"D14","v":"Vannmengde [l/h]"},{"$f":"E14","v":"trykktap på vannsiden [kPa]"},"Lydtrykk [dB(A)]***","Lydeffekt [dB(A)]***","Elektrisk effekt [W]","Vannvolum [l]"]
[{"$f":"\"Mini Canal, \"&L6&\" \"&ROUND(data!C5,1)&\"cm, \"&J6&\" \"&ROUND(data!B5,1)&\"cm, \"&K6&\" \"&ROUND(data!E5,1)&\"cm\"","v":"Mini Canal, Lengde 290cm, Høyde 14cm, Bredde 34cm"}]
[]
[]
[]
[]
["Kjølekapasitet beregnes i henhold til EN16430 med viftene som blåser oppover for alle typer.",{"$nulls":11},{"$f":"'Mini Canal'!M22","v":"v2023-06-16"}]
["Når vannvolumet er gitt i gallon, er dette imperial gallons."]
["Lydeffekt i henhold til ISO 3741: 2010. For lydtrykknivået er det en antatt romdemping på 8 dB (A)."]

{"sheet":"SP","index":7,"n_rows":22,"n_cols":17,"rows_kept":22,"hidden":true,"merged":[[7,0,7,2],[7,5,7,8],[8,0,8,2],[8,5,8,8],[9,0,9,2],[9,5,9,8],[10,5,10,8],[14,0,14,12]]}
[]
["Formulaire"]
[{"$nulls":6},"Modelo"]
["Conditions",{"$nulls":5},"Versión"]
[]
["Temperaturas",{"$nulls":8},"Altura","Anchura","Longitud","Tipo"]
["Calefacción:",{"$nulls":4},"Enfriamiento:",{"$nulls":10},"Copiar todos los datos"]
["Agua impulsión",0,0,{"$f":"'Mini Canal'!E10","v":35},null,{"$f":"A8","v":"Agua impulsión"},{"$nulls":3},{"$f":"'Mini Canal'!J10","v":16},null,"Convers. de unidades",{"$nulls":4},"Unidades-SI"]
["Agua retorno",0,0,{"$f":"'Mini Canal'!E11","v":30},null,{"$f":"A9","v":"Agua retorno"},{"$nulls":3},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":6},"Unidades-Imperial"]
["Ambiente",0,0,{"$f":"'Mini Canal'!E12","v":20},null,{"$f":"A10","v":"Ambiente"},{"$nulls":3},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}}]
[{"$nulls":5},"Humedad relativa",{"$nulls":3},{"$f":"'Mini Canal'!J13","v":{"v":0.5,"d":"50%"}}]
[]
[]
["Nivel de velocidad:"," Voltaje control [V]",{"$f":"CONCATENATE(\"Emisión calefacción * \",ROUND(D8,0),\"/\",ROUND(D9,0),\"/\",ROUND(D10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Emisión calefacción * 35/30/20 [W]"},{"$f":"\"Caudal de agua, calefacción [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Caudal de agua, calefacción [l/h]"},{"$f":"\"Pérdida de carga del agua [\"&IF(data!$P$1=1,\"kPa\",IF(data!$P$1=2,\"ftH2O\"))&\"]\"","v":"Pérdida de carga del agua [kPa]"},{"$f":"CONCATENATE(\"Emisión Frío * \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Emisión Frío * 16/18/27 [W]"},{"$f":"CONCATENATE(\"Emisión total Frío * \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Emisión total Frío * 16/18/27 [W]"},{"$f":"\"Caudal de agua, calefacción [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Caudal de agua, calefacción [l/h]"},{"$f":"E14","v":"Pérdida de carga del agua [kPa]"},"Presión sonora *** [dB(A)]","Potencia sonora ** [dB(A)]","Potencia eléctrica absorbida [W]","Vannvolum [l]"]
[{"$f":"\"Mini Canal, \"&L6&\" \"&ROUND(data!C5,1)&\"cm, \"&J6&\" \"&ROUND(data!B5,1)&\"cm, \"&K6&\" \"&ROUND(data!E5,1)&\"cm\"","v":"Mini Canal, Longitud 290cm, Altura 14cm, Anchura 34cm"}]
[]
[]
[]
[]
["La potencia de enfriamiento se calcula según la norma EN 16430 con ventiladores de todas las alturas.",{"$nulls":11},{"$f":"'Mini Canal'!M22","v":"v2023-06-16"}]
["Potencia sonora según ISO 3741: 2010."]
["Nivel de presión acústica con una amortiguación ambiental supuesta de 8 dB (A)."]

{"sheet":"SW","index":8,"n_rows":22,"n_cols":17,"rows_kept":22,"hidden":true,"merged":[[7,0,7,2],[7,5,7,8],[8,0,8,2],[8,5,8,8],[9,0,9,2],[9,5,9,8],[14,0,14,12]]}
[]
["Formulary"]
[{"$nulls":6},"Modell"]
["Conditions",{"$nulls":5},"Storlek"]
[]
["Temperaturer",{"$nulls":8},"Höjd","Djup","Längd","Type"]
["Värme:",{"$nulls":4},"Kyla:",{"$nulls":10},"Kopiera all data"]
["Tillopp",null,null,{"$f":"'Mini Canal'!E10","v":35},null,{"$f":"A8","v":"Tillopp"},{"$nulls":3},{"$f":"'Mini Canal'!J10","v":16},null,"Enhetssystem",{"$nulls":4},"SI-enheter"]
["Retur",null,null,{"$f":"'Mini Canal'!E11","v":30},null,{"$f":"A9","v":"Retur"},{"$nulls":3},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":6},"Imperiella-enheter"]
["Rum (torr)",null,null,{"$f":"'Mini Canal'!E12","v":20},null,{"$f":"A10","v":"Rum (torr)"},{"$nulls":3},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}}]
[{"$nulls":5},"rel. Fuktighet [%]",{"$nulls":3},{"$f":"'Mini Canal'!J13","v":{"v":0.5,"d":"50%"}}]
[]
[]
["Fläkthastighet:","Styrsignal [V]",{"$f":"CONCATENATE(\"Effekt * \",ROUND(D8,0),\"/\",ROUND(D9,0),\"/\",ROUND(D10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Effekt * 35/30/20 [W]"},{"$f":"\"Vattenflöde, Värme [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Vattenflöde, Värme [l/h]"},{"$f":"\"Tryckfall, vatten [\"&IF(data!$P$1=1,\"kPa\",IF(data!$P$1=2,\"ftH2O\"))&\"]\"","v":"Tryckfall, vatten [kPa]"},{"$f":"CONCATENATE(\"kyleffekt * \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"kyleffekt * 16/18/27 [W]"},{"$f":"CONCATENATE(\"Total kyleffekt \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Total kyleffekt 16/18/27 [W]"},{"$f":"\"Vattenflöde, kyla [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Vattenflöde, kyla [l/h]"},{"$f":"E14","v":"Tryckfall, vatten [kPa]"},"Vattenflöde, *** [dB(A)]","Ljudeffekt ** [dB(A)]","Effektförbrukning [W]","Vattenvolym [l]"]
[{"$f":"\"Mini Canal, \"&L6&\" \"&ROUND(data!C5,1)&\"cm, \"&J6&\" \"&ROUND(data!B5,1)&\"cm, \"&K6&\" \"&ROUND(data!E5,1)&\"cm\"","v":"Mini Canal, Längd 290cm, Höjd 14cm, Djup 34cm"}]
[]
[]
[]
[]
["Värden engligt EN 16430",{"$nulls":11},{"$f":"'Mini Canal'!M22","v":"v2023-06-16"}]
["Ljudeffekt enligt ISO 3741:2010"]
["Ljudtryck med antagen ljudreduktion från rummet på 8 dB(A) "]

{"sheet":"TS","index":9,"n_rows":22,"n_cols":17,"rows_kept":22,"hidden":true,"merged":[[7,0,7,2],[7,5,7,8],[8,0,8,2],[8,5,8,8],[9,0,9,2],[9,5,9,8],[14,0,14,12]]}
[]
["Formulary"]
[{"$nulls":6},"Jednotka"]
["Conditions",{"$nulls":5},"Verze"]
[]
["Teploty",{"$nulls":8},"Šířka","Délka","Výška","Typ"]
["Topení:",{"$nulls":4},"Chlazení:",{"$nulls":10},"Kopírovat všechna data"]
["Voda na přívodu","Voda na přívodu","Voda na přívodu",{"$f":"'Mini Canal'!E10","v":35},null,{"$f":"A8","v":"Voda na přívodu"},{"$nulls":3},{"$f":"'Mini Canal'!J10","v":16},null,"Převod jednotek",{"$nulls":4},"Mezinárodní (Sl)"]
["Voda na zpátečce","Voda na zpátečce","Voda na zpátečce",{"$f":"'Mini Canal'!E11","v":30},null,{"$f":"A9","v":"Voda na zpátečce"},{"$nulls":3},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":6},"Imperiální"]
["\"Suchá\" teplota vzduchu","teplota vzduchu","teplota vzduchu",{"$f":"'Mini Canal'!E12","v":20},null,{"$f":"A10","v":"\"Suchá\" teplota vzduchu"},{"$nulls":3},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}}]
[{"$nulls":5},"Relativní vlhkost [%]",{"$nulls":3},{"$f":"'Mini Canal'!J13","v":{"v":0.5,"d":"50%"}}]
[]
[]
["Rychlost","Ovládací napětí [V]",{"$f":"CONCATENATE(\"Výkon Topení * \",ROUND(D8,0),\"/\",ROUND(D9,0),\"/\",ROUND(D10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Výkon Topení * 35/30/20 [W]"},{"$f":"\"Průtok vody, topení [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Průtok vody, topení [l/h]"},{"$f":"\"Tlaková ztráta [\"&IF(data!$P$1=1,\"kPa\",IF(data!$P$1=2,\"ftH2O\"))&\"]\"","v":"Tlaková ztráta [kPa]"},{"$f":"CONCATENATE(\"Výkon chlazení* \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Výkon chlazení* 16/18/27 [W]"},{"$f":"CONCATENATE(\"Výkon chlazení Celkový \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Výkon chlazení Celkový 16/18/27 [W]"},{"$f":"\"Průtok vody, chlazení [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Průtok vody, chlazení [l/h]"},{"$f":"E14","v":"Tlaková ztráta [kPa]"},"Akustický tlak *** [dB(A)]","Akustický výkon ** [dB(A)]","Elektrický výkon [W]","Objem vody [l]"]
[{"$f":"\"Mini Canal, \"&L6&\" \"&ROUND(data!C5,1)&\"cm, \"&J6&\" \"&ROUND(data!B5,1)&\"cm, \"&K6&\" \"&ROUND(data!E5,1)&\"cm\"","v":"Mini Canal, Výška 290cm, Šířka 14cm, Délka 34cm"}]
[]
[]
[]
[]
["Chladicí výkon vypočítán podle EN 16430  s ventilátory, které u všech typů - výšek foukají nahoru.",{"$nulls":11},{"$f":"'Mini Canal'!M22","v":"v2023-06-16"}]
["Akustický tlak podle ISO 3741:2010 "]
["Akustický výkon s předpokládaným útlumem místnosti 8 dB (A)."]

{"sheet":"ExtraTaal1","index":10,"n_rows":22,"n_cols":17,"rows_kept":22,"hidden":true,"merged":[[7,0,7,2],[7,5,7,8],[8,0,8,2],[8,5,8,8],[9,0,9,2],[9,5,9,8],[14,0,14,12]]}
[]
["Formulary"]
[{"$nulls":6},"Device"]
["Conditions",{"$nulls":5},"Version"]
[]
["Temperatures",{"$nulls":8},"Heigth","Width","Length","Type"]
["Heating:",{"$nulls":4},"Cooling:",{"$nulls":10},"Copy all data"]
["Inlet temp.",null,null,{"$f":"'Mini Canal'!E10","v":35},null,{"$f":"A8","v":"Inlet temp."},{"$nulls":3},{"$f":"'Mini Canal'!J10","v":16},null,"Unit conversion",{"$nulls":4},"SI-units"]
["Return temp.",null,null,{"$f":"'Mini Canal'!E11","v":30},null,{"$f":"A9","v":"Return temp."},{"$nulls":3},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":6},"Imperial-units"]
["Room temp.",null,null,{"$f":"'Mini Canal'!E12","v":20},null,{"$f":"A10","v":"Room temp."},{"$nulls":3},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}}]
[{"$nulls":5},"rel. humid. [%]",{"$nulls":3},{"$f":"'Mini Canal'!J13","v":{"v":0.5,"d":"50%"}}]
[]
[]
["Speed level:","Control voltage [V]",{"$f":"CONCATENATE(\"Heat output * \",ROUND(D8,0),\"/\",ROUND(D9,0),\"/\",ROUND(D10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Heat output * 35/30/20 [W]"},{"$f":"\"Water flowrate, heating [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Water flowrate, heating [l/h]"},{"$f":"\"Watersided pressure loss [\"&IF(data!$P$1=1,\"kPa\",IF(data!$P$1=2,\"ftH2O\"))&\"]\"","v":"Watersided pressure loss [kPa]"},{"$f":"CONCATENATE(\"Sens. cooling capacity * \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Sens. cooling capacity * 16/18/27 [W]"},{"$f":"CONCATENATE(\"Tot. cooling capacity \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Tot. cooling capacity 16/18/27 [W]"},{"$f":"\"Water flowrate, cooling [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Water flowrate, cooling [l/h]"},{"$f":"E14","v":"Watersided pressure loss [kPa]"},"Sound pressure *** [dB(A)]","Sound power ** [dB(A)]","Electrical power [W]","Water volume [l]"]
[{"$f":"\"Mini Canal, \"&L6&\" \"&ROUND(data!B5,1)&\"cm, \"&J6&\" \"&ROUND(data!E5,1)&\"cm, \"&K6&\" \"&ROUND(data!C5,1)&\"cm\"","v":"Mini Canal, Length 14cm, Heigth 34cm, Width 290cm"}]
[]
[]
[]
[]
["Values according to EN 16430",{"$nulls":11},{"$f":"'Mini Canal'!M22","v":"v2023-06-16"}]
["Sound power according to ISO 3741:2010"]
["Sound pressure with an assumed room damping of 8dB(A)"]

{"sheet":"ExtraTaal2","index":11,"n_rows":22,"n_cols":17,"rows_kept":22,"hidden":true,"merged":[[7,0,7,2],[7,5,7,8],[8,0,8,2],[8,5,8,8],[9,0,9,2],[9,5,9,8],[14,0,14,12]]}
[]
["Formulary"]
[{"$nulls":6},"Device"]
["Conditions",{"$nulls":5},"Version"]
[]
["Temperatures",{"$nulls":8},"Heigth","Width","Length","Type"]
["Heating:",{"$nulls":4},"Cooling:",{"$nulls":10},"Copy all data"]
["Inlet temp.",null,null,{"$f":"'Mini Canal'!E10","v":35},null,{"$f":"A8","v":"Inlet temp."},{"$nulls":3},{"$f":"'Mini Canal'!J10","v":16},null,"Unit conversion",{"$nulls":4},"SI-units"]
["Return temp.",null,null,{"$f":"'Mini Canal'!E11","v":30},null,{"$f":"A9","v":"Return temp."},{"$nulls":3},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":6},"Imperial-units"]
["Room temp.",null,null,{"$f":"'Mini Canal'!E12","v":20},null,{"$f":"A10","v":"Room temp."},{"$nulls":3},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}}]
[{"$nulls":5},"rel. humid. [%]",{"$nulls":3},{"$f":"'Mini Canal'!J13","v":{"v":0.5,"d":"50%"}}]
[]
[]
["Speed level:","Control voltage [V]",{"$f":"CONCATENATE(\"Heat output * \",ROUND(D8,0),\"/\",ROUND(D9,0),\"/\",ROUND(D10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Heat output * 35/30/20 [W]"},{"$f":"\"Water flowrate, heating [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Water flowrate, heating [l/h]"},{"$f":"\"Watersided pressure loss [\"&IF(data!$P$1=1,\"kPa\",IF(data!$P$1=2,\"ftH2O\"))&\"]\"","v":"Watersided pressure loss [kPa]"},{"$f":"CONCATENATE(\"Sens. cooling capacity * \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Sens. cooling capacity * 16/18/27 [W]"},{"$f":"CONCATENATE(\"Tot. cooling capacity \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Tot. cooling capacity 16/18/27 [W]"},{"$f":"\"Water flowrate, cooling [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Water flowrate, cooling [l/h]"},{"$f":"E14","v":"Watersided pressure loss [kPa]"},"Sound pressure *** [dB(A)]","Sound power ** [dB(A)]","Electrical power [W]","Water volume [l]"]
[{"$f":"\"Mini Canal, \"&L6&\" \"&ROUND(data!B5,1)&\"cm, \"&J6&\" \"&ROUND(data!E5,1)&\"cm, \"&K6&\" \"&ROUND(data!C5,1)&\"cm\"","v":"Mini Canal, Length 14cm, Heigth 34cm, Width 290cm"}]
[]
[]
[]
[]
["Values according to EN 16430",{"$nulls":11},{"$f":"'Mini Canal'!M22","v":"v2023-06-16"}]
["Sound power according to ISO 3741:2010"]
["Sound pressure with an assumed room damping of 8dB(A)"]

{"sheet":"ExtraTaal3","index":12,"n_rows":22,"n_cols":17,"rows_kept":22,"hidden":true,"merged":[[7,0,7,2],[7,5,7,8],[8,0,8,2],[8,5,8,8],[9,0,9,2],[9,5,9,8],[14,0,14,12]]}
[]
["Formulary"]
[{"$nulls":6},"Device"]
["Conditions",{"$nulls":5},"Version"]
[]
["Temperatures",{"$nulls":8},"Heigth","Width","Length","Type"]
["Heating:",{"$nulls":4},"Cooling:",{"$nulls":10},"Copy all data"]
["Inlet temp.",null,null,{"$f":"'Mini Canal'!E10","v":35},null,{"$f":"A8","v":"Inlet temp."},{"$nulls":3},{"$f":"'Mini Canal'!J10","v":16},null,"Unit conversion",{"$nulls":4},"SI-units"]
["Return temp.",null,null,{"$f":"'Mini Canal'!E11","v":30},null,{"$f":"A9","v":"Return temp."},{"$nulls":3},{"$f":"'Mini Canal'!J11","v":18},{"$nulls":6},"Imperial-units"]
["Room temp.",null,null,{"$f":"'Mini Canal'!E12","v":20},null,{"$f":"A10","v":"Room temp."},{"$nulls":3},{"$f":"'Mini Canal'!J12","v":{"v":26.999999999999996,"d":"27"}}]
[{"$nulls":5},"rel. humid. [%]",{"$nulls":3},{"$f":"'Mini Canal'!J13","v":{"v":0.5,"d":"50%"}}]
[]
[]
["Speed level:","Control voltage [V]",{"$f":"CONCATENATE(\"Heat output * \",ROUND(D8,0),\"/\",ROUND(D9,0),\"/\",ROUND(D10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Heat output * 35/30/20 [W]"},{"$f":"\"Water flowrate, heating [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Water flowrate, heating [l/h]"},{"$f":"\"Watersided pressure loss [\"&IF(data!$P$1=1,\"kPa\",IF(data!$P$1=2,\"ftH2O\"))&\"]\"","v":"Watersided pressure loss [kPa]"},{"$f":"CONCATENATE(\"Sens. cooling capacity * \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Sens. cooling capacity * 16/18/27 [W]"},{"$f":"CONCATENATE(\"Tot. cooling capacity \",ROUND(J8,0),\"/\",ROUND(J9,0),\"/\",ROUND(J10,0),\" [\"&IF(data!$P$1=1,\"W\",IF(data!$P$1=2,\"Btu/h\"))&\"]\")","v":"Tot. cooling capacity 16/18/27 [W]"},{"$f":"\"Water flowrate, cooling [\"&IF(data!$P$1=1,\"l/h\",IF(data!$P$1=2,\"GPM\"))&\"]\"","v":"Water flowrate, cooling [l/h]"},{"$f":"E14","v":"Watersided pressure loss [kPa]"},"Sound pressure *** [dB(A)]","Sound power ** [dB(A)]","Electrical power [W]","Water volume [l]"]
[{"$f":"\"Mini Canal, \"&L6&\" \"&ROUND(data!B5,1)&\"cm, \"&J6&\" \"&ROUND(data!E5,1)&\"cm, \"&K6&\" \"&ROUND(data!C5,1)&\"cm\"","v":"Mini Canal, Length 14cm, Heigth 34cm, Width 290cm"}]
[]
[]
[]
[]
["Values according to EN 16430",{"$nulls":11},{"$f":"'Mini Canal'!M22","v":"v2023-06-16"}]
["Sound power according to ISO 3741:2010"]
["Sound pressure with an assumed room damping of 8dB(A)"]